***SCHEDULE B* REPAIR & RENOVATION OF EXISTING WATER WORKS FOR IMPROVEMENT AND EXTENSION OF URBAN WATER SUPPLY SCHEME SHAHDADPUR I/C FILTRATION DISTRICT SANGHAR.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.# | Description | Qty | Rate | Unit | Amount |

1. Full hire charges of the pumping set p/day inclusive wage of driver & assistant fuel or electric egy: plat forms required for placing pumps etc at lower depth with suction and delievery pipes for pumping outw/found at various depths from trench ic cost of errection and dism: after completionof the job hire charges of pumping set of intp 10 HP pumping out water from 10 ft deep trench (PHSI No. 23 P/53)

30.0 Days Rs: 1500/- P/Day Rs: 45000/-

2. Earth work Excavation in ashes and soft soil of site cleareance undressed lead upto 50’ in silt clreance (GSI NO. 2 (a) P/1)

315747. Cft Rs: 1663/75 P% 0 Cft Rs: 525324/-

3. Extra for wet earth

315747.0 Cft Rs. 1058/75 P%0 Cft Rs. 334297/-

4. Extra for every 50’ ft additional lead or part of tank and reservoirs for earth work (soft ordinary hard or very hard ) (GSI No. 8 (a) P-2)

315747.0 Rs. 907/02 P% 0 Cft Rs. 286389/-

5. Jungle clearance of removing with in 100 ft (a) light (GSI No. 4 (a) P/95)

77500.0 Cft Rs. 75/63 P%0 Cft Rs. 5861/-

6. Cement concrete plain i/c placing compacting finishing curing etc complete i/c screening and washing of stone aggregate with out shuttering (Ratio 1:4:8)(GSI No: 5 (i) P/17 )

16023.0 Cft Rs: 11288/75 P% Cft Rs: 1808796/-

7. Brick lining 9”x4” ½” 3 in (1:6) cement sand mortar (GSI NO. 8 P/75)

ON SLOPE

5120.46 Cft Rs. 13163/40 P% Cft Rs. 674027/-

ON BED

4333.75 Cft Rs. 12519/07 P% Cft Rs. 542545/-

8. Pucca brick work in foundation and plinth in cement sand mortar (1:6) (GSI NO. 4 (e) P/21)

4359.37 Cft Rs. 11948/36 P% Cft Rs. 520873/-

9. Cement plaster (1:6) up to 12” height 1/2” thick(G.SI No:13(a) P/52

14531.25 Sft. @Rs.2206/60 P% Sft. Rs. 320646/-

10. Cement plaster (1:4) up to 12” height 3/8” thick(G.SI No:11(a) P/59

14531.25 Sft. @Rs.2197/52 P% Sft. Rs. 319327/-

11. Cement pointing struck joint on wall ratio (1:3) (GSI No, 19 P/53)

65852.04 Sft Rs. 1213/58 P% Sft Rs. 799167/-

**Total Rs. 6182252/-**

**CONDITIONS.**

1. Any error omission in the specification quantity and unit will be governed by the relevant schedule items.
2. The rates should be inclusive of all taxes i.e sales tax octori tax etc.
3. No separate carriage will be paid to the contractor
4. No premium will be allowed for no-schedule items.
5. The decision of the Superintending Engineer, Public Health Engineering Circle Mirpurkhas will be final and binding the parties if in any dispute.

EXECUTIVE ENGINEER

PUBLIC HEALTH ENGG: DIVISION

SANGHAR