**NAME OF WORK: M/R TO SINDH HIGH COURT BUILDING KARACHI (S/F GYSER IN CHAMBERS & GENERAL REPAIRING WORK)**

**SCHEDULE”B”**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S/No** | **Description** | **Qty** | **Rate** | **Unit** | **Amount** |
|  | **Part-A Building Schedule Item** |  |  |  |  |
| **1.** | **Scraping (b) Ordinary distemper, oil bound distemper or paint on walls.(54-b/13).** | **111531.70 Sft.** | **226/88** | **%Sft.** | **253043** |
| **2.** | **Preparing the surface and painting with plastic emulsion of approved make (ld surface) (b) 2nd & subsequent coat. ( 41-a+b/56).** | **67627.70 Sft.** | **1402/23** | **%Sft.** | **948297/-** |
| **3.** | **Preparing the surface & painting with matt finish paint of approved make to old matt finish surface(b)2nd & subsequent coat.(SI.N. 37-a+b/55)** | **43904.0 Sft.** | **1772/38** | **%Sft.** | **778145/-** |
| **4.** | **Supplying and fixing in position aluminum framing for sliding windows and ventilators of alcop made with 5mm thick tinted glass glazing (Belgium)and aluminum fly screen i/c handles stoppers and locking arrangement etc complete. (b) Deluxe model (Bronze).(84-b/108).** | **119.0 Sft.** | **1647/69** | **P.Sft.** | **196075/-** |
| **5.** | **Providing and fixing iron steel grill using solid square bars of size ½” x1/2” placed at 4 and frame of flat iron patti of ¾” x3/4” i/c circle shape at 1-0 apart equivalent fitted with screws are pins oxide painting 3 coats with 1st coat of red oxide paint etc ( 94/30).** | **546.0 Sft.** | **194/16** | **P.Sft.** | **106011/-** |
| **6.** | **Providing and fixing iron collapsible gate with channel framing of section ¾” x5/16 at 4” i/c revitted with ¾” x1/8” flat iron patti placed diagonally and provided with top and bottom t-section 1”x1”x1/8” along with rollers also i/c locking arrangement and fixing in floor/ ceiling wall etc completed. ( 94/32).** | **96.0 Sft** | **387/04** | **P.Sft.** | **37155/-** |
|  |  | **Rs.** | | | **2318726/-** |
|  |  |  | | |  |
|  |  |  | | |  |
|  |  | **Total Part-A Rs.** | | |  |
|  | **PART(B) NON SCHEDULE ITEM.** |  |  |  |  |
| **1.** | **Providing and fixing electric gyser 15 gallon fixing on wall with rowel bolts i/c necessary connection & cartage from site & back to site etc complete** | **20-Nos** |  | **Each.** |  |
| **2.** | **Providing and fixing CPVC pipe schedule 40 i/c cutting, filling and jointing with solution and fixing clamps etc complete .** |  |  |  |  |
| **a).** | **¾” dia (CPVC)** | **84.0 Rft.** |  | **P.Rft.** |  |
| **b).** | **½” dia (CPVC)** | **200.0 Rft.** |  | **P.Rft.** |  |
| **c).** | **1” dia . (CPVC)** | **170.0 Rft.** |  | **P.Rft.** |  |
| **d).** | **1 ¼” dia . (CPVC)** | **2400.0 Rft.** |  | **P.rft.** |  |
| **3).** | **Providing and fixing Handle valve Mughal make .** |  |  |  |  |
| **a).** | **¾” dia** | **20-Nos** |  | **Each.** |  |
| **b).** | **1”dia** | **10-Nos** |  | **Each.** |  |
| **c).** | **1 ¼” dia** | **40-Nos** |  | **Each.** |  |
| **4.** | **Providing and fixing basin mixer Master make .** | **20-Nos** |  | **Each.** |  |
| **5).** | **Providing and fixing Razer barbed wire G.I fixing horizontal and vertical on existing grill etc complete.** | **225.0 rft.** |  | **P.Rft.** |  |
| **6).** | **Providing and fixing commode set complete (Porta make ) i/c P-Trap and commode seat cover etc complete.** | **2-Nos .** |  | **Each.** |  |
| **7).** | **Providing and fixing Door closer approved quality and make (Imported).** | **12-Nos** |  | **Each.** |  |
| **8).** | **Painting oil paint on foot path reflection shine on dark time i/c filling and painting 3 coats ICI make upto (12” height) .** | **2400.0 Rft.** |  | **P/Rft.** |  |
| **9).** | **Repairing of aluminum door and windows i/c replacement wheel & channel and making into good running condition and repairing of locks and hinges of doors etc complete.** | **11-Nos** |  | **Each.** |  |
| **10).** | **Providing and fixing Glass pane transparent 5 mm i/c golden teak wood gola etc complete.** | **66.16 sft.** |  | **P.sft.** |  |
| **11).** | **Providing and fixing side piller cock Master make.** | **12-Nos** |  | **Each.** |  |
| **12).** | **Providing and fixing commode seat cover approved quality and make .** | **16-Nos** |  | **Each.** |  |
| **13).** | **Providing and fixing Muslim shower with chain (Master make)** | **20-Nos** |  | **Each.** |  |
| **14).** | **Providing and fixing door lock handle type approved quality and make .** | **10-Nos** |  | **Each.** |  |
| **15).** | **Providing and fixing sitting benches of RCC mosaic flooring material white 4 seater with cc bracket fix on floor etc complete.** | **6-Nos** |  | **Each.** |  |
| **16).** | **Providing and fixing paver bottle neck style i/c 2” thick khaka bed and cc flooring on edges i/c compacting etc complete.** | **252.0 Sft.** |  | **P.Sft.** |  |
| **17).** | **Providing and fixing G.I Sheet 10 guage over existing I. door & grill with welding and fixing flat pattiee on edges and painting 2 coats etc complete.** | **42.0 Sft.** |  | **P.Sft.** |  |
| **18).** | **Providing and fixing G.I pipe post 2 ½” x3’-0 size fixing on chain and making i/c making holes on road upto 6” and fixing wire cc 1:4 and painting 3 coats etc complete.** | **18-Nos** |  | **Each.** |  |
| **19).** | **Providing and fixing parking board and 24”x18” size and writing as per required on G.I 21/2” pipe i/c making holes on road and making good etc complete.** | **2-Nos** |  | **Each.** |  |
| **20.** | **Providing and fixing 2” dia foot valve approved quality and make .** | **01-No .** |  | **Each.** |  |
| **21.** | **Repairing of main gate i/c P/F new grill on bottom side on gate and making with running condition etc complete.** | **4-Nos** |  | **Each.** |  |
|  |  | **Total (B) Rs.** | | |  |
|  |  | **Total (A)** | | |  |
|  |  | **G.Total Rs.** | | |  |

**TERMS AND CONDITION**

**1. Any typographical errors in the schedule ‘B’ are subjected to any correction with the reference to the schedule of Rates General item 2012 in force from `12-07-2012 as approved by the standing rates committee Sindh Karachi.**

**2. 100% well graded crushed bajri shall be used in item of RCC 1:2:4.**

**3. No Premium shall be paid on Non schedule items.**

**4. The work will be carried out as per PWD Specifications.**

|  |  |  |
| --- | --- | --- |
| **Contractor.** | **--s/d--**  **ASSISTANT ENGINEER**  **Provincial Building Sub Division-XI,**  **Karachi** | **--s/d--**  **EXECUTIVE ENGINEER**  **Provincial Building Division-No.III**  **Karachi** |