***SCHEDULE - B***

***CONSTRUCTION OF R.C.C NALA FROM JAM TAMACHI REST HOUSE TO BHITSHAH CHOCK TALUKA TANDO ADAM DISTRICT SANGHAR***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.N*** | ***DESCRIPTION*** | ***QTY*** | ***RATE*** | ***UNIT*** | ***AMOUNT*** |

1. Dismantling & removing road metralling (GSI: No.51.P-13)

**6018.75 Cft @ Rs. 605/- P% Cft Rs. 36413/-**

1. Excavation in foundation of building bridge & other structure i/c degbelling dressing refilling around structure with excavated earth watering & remaining Lead upto 5ft in soft soill (GSI: No:18 (b) P/4).

**15046.87 Cft @ Rs. 3176.25/- P% Cft Rs. 47793/-**

1. Extra for wet earth work (GSI: No.15,P-4)

**15046.87 Cft @ Rs. 1058.75/= P% Cft Rs. 15931/-**

1. Cement Concrete brick or stone ballast 1½ to 2” gauge (GSI: No:4 P-15).

Ration (1:4:8)

**2006.25 Cft @ Rs. 9416.28/- P% Cft Rs. 188914/-**

1. Full hire charges of the pumping set P/day inclusive wage of drive & assistant fuel or electric egy: plat forms required for placing pumps etc. at lower depth with suction an delivery pipes for pumping out w/ found at various depths from tench i/c of errection and dism: after completion of the jobi) hire charges of pumping set of up to 10 Hp pumping out water from 10ft deep trench (PHSI No: 23 P/76).

**150.00 Days @ Rs. 1500/= P. Day Rs. 225000/-**

1. RCC work i/c Labor and material except the cost of steel reinforcement and Its labor for bending and binding which will be paid separately. This rate also Includes all kinds of forms mould lifting shuttering curing rendering and finishing the exposed surface (i/c screening and washing of shingle)a RCC work in roofs slabs beams columns rafts lintels and other structural members laid in situ or precast laid in position complete the all respect (I) Ratio 1:2:4 90 lbs cement 2cft sand 4 Cft shingle 1/8” to ¼”guage. (GSI No: 6 (a) P-17).

**7592.18 Cft @ Rs. 337/- P. Cft Rs. 2558565/-**

1. Fabrication of mild steel reinforcement cement concrete i/c cutting bending Laying in position and making joint and fastening i/c cost of binding. Swire also includes removal or rust from bars. (GSI:8(b) P-17)

**271.14 Cwt @ Rs. 5001/70 P. Cwt Rs. 1356161/-**

1. Cement concrete plain i/c placing compacting finishing and curing complete i/c screening and washing of stone aggregate without shuttering. Ratio 1:2:4. (G.S.I.No: 5,P/18).

**882.75 Cft @ Rs.14429/25 P% Cft Rs. 127374/-**

9) Small iron works such as gusset plate knees bend erection in position (GSI No:2,P/96).

**13.75 Cwt @Rs. 6420/61 P/Cwt Rs. 88283/-**

10) Precast Reinforcement Cement Concrete in columns , beams lintels stains cases, shelves etc. (G.S.I No-6/B P-17)

**72.84 Cft @ Rs. 349/- P/Cft Rs. 25421/-**

11) Errection & Fixing in position cement concrete on stone slab in roof or lintels, etc .

(GSI No: 6/C 7 P-17)

**72.84 Cft @Rs. 41/77 P/Cft Rs. 3043/-**

**Total Rs. 4672898/-**

***CONDITIONS.***

*1. Any error omission in the specification quantity and unit will be governed by the relevant schedule items.*

*2. The rates should be inclusive of all taxes i.e. sales tax octori tax etc.*

*3. No separate carriage will be paid to the contractor.*

1. *No premium will be allowed for non-schedule items.*
2. *The decision of the Superintending Engineer, Public Health Engineering Circle Mirpurkhas will be final and binding the parties in any dispute.*

EXECUTIVE ENGINEER

CONTRACTOR. PUBLIC HEALTH ENGG: DIVISION

SANGHAR