**Tender Reference No. 01(18)/ 2015-2016**

**SCHEDULE RATE BASED ON (2012)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. NO** | **DESCRIPTION OF ITEMS** | **QTY** | **RATE IN FIGURE** | **RATE IN WORD** | **UNIT** | **AMOUNT** |
| 1. | Excavation of pipe line trenches pipe all kind of soil murum i/c trimming dressing leveling beds trenches correct level and graded cutting joints holes disposal of surplus earth with in 1 chains as directed by the Engg: Inch: P. fence guard lights flags temporary  crossing non vehicler traffic where ever req: a lift upto 5 ft & lead up to 1 chain. | 50000/Cft  26250/Cft | 4650/-  5200/- | Four Thousand Six Hundred & Fifty  Five Thousand & Two Hundred | %0Cft  %0Cft | 232500/-  136500/- |
| 2. | P. Rcc pipe ASTM class class ‘C’ 76-62 T/C 76-70 class II wall ‘B’ and fixing in trenches i/c cutting fitting jointing with rubber ring i/c testing with water  to specified pressure 9″ & 12″dia pipe. | 4000/P.Rft | 412/- | Four Hundred & Twelve | P.Rft | 1648000/- |
| 3. | Const of Main Holes 4 inside with Rcc covers 21″dia 3×¾ with flat iron frame 5ft depth 1:2:4 in laying CC cost in situ 9″ thick wall and disposal of surplus stuff etc comp: | 170 No | 13028/- | One Thousand Three Hundred & Twenty Eight | Each | 2214760/- |
| 4. | Add or deduct for depth of man holes above or beyond 5 ft (RA). | 255/Rft | 2245/55 | Two Thousand Two Hundred Forty Five & Fifity Five Paisa | P.Rft | +572615/- |
| 5. | Refilling the excavated stuff in trenches 6″ thick layer i/c watering ramming to full compaction etc comp: | 68625/Cft | 2760/- | Two Thousand Seven Hundred & Sixty | %0Cft | 189405/- |
| **Total Amount of Schedule Items** | | | | | | **49,93,780/-** |