***BIDDING DATA***

***(The Section Should Be Filed In The Engineer /Production Agency Before Issuance Of The Bidding Documents)***

|  |  |  |
| --- | --- | --- |
| ***a)*** | *Name of procuring agency:* | ***Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***b*** | *Briel description of work :* | Surface Drains and CC Block for Village Qaisar Khan Shahani UC Gadeji Taluka Sobhodero. |
| ***c*** | *procuring agency’s Address* | **Taluka Sobhodero District Khairpur** |
| ***d*** | Estimated Cost | Rs. 19, 00, 000/- |
| ***e*** | Amount of BID Security | **2%** |
| ***f*** | Period of bid validity (Security) | **15 Days** |
| ***g*** | Security Deposit(including Bid Security) | **N/A** |
| ***h*** | Dead Line for bid submission of bid along with time | **N/A** |
| ***i*** | Venue time and date of bid opening | ***At Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***j*** | Time for completion form written order of commence | 12 Months |
| ***k*** | Liquidity damages | N/A |
| ***l*** | Deposit receipt No: date amount (kin word & Figure) | N/A |
|  |  |  |

***(Executive Engineer/Authority issuing bedding document)***

|  |  |
| --- | --- |
| ***Assistant Engineer***  ***Public Health Engineering***  ***Sub Division Sobhodero*** | ***Executive Engineer***  ***Public Health Engineering***  ***Division II Khairpur @ Ranipur*** |

**SCHEDULE B**

**NAME OF WORK: CONSTRUCTION OF SURFACE DRAINS & C.C BLOCK FOR VILLAGE QASAR KHANSHAHANI U/C GADEJI TALUKA SOBHODERODISTRICT KHAIRPUR**

**PART.I** **SURFACE DRAINS**

1. Excavation in foundation of building bridges and other

structure i/c dag belling refilling around the structure

with excavated earth watering ramming lead up to one

chain and lift up to 5 ft. (C S I No.18 (b) P.NO.4)

Qty.1535.25 Cft @ Rs.3176/25 P %Cft. Rs: 4876/-

1. Cement concrete plain i/c placing compacting finishing

curing complete i/c screening and washing stone

aggregate w/o shuttering (CSI No.5(i) P.NO.16)

**(a) Ratio 1:4:8**

Qty: 409.75 Cft. @Rs.11288/75 P %CftRs:46.256/-

1. Pacca Brick work in foundation and plinth in cement sand

Ratio (1;6) (CSI No.4 (e) P.NO.21)

Qty1116.0 Cft@Rs.11948/36P% CftRs:1,33,344/-

1. Construction of standard of open drains cunette block

of cement concrete 1:2:4 in situ to design profile i/c cost

of mould as per drawing i/c applying floating coat of

cement 1/32” thick to the exposed face finished smooth

curing etc complete as per detail drawing

(PHSI No. D P.NO.44)

Type –I

Qty.350.0 Rft @Rs.94/- P Rft. Rs.32,900/-

Type –II

Qty.200.0 Rft @Rs.174/- P Rft. Rs.34,800/-

1. Cement plaster 1:4 20’ height ½” thick

(CSI No.13 P.NO.52)

Qty.2141.0Sft @Rs.2283/93 P% **Sft.** Rs.48,899/**-**

1. RCC work in roof slab, beams columns rafts, lintels,

and other structure members laid in situ of pre cost

laid in position complete in all respect 1:2:4

(CSI No.7 P.NO.17).

Qty**.101.87**Cft @Rs.337/- P% **Sft.** Rs.34,330/-

1. Fabricationof mild steel reinforcement for cement

concrete i/c cutting bending laying in position

making K=joints and festering i/c cost of binding

wire also i/c removal of rust from bars

(CSI No.7(ii) P.NO.19).

Qty.3.638 Cwt. @Rs.5001/70 P cwt Rs.18,196/-

***Total*** Rs3,53,601/-

PART .II **C.CBLOCK**

1. Barrow pit excavation undressed lead up to 100 ft in

ordinary soil (CSI-3(a) P-1)

Qty.16155.0 CFT @Rs.2117/50 P%0 Cft. Rs.34,208/-

2. Lying Earth in 6” layers & leveling dressing &

Watering for Etc complete. (CSI-13(b)P-3)

Qty:16155.0 CFT @Rs.354/- P%0 Cft Rs.5719/-

3. Extra for every 50”ft additional lead or part there of

(C.S.I No: 8 (a) P-3)

Qty:16155.0 CFT @Rs.5039/- P%0 Cft Rs.81405/-

4. Cement concrete brick or stone ballast 1 ½” to 2” guage

Ratio 1:4:8 (CSI No.4(b)9 P. 15).

Qty. 4264.92 CFT @Rs.9416/28 P% Cft. Rs.401597/-

5. Cement concrete plain 1:2:4 i/c placing compacting

finishing and curing complete i/c screening and

washing of stone aggregate without shuttering

(CSI No.5 P.No.16)

Qty. 3231.0 CFT @Rs.14429/25 P% Cft. Rs.466209/-

6. Errection& removal for centering of therefore ofRcc

Partial wood (CSI .No. ) Ratio: 1:2:4.

Qty. 638.0 Sft @Rs.3127/41 P% Sft. Rs.19,953/-

**Total Rs.10,09,091/-**

**GENERAL ABSTRACT OF COST**

**PART: 1 Surface Drains Rs:353601/-**

**PART: II C.C. BLOCK Rs:10,09,091/-**

**Total Rs:13,62,692/-**

***C O N D I T I O N S***

01. Any error / omission in the description of items of work rate original schedule

will correct accordingly under executive engineer Public Health Engineering

division II Khairpur @ Ranipur .

02. premium will be allowed as non , schedule items.

03. The work will be carried out as per P.W.D. specification and approval details.

working estimates .

|  |  |
| --- | --- |
| CONTRACTOR | EXECUTIVE ENGINEER  PUBLIC HEALTH ENGINEERING  DIVISION-II KHAIRPUR @ RANNIPUR |