***BIDDING DATA***

***(The Section Should Be Filed In The Engineer /Production Agency Before Issuance Of The Bidding Documents)***

|  |  |  |
| --- | --- | --- |
| ***a)*** | *Name of procuring agency:* | ***Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***b*** | *Briel description of work :* | ***Construction of surface Drains and Paver Block of Sial Mohalla Near Old Bus Satand Ranipur.*** |
| ***c*** | *procuring agency’s Address* | **Taluka Sobhodero District Khairpur** |
| ***d*** | Estimated Cost | Rs. 48, 00, 000/-/- |
| ***e*** | Amount of BID Security | **2%** |
| ***f*** | Period of bid validity (Security) | **15 Days** |
| ***g*** | Security Deposit(including Bid Security) | **N/A** |
| ***h*** | Dead Line for bid submission of bid along with time | **N/A** |
| ***i*** | Venue time and date of bid opening | ***At Executive Engineer Public Health Engineering Division II Khairpur @ Ranipur*** |
| ***j*** | Time for completion form written order of commence | 12 Months |
| ***k*** | Liquidity damages | N/A |
| ***l*** | Deposit receipt No: date amount (kin word & Figure) | N/A |
|  |  |  |

***(Executive Engineer/Authority issuing bedding document)***

|  |  |
| --- | --- |
| ***Assistant Engineer***  ***Public Health Engineering***  ***Sub Division Sobhodero*** | ***Executive Engineer***  ***Public Health Engineering***  ***Division II Khairpur @ Ranipur*** |

**SCHEDULE B**

**NAME OF WORK: CONSTRUCTION for SURFACE DRAINS & CC PAVER BLOCK FOR SIAL MUHALLA OLD BUS STAND RANIPUR U/C RANIPUR taluka SOBHO DERO dISTRICT KHAIRPUR.**

**.**

**SUB HEAD NO.1 Surface drains**

1. Excavation in foundation of building bridges and other structure

i/c dag belling refilling around the structure with excavated

earth watering ramming lead up to one chain and lift up to 5 ft

. (PH Sch. No.18 P.NO.4)

Qty. 9256.81 Cft. @Rs.3176/25 P%0 Cft. Rs 29,402/-

1. Cement concrete plain i/c placing compacting finishing curing

complete i/c screening and washing stone aggregate w/o

shuttering (CSI No.5(i) P.NO.17) **(a) Ratio 1:4:8**

Qty. 2364.72 Cft @Rs.11288/75 P% Cft. Rs.2,66,947/-

1. Pacca Brick work in foundation and plinth in cement sand Ratio

(1;6) (CSI No.7 P.NO.23)

Qty. 6758.10 Cft @Rs.11948/36 P% Cft. Rs. 8,07,482/-

4. Construction of standard of open drains cunette block of cement

concrete 1:2:4 in situ to design profile i/c cost of mould as per

drawing i/c applying floating coat of cement 1/32” thick to the

exposed face finished smooth curing etc complete as per detail

drawing (PHSI No.D P.NO.44)

T-I Drain

Qty. 1945.0 Rft @Rs.94/- P Rft. Rs.1,82,830/-

T-II Drain

Qty. 1200.0 Rft @Rs.174/- P Rft. Rs.2,08,800/-

5. Cement plaster 1:4 20’ height ½” thick (CSI No.11 P.NO.57)

Qty.10428.10 Sft @Rs.2283/93 P% Sft. Rs.2,38,171/-

6. RCC work in roof slab, beams columns rafts, lintels, and other

structure members laid in situ of pre cost laid in position

complete in all respect 1:2:4 (CSI No.7 P.NO.17)

Qty.759.80 Cft @Rs.337/- P Cft. Rs.2,56,053/-

1. Fabricationof mild steel reinforcement for cement concrete i/ccutting bending laying in position making K=joints andfastering i/c cost of binding wire also i/c removal of rust from bars (CSI No.7(ii) P.NO.19).

Qty.27.13 Cwt @Rs.4820/20 P cwt. Rs: 1,20,457/-

**Total Rs: 21,20,457/-**

**SUB HEADNO.II** **C.CPAVER BLOCK.**

1. Barrow pit excavation undressed lead up to 100 ft in ordinary soil (CSI NO 3 (a) P.No 1)

Qty.8267.28 Cft @Rs.2117/50 P%0 Cft. Rs.17,506/-

2. Lying Earth in 6” layers & leveling dressing & Watering for Etc complete. (CSI NO 3 (b) P.No 3)

Qty:8267.28 Cft @Rs.354/- P%0 Cft Rs.2,927/-

03. Extra every 50 ft additional lead or part therefore (CSI No 8 (a) PNO 2 )

Qty:8267.28 Cft@Rs.5039/- P%0 Cft Rs.41,659/-

04. C.C Brick or Stone Ballast 1” to 2” guage .1:4:8 (CSI -5 P 16) 1:4:8

Qty: 2051.28 Cft@ Rs.9416/28 P % Cft Rs.1,93,154/-

05. C.C Plain i/c placing compacting finishing curring completescreening and washing of

stone aggregates w/o shutCSI -5 P 16) 1:4:8

Qty: 1554.0 Cft @ Rs.14429/25 P %Cft Rs.2,24,231/-

06 Errection & removal for centering of therefore of RccPartial wood (CSI .No. ) Ratio: 1:2:4.

Qty. 129.50 SFT @Rs.7693/13 P% Sft. Rs.9,969/-

# 07. Providing and fixing cement paving block flooring having size

# 197x97x60(mm) of city / quddara coble shape with natural colours

# having strength b/w 5000 psi 8500 psi i/c filling the joints with hill

# sand specified manner / pattern and design etc complete

(CSI –NO:71 - P NO: 49)

# Qty: 6216.0 Sft @ Rs.223/97 P Sft Rs.13,92,198/-

# **Total** = **Rs.18,81,638/-**

**ABSTRACT OF COST**

**SUB HEAD NO: 1 Surface Drains**  Rs:21,20,457/-

**SUB HEAD NO: 2 C.C Paver Block** Rs:18,81,638/-

**Total Rs:40,02,095/-**

C O N D I T I O N S

01. Any error / omission in the description of items of work rate original schedule

will correct accordingly under executive engineer Public Health Engineering

division II Khairpur @ Ranipur .

02. premium will be allowed as non , schedule items.

03. The work will be carried out as per P.W.D. specification and approval details.

working estimates .

**CONTRACTOR EXECUTIVE ENGINEER**

PUBLIC HEALTH ENGINEERING

DIVISION-II KHAIRPUR @ RANNIPUR