|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO.II, ( TUGHLAQ HOUSE ) KARACHI, ( COLOURING, PAINTING, ELECTRIC & SANITARY WORK AT DIFFERENT OFFICES VIZ DEPUTY SECRETARY AGRICULTURE, SECRETARY CULTURE, SECRETARY MINES, CHIEF EDUCATION PLANNING & DEVELOPMENT DEPARTMENT ETC.** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  | |  |  |
| 1. | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 1233.0  Sft | 226/88 | | %Sft | 2797/- |
|  | Rupees. Two hundred twenty six. And. Eighty eight. Paisa | | | | | |
| 2. | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 1233.0  Sft | 1772/38 | | %Sft | 21853/- |
|  | Rupees. One thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | | |
|  |  | **Total Part-“A” Rs.** | | | | **24650/-** |
|  |  |  | | | |  |
|  | **SCHEDULE ITEMS PART-“B” ( SANITARY WORK )** |  |  | |  |  |
| 1. | Providing & fixing European white glazed earthen ware wash down W.C pan complete with and In/c the cost of white/black plastic seat ( Best Quality ) and lid with C.P. brass hinges and buffers, 3 gallons white glazed earthen ware low level flushing cistern with siphon fitting 1-1/2” dia white porcelain enameled flush bend ¾” dia and making requisite number of holes in walls, plinth and floor for Pipe connections and making good in cement concrete 1:2:4 ( Foreign Quality ).( SI.5 / P-2 ). | 01  No | 11477/40 | | Each | 11477/- |
|  | Rupees. Eleven thousand four hundred seventy seven. And. Forty. Paisa | | | | | |
| 2. | Providing & fixing 24” x 18” lavatory basin in white glazed earthen ware complete with & I/c the cost of W.I or C.I cantilever brackets 6 inches built into wall, painted white in two coast inches built into wall, painted white in two coast after a primary coat of red lead paint, a pair of ½” dia rubber plug & chrome plate brass chain 1-1/4” dia malleable iron or C.P. brass traps malleable iron or brass unions and making requisite number of holes in walls, plinth & floor for pipe connection and making good in cement concrete 1:2:4 ( Standard pattern ).( SI.8 / P-3 ). | 01  No | 4253/70 | | Each | 4254/- |
|  | Rupees. Four thousand two hundred fifty three. And. Seventy. Paisa | | | | | |
| 3. | Add extra for labour for providing & fixing of earthen ware pedestal white or colored glazed (Foreign or Equivalent ).  ( SI.9 / P-3 ). | 01  No | 938/47 | | Each | 938/- |
|  | Rupees. Nine hundred thirty eight. And. Forty seven. Paisa | | | | | |
|  |  | **Total Part-“B” Rs.** | | | | **16669/-** |
|  |  |  | | | |  |
|  | **SCHEDULE ITEMS PART-“C” ( ELECTRIC WORK )** |  |  | |  |  |
| 1. | Wiring for light or fan point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit recessed in the wall or column as required.( SI.124 / P-15 ). | 13  Nos | 1130/- | | P.Point | 14690/- |
|  | Rupees. One thousand one hundred thirty. Only. | | | | | |
| 2. | Wiring for plug point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit on surface as required.( SI.125 /P-15 ). | 05  Nos | 669/- | | P.Point | 3345/- |
|  | Rupees. Six hundred sixty nine. Only. | | | | | |
| 3. | Wiring for call bell point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVBC conduit on surface as required.( SI.127 / P-15 ). | 01  No | 1380/- | | P.Point | 1380/- |
|  | Rupees. One thousand three hundred eighty. Only. | | | | | |
| 4. | Providing & laying ( MAIN or SUB MAIN ) PVC insulated with single core copper conductor 250/440 volts size 2-7 / .029. ( SI.45 / P-6 ). | 46.0  Meter | 118/- | | P.Meter | 5428/- |
|  | Rupees. One hundred eighteen. Only. | | | | | |
| 5. | Providing & Laying ( MAIN or MAIN ) PVC insulated with single core copper conductor 250/440 volts size ( 2-7/.044 ) 6mm2. ( SI.47 / P-06 ) | 15.32  Meter | 213/- | | P.Meter | 3263/- |
|  | Rupees. Two hundred thirteen. Only. | | | | | |
| 6. | Providing & fixing one way SP 10 / 15amp switch surface type.( SI.218 / P-33 ). | 20  Nos | 58/- | | Each | 1160/- |
|  | Rupees. Fifty eight. Only. | | | | | |
| 7. | Providing & fixing three pin 10/15 amp plug & socket flush type.( SI.227 / P-33 ). | 05  Nos | 162/- | | Each | 810/- |
|  | Rupees. One hundred sixty two. Only. | | | | | |
| 8. | Providing & fixing Brass bracket lamp holder suitable for 12mm ( ½ )” dia bracket.(SI.230 / P-33 ). | 34  Nos | 72/- | | Each | 2448/- |
|  | Rupees. Seventy two. Only. | | | | | |
| 9. | Providing & fixing Bakelite ceiling rose with two terminals . ( SI.228 / P-33 ). | 34  Nos | 72/- | | Each | 2448/- |
|  | Rupees. Seventy two,. Only. | | | | | |
|  |  | **Total Part-“C” Rs.** | | | | **34972/-** |
|  |  |  | | | |  |
|  | **NON-SCHEDULE ITEMS PART-“D”** |  |  |  | |  |
| 1. | P/F exhaust fan 12” dia or 12”x12” of approved make and quality in/c making hole of required Size in C.C. block masonary in/c cutting, chiseling and making corner with cement sand mortar 1:4 also in/c removing dismantled debries to out side premises. | 01  No |  | Each. | |  |
| 2. | P/F fancy tube light shade size 2’.0x2’.0 with reflector louver complete with energy saver & holder 24-watts (04 Nos) (Phillips or equivalent make) in/c necessary electric connection wiring and fixing on ceiling etc complete as directed by the Engineer Incharge. | 01  No |  | Each | |  |
| 3. | Providing and fixing door closer heavy type (OPAL OR KGI) make i/c. fixing on door with screws and adjusting speed as required etc. complete and as directed by Engineer Incharge. | 04  Nos |  | Each | |  |
| 4. | S/F Energy saver of approved quality (Phillips or equivalent make) fitted on wall, ceiling, & pendent upto required height in existing holder as directed by the Engineer Incharge **Energy Saver 24 watts.** | 80  Nos |  | Each | |  |
| 5. | P/F vertical blinds 4” wide with good quality fabric and approved shade & colour with all accessories i.e. aluminum section, dori, rulers, etc complete. | 55.25  Sft |  | P.Sft | |  |
| 6. | French polishing for door / windows / ventilators stair floor in/c etc preparing surface and polishing by using in door lakh Dana sprit, Thinner pigment ICI Regmal ( Germany ) tarpine oil polishing as per scaffolding of component author etc complete. | 317.0  Sft |  | P.Sft | |  |
| 7 | P/F double holder of approved quality and make as directed by Engineer Incharge. | 16-Nos |  | Each | |  |
|  |  | **Total Part-“D” Rs.** | | | |  |
|  |  | **Total Part-“C” Rs.** | | | |  |
|  |  | **Total Part-“B” Rs.** | | | |  |
|  |  | **Total Part-“A” Rs.** | | | |  |
|  |  | **G: Total Part ( A+B+C+D ) Rs.** | | | |  |
|  |  | **Say Rs.** | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |