|  |  |
| --- | --- |
| **NAME OF WORK:** | **M/R TO SINDH SECRETARIAT NO. I , KARACHI**  **(CONSTRUCTION OF POLICE CHECK POSTS WITH FIBRE GLASS ROOF FOR SECURITY MEASURES AND IMPROVING EXTERNAL LIGHTING SYSTEM.)** |

**“ SCCHEDULE ‘B’ ”**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **S.#.** | **DESCRIPTION OF ITEMS.** | | **QTY:** | **RATE.** | | **UNIT.** | | **AMOUNT.** | |
|  | | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** | | | | | | | |
| 1 | Providing and laying 1: 3: 6 cement concrete solid block masonry wall 6” and below in thickness set in 1:6 cement mortar in ground floor Super Structure including raking out joints & curring etc, complete.( SI.24 / P-19 ). | | 622.50 Cft | 15771/01 | | % Cft | | 98174/- | |
|  | Rupees. Fifteen thousand seven hundred seventy one. And. One. Paisa | | | | | | | | |
| 2 | P/L 1” thick topping cement concrete (1:2:4) including surface finishing and dividing into panels. (b) 1-1/2” thick. (SI.16-b/P-42) | | 68.00 Sft | 2548/29 | | %Sft. | | 1733/- | |
|  | Rupees. Two thousand five hundred forty eight. And. Twenty nine. Paisa | | | | | | | | |
| 3 | Cement plaster 1:6 upto 12” height (b) 1/2”thick.(SI.13-b/P-52) | | 2484.56 Sft | 2206/60 | | %Sft. | | 54824/- | |
|  | Rupees. Two thousand two hundred & six. And. Sixty. Paisa | | | | | | | | |
| 4 | Cement plaster 1:6 upto 12' height. (a) 3/8" thick.  ( SI.13(a)/P-52 ). | | 2484.56 Sft | 2122/72 | | %Sft | | 52740/- | |
|  | Rupees. Two thouand one hundred twenty two,. And. Seventy two. Paisa | | | | | | | | |
|  |  | |  | **(A). Total Rs :** | | | | **207471/-** | |
|  |  | |  | | | | |  | |
|  | **SCHEDULE ITEMS PART-“B” ( ELECTRIC WORK )** | | |  | | | |  | |
| 1 | Wiring for light or fan point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit on surface as required. ( SI.123 / P-15 ) | | 18 Nos | | 797/- | | P.Point | | 14346/- |
|  | Rupees. Seven hundred ninety seven. Only. | | | | | | | | |
| 2 | Wiring for plug point with 3/.029 PVC insulated wire in 20mm (3/4”) PVC conduit on surface as required . (SI.125/P-15) | | 06 Nos | 669/- | | P/Point. | | 4014/- | |
|  | Rupees. Six hundred sixty nine. Only | | | | | | | | |
| 3 | Providing & fixing one way SP 5amp switch flush type (33/219) | | 18 Nos | 54/- | | P/ No. | | 972/- | |
|  | Rupees. Fifty four. Only. | | | | | | | | |
| 4 | P/F surface type 3-pin 15-amps SP surface plug socket, switch and shoe unit on metal board recessed in the walls or columns and covered with plastic sheet (227/P-33) | | 06-Nos | 162/- | | P/No | | 972/- | |
|  | Rupees. One hundred sixty two. Only. | | | | | | | | |
| 5 | Providing & fixing Brass Batten holder. (SI.232/P-33) | | 12 Nos | 70/- | | P/ No. | | 840/- | |
|  | Rupees. Seventy. Only. | | | | | | | | |
| 6 | Providing & laying ( MAIN or SUB MAIN ) PVC insulated with size 2-3 /.036 copper conductor in ¾” dia PVC conduit on surface. ( SI.2 /P-1 ) | | 180.00 Meter | 139/- | | P/Meter | | 25020/- | |
|  | Rupees. One lhundred thiety nine. Only. | | | | | | | | |
| 7 | P/F circuit breaker 6,10,15,20,30,40,50, & 63 amp DP (TB-5S) on prepared board as required. (SI.204/P-31) | | 02 Nos | 2456/- | | Each. | | 4912/- | |
|  | Rupees. Two thousand four hundred fifty six. Only,. | | | | | | | | |
| 8 | P/F of flood light 400 watts (HPIT) having IP 65 classification with 400 W lamp, chock, capacitor, igniter &internal wiring complete in all respect at the height up to 40ft with the help hydraulic crane and manual labour as per site requirement and instruction of Engineer Incharge. (SI.167/P-26) | | 02 Nos | 16980/- | | P/ No | | 33960/- | |
|  | Rupees. Sixteen thousand nine hundred eighty. Only. | | | | | | | | |
| 9 | P/F 400 watts (SON-T) lamp @ the height with the holp of hydraulic crane as per site requirement & instruction of Engineer Incharge.(S.No.179/P-28) | | 05 Nos | 2132/- | | P/ No | | 10660/- | |
|  | Rupees. Two thousand one hundred thirty two. Only. | | | | | | | | |
| 10 | P/F 400 watts (HPIT) lamp @ the height with the help of hydraulic crane as per site requirement & instruction of Engineer Incharge. (SI.185/P—29) | | 06 Nos | 2380/- | | P/No. | | 14280/- | |
|  | Rupees. Two thousand three hundred eighty. Only. | | | | | | | | |
| 11 | P/F 250 watts (SON) capacitor in all respect at the height up to 40ft with the help of hydraulic crane & manual labor as per site requirement and instruction of Engineer Incharge.  (SI.No.177/P-27) | | 04 Nos | 1174/- | | P/ No. | | 4696/- | |
|  | Rupees. One thousand se one hundred seventy four. Only. | | | | | | | | |
|  |  | |  | **(B). Total Rs :** | | | | **114672/-** | |
|  |  | |  |  | | | |  | |
|  | **PART ‘C’ NON SCHEDULE ITEMS.** | |  |  | |  | |  | |
| 1 | P/Fixing fiber glass shade with fiber glass sheet 2-3mm thick including necessary frame work of angle iron or G.I pipe & fixing sheet with screws in proper design & shape as directed by Engineer Incharge | | 758.65 Sft |  | | P/Sft. | |  | |
| 2 | S/F Energy saver lamp 220 volts of approved quality (Phillips or equivalent make) fitted on wall, ceiling, & pendent upto required height in existing holder as directed by the Engineer Incharge.  **Energy Saver 24 watts.** | | 12 Nos |  | | Each | |  | |
| 3 | P/F wall bracket fan 18” dia of approved make & quality (Royal/Pak, Millat or equivalent) in/c fixing on wall as directed by the Engineer Incharge | | 06 Nos |  | | Each | |  | |
|  |  | | **Total Part-“C” Rs.** | | | | |  | |
|  |  | | **Total Part-“B” Rs.** | | | | |  | |
|  |  | | **Total Part-“A” Rs.** | | | | |  | |
|  | **G. Total Part (A+B+C) Rs.** | | | | | | |  | |
|  | **Say Rs.** | | | | | | |  | |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |