**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/01**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LYING RCC PIPE AT BLOCK B MOMINABAD UC-01 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*9,54,416/= (+) O/R

*BID SECURITY.* Rs. 19,088/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/01**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 9,54,416/= (+) O/R

Earnest Money Rs. 19,088/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **1-PROVIDING AND LYING RCC PIPE AT BLOCK B MOMINABAD UC-01 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) | 2696 Cft | 3327.50 % CFT | 99692/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 3900 Cft | 4650.00%  Sft | 18135/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 900 Cft | 10770.00 %0 CFT | 9693/- |
| 04 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 300  Rft  600 Rft | 206.00 Rft  367.00 Rft | 61800/-  220200/- |
| 05 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 40 Nos. | 13064  Each | 522560/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 70  Rft | 1540.00  Rft | -107600/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 3930  Cft | 2760.00%0  Cft | 10847/- |
| 08 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 8299  Cft | 1065.04%  Cft | 88384/- |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 14 Nos. | 913.63  Each | 12791/- |
| 10 | Earth Excavation in irrigation channels, and disposal of cerplus staff e.t.c. | 7200 Cft | 2420.00 % 0 Cft | 17424/- |
| 11 | Providing and Fixing Cast iron frame for main hole i/c the cost of material | 4.93 KG | 140 per KG | 690/- |
| **SUB TOTAL PART-A** | | | | **9,54,416/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LYING RCC PIPE AT BLOCK B MOMINABAD UC-01 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 05 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/02**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMPROVMENT OF ROAD NEAR MASHALLAH HOUSE BEHZAD COMMISSION AZIZ BAKERY IN UC-03**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,81,619 /= + O/R

*BID SECURITY.* Rs. 13,632 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/02**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,81,619 /= + O/R

Earnest Money Rs. 13,632 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **IMPROVMENT OF ROAD NEAR MASHALLAH HOUSE BEHZAD COMMISSION AZIZ BAKERY IN UC-03**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15,280 Cft | 1065.00%  Cft | 162732/- |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| **SUB TOTAL PART-A** | | | | **6,81,619/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMPROVMENT OF ROAD NEAR MASHALLAH HOUSE BEHZAD COMMISSION AZIZ BAKERY IN UC-03**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2820 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/03**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIRING OF RCC PIPE AND CC STREET IN TOUHEED MUHALLAH CHUTTA MUHALLAH AND BURRA MUHALLAH IN ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*7,79,775/= (+) O/R

*BID SECURITY.* Rs. 15,596/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/03**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,79,775/= (+) O/R

Earnest Money Rs. 15,596/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **REPAIRING OF RCC PIPE AND CC STREET IN TOUHEED MUHALLAH CHUTTA MUHALLAH AND BURRA MUHALLAH IN ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) | 2761 Cft | 3327.50 % CFT | 91872/- |
| 06 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 4416  Cft | 1065.04%  Cft | 47030/- |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1100 Cft | 4650.00 %0 CFT | 5115/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 200 Rft | 367.00 Rft | 73400/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 10 Nos. | 13064  Each | 130640/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 17.5  Rft | 1540.00  Rft | -26950/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 889 ft | 2760.00%0 Cft | 2454/- |
| 07 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 12000  Sft | 3275.50%  Sft | 393060/- |
| 08 | Preparing of subgrade i/c earth excavation leveling to an average depth of nine inch dressing to camber e.t.c | 12000 Sft | 526.28 % Sft | 63,154/- |
| 09 |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **7,79,775/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIRING OF RCC PIPE AND CC STREET IN TOUHEED MUHALLAH CHUTTA MUHALLAH AND BURRA MUHALLAH IN ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per coated Rcc Ring slab 39”dia with RCC Manhole Cover of 21” dia as per instruction of Engineer Incharge | 12 Nos | Offer Rate |  |
| 02 | S/F Imported Earth with in the a radius of 5 miles i/c digging loading unloading all lead and lift leveling and water compaction etc complete | 1688 Cft | Offer Rate |  |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 2640 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/04**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF SEWERAGE SYSTEM AND OTHER WORKS ON DIFFERENT LOCATION NEAR CHANDNI CHOWK IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*8,18,000/= (+) O/R

*BID SECURITY.* Rs. 16,360/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/04**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 8,18,000/= (+) O/R

Earnest Money Rs. 16,360/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

Subject: **REHABILITATION OF SEWERAGE SYSTEM AND OTHER WORKS ON DIFFERENT LOCATION NEAR CHANDNI CHOWK IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) RCC1:2:4 | 1228 Cft | 5445 % Cft | 66865/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 5906 Cft | 4650.00%  Sft | 27463/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 750  Rft | 436.00  Rft | 327000/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 30 Nos. | 13064  Each | 391920/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 60  Rft | 1540.00  Rft | -92400 |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 4580  Cft | 2760.00%0  Cft | 12640/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 6037  Cft | 1065.04%  Cft | 64294/- |
| 08 | Providing and Lying 1:3:6 CC Ussing GSB 3/4 inch and down gadg i/c consolideation compecting and curring e.t.c | 100 Cft | 12595.00 % Cft | 12595/- |
| 09 | Earth Excavation in irrigation channels, and disposal of cerplus staff e.t.c. | 3150 Cft | 2420.00 % 0 Cft | 7623/- |
| **SUB TOTAL PART-A** | | | | **8,18,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF SEWERAGE SYSTEM AND OTHER WORKS ON DIFFERENT LOCATION NEAR CHANDNI CHOWK IN ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S.No. | Description | Quantity | Days | Market Rate | Unit | Amount (Rs) |
| 1 | Hiring of Excavator for desalting and Cleaning of Nallaha Long Boom i/c POL  08 hours per day | 01 | 02 | O/Rate | Per day | O/Rate |
| 2 | Hiring Seal Dumpers for Lifting of Garbage & silt of Nallah i/c loading & unloading in all respect with pool  08 hours per day | 03 | 02 | O/Rate | Per day | O/Rate |
| 3 | Hiring of Loader for lifting of Garbage & silt with POL  08 hours per day |  |  |  |  |  |
| 4 | Hiring of Tractor Blade heavy Duty for Cleaning of streets & Roads etc with POL.  08 hours per day | 01 | 05 | O/Rate | Per day | O/Rate |
| 5 | Hiring of Skilled Afghani Labour for Cleaning of Nalah in different points all respect.  08 hours per day | 02 | 05 | O/Rate | Per day | O/Rate |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/05**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **MAINTENANCE AND REPAIR OF ROAD NEAR JAMA MASJID SIDDIQUI AKBAR IN SADDAT QUARTER IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,82,515 /= + O/R

*BID SECURITY.* Rs. 13,650 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/5**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,82,515 /= + O/R

Earnest Money Rs. 13,650 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **MAINTENANCE AND REPAIR OF ROAD NEAR JAMA MASJID SIDDIQUI AKBAR IN SADDAT QUARTER IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15106.75Cft | 1065.00%  Cft | 160,887/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 03 Nos. | 913.63 Each | 2,741/= |
| **SUB TOTAL PART-A** | | | | **682,515/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **MAINTENANCE AND REPAIR OF ROAD NEAR JAMA MASJID SIDDIQUI AKBAR IN SADDAT QUARTER IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 05 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/06**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF ROAD INFRONT DIYAN HOTEL NAMATULLAH MACHINES BLOCK WORK IN RAIS AMROHI COLONY IN UC-7.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,84,094/= + O/R

*BID SECURITY.* Rs. 13,682 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/06**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,84,094/= + O/R

Earnest Money Rs. 13,682 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REHABILITATION OF ROAD INFRONT DIYAN HOTEL NAMATULLAH MACHINES BLOCK WORK IN RAIS AMROHI COLONY IN UC-7.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 14997.68Cft | 1065.00%  Cft | 159,725/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 06 Nos. | 913.63 Each | 5,482/= |
| **SUB TOTAL PART-A** | | | | **684,094/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF ROAD INFRONT DIYAN HOTEL NAMATULLAH MACHINES BLOCK WORK IN RAIS AMROHI COLONY IN UC-7.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/07**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR OF ROAD / FILLING OF DAMAGES ROAD BY CARPETING NEAR SOFAID CHOWK AND ROSE GRAMMAR SCHOOL & OTHER PLACES IN UC-09**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*7,98,755 /= + O/R

*BID SECURITY.* Rs. 15,976 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/07**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,98,755 /= + O/R

Earnest Money Rs. 15,976 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REPAIR OF ROAD / FILLING OF DAMAGES ROAD BY CARPETING NEAR SOFAID CHOWK AND ROSE GRAMMAR SCHOOL & OTHER PLACES IN UC-09**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7000 Sft | 773.86%  Sft | 54170/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 28263 Cft | 1437.00%0  Cft | 40614/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 31203 Cft | 1065.00%  Cft | 332312/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **6,81,619/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR OF ROAD / FILLING OF DAMAGES ROAD BY CARPETING NEAR SOFAID CHOWK AND ROSE GRAMMAR SCHOOL & OTHER PLACES IN UC-09**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 2925 Cft | Offer Rate | Offer Rate |
| 02 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 2820 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/08**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LYING RCC PIPE STREET NO. 3 AND 1 SHAH WALIULLAH NAGAR UC-7.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.2,22,539 /= + O/R*

*BID SECURITY.* Rs. *4,451 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/08**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 2,22,539 /= + O/R*

Earnest Money *RS. 4,451 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LYING RCC PIPE STREET NO. 3 AND 1 SHAH WALIULLAH NAGAR UC-7.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1500  Sft | 4650.00 %0 CFT | 6975/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 200  Cft | 10770.00 %0 CFT | 2154/= |
| 03 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed b engineer in charge (64/10) | 150  Cft | 24510.00 %0 Cft | 3677/= |
| 04 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  15” DIA | 300  RFT | 206.00 RFT | 61,800/= |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 14 Nos | 13064 /= Each | 1,82,896/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -25  Rft | 1540.00 RFT | -38,500/= |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1425  Cft | 2760.00 %0 CFT | 3933/= |
| **SUB TOTAL PART-A** | | | | **2,22,539/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LYING RCC PIPE STREET NO. 3 AND 1 SHAH WALIULLAH NAGAR UC-7.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Providing& Fixing pre cost RCC Ring Slab 39” Dia with RCC Main hole Cover 21” Dia as per direction | 250 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/09**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF ROAD AND CC STREET NEAR YAMEEN BLOCK WORKS AND OTHER PLACES IN UC-.4**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,30,876 /= + O/R*

*BID SECURITY.* Rs. *10,618 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/09**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 5,30,876 /= + O/R*

Earnest Money *RS. 10,618 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

Subject: **REHABILITATION OF ROAD AND CC STREET NEAR YAMEEN BLOCK WORKS AND OTHER PLACES IN UC-.4**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 384 Cft | 4650.00 %0 CFT | 17,86/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 96 Rft | 206.00 RFT | 19m776/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 4 Nos. | 13064 /= Each | 52,256/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -7 Rft | 1540.00 RFT | -10,780/= |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 309 Cft | 2760.00 %0 CFT | 853/= |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 12,709 Cft | 1065.00% CFT | 1,35,351/= |
|  | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12,163 | 1437.00%0  Cft | 17,478/= |
| 05 | Premixed Patch Repair 1” thick including cleaning cutting scattered patches in proper shapes laying premixed chips, rolling etc complete (Rate i/c all cost of materials T&P and carriage upto 3 chains) P-09/19 using Crushed Bajri laying premixed carpet | 3100 Sft | 4765.11%  Sft | 1,47,718/= |
|  | Dismantling of cement concrete, flooring 1:2:4 Plain etc | 546 Sft | 3327.50% Cft | 18,168/= |
|  | Preparing of Sub-Grade including Earth Excavation leveling to an average depth of 9” dressing & camber etc. | 3900 Sft | 526.28% Sft | 20,525/= |
|  | Providing and Laying CC Toping 1:2:4 including surface finishing and dividing into panel etc. | 3900 Sft | 3275.50% Sft | 1,27,745/= |
| **SUB TOTAL PART-A** | | | | **5,30,876/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Signature of Contractor***

Subject: **REHABILITATION OF ROAD AND CC STREET NEAR YAMEEN BLOCK WORKS AND OTHER PLACES IN UC-.4**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
|  | Supplying & Filling of imported earth within the radios of 5 miles including digging, loading & unloading all lead & lifts and leveling & compacting | 2,438 Cft | Offer Rate | Offer Rate |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 3000  Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3500  Cft | Offer Rate | Offer Rate |
| 03 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 40 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/10**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF ROAD BY CARPETING NER JAMA MADNI WESTERN GRAMMER SCHOOLDIAMOND ELECTRONIC NEAR MUHAJIR CHOWK IN UC-03**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,88,129/= + O/R

*BID SECURITY.* Rs. 13,763 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/10**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,88,129/= + O/R

Earnest Money Rs. 13,763 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REHABILITATION OF ROAD BY CARPETING NER JAMA MADNI WESTERN GRAMMER SCHOOL DIAMOND ELECTRONIC NEAR MUHAJIR CHOWK IN UC-03**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15,280 Cft | 1065.00%  Cft | 161933/- |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| 07 ` | P/F 1:2:4 RCC Main holes cover i/c tor bars frame using GSB ¾ and down guage etc complete (Ch-16/13-1) | 08 Nos | 913 Each | 7309/- |
| **SUB TOTAL PART-A** | | | | **6,88,129/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF ROAD BY CARPETING NER JAMA MADNI WESTERN GRAMMER SCHOOL DIAMOND ELECTRONIC NEAR MUHAJIR CHOWK IN UC-03**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2200 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/11**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMP/REPAIR OF ROAD BY CARPETING NEAR ISLAM CHOWK, MASJID KHALIL IN UC-09**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,55,664 /= + O/R

*BID SECURITY.* Rs. 15,113 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/11**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,55,664 /= + O/R

Earnest Money Rs. 15,113 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **IMP/REPAIR OF ROAD BY CARPETING NEAR ISLAM CHOWK, MASJID KHALIL IN UC-09**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6500 Sft | 773.86%  Sft | 50301/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 27143Cft | 1065.00%  Cft | 28073/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 8000Sft | 4765.11%Sft | 381209/- |
| **SUB TOTAL PART-A** | | | | **7,55,664/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMP/REPAIR OF ROAD BY CARPETING NEAR ISLAM CHOWK, MASJID KHALIL IN UC-09**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 |  |  |  |  |
|  | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 800 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/12**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR AND MAINTENANCE OF ROAD BY CARPETING NEAR ZAMZAM**

**MILK SHOP SECTOR 11-A IN UC-4.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,60,816 /= + O/R*

*BID SECURITY.* Rs. *15,216 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/12**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.7,60,816 /= + O/R*

Earnest Money *RS.15,216 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

Subject: **REPAIR AND MAINTENANCE OF ROAD BY CARPETING NEAR ZAMZAM**

**MILK SHOP SECTOR 11-A IN UC-4.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7200 SFT | 773.86%  Sft | 55,718/= |
| 02 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 28,013 Cft | 1065.00% CFT | 2,98,338/= |
| 03 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24,413 | 1437.00%0  Cft | 35,081/= |
| 04 | Premixed Patch Repair 1” thick including cleaning cutting scattered patches in proper shapes laying premixed chips, rolling etc complete (Rate i/c all cost of materials T&P and carriage upto 3 chains) P-09/19 using Crushed Bajri laying premixed carpet | 7800 Sft | 4765.11%  Sft | 3,71,679/= |
| **SUB TOTAL PART-A** | | | | **7,60,816/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR AND MAINTENANCE OF ROAD BY CARPETING NEAR ZAMZAM MILK SHOP SECTOR 11-A IN UC-4.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 800  Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3600  Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/13**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF ROAD DUBBA MOOR AND MUMMADI IRON WORKS AND MAIN ROAD IN MUHAMMAD MUTAFA COLONY UC-7.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,81,540 /= + O/R

*BID SECURITY.* Rs. 13,631 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/13**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,81,540 /= + O/R

Earnest Money Rs. 13,631 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REHABILITATION OF ROAD DUBBA MOOR AND MUMMADI IRON WORKS AND MAIN ROAD IN MUHAMMAD MUTAFA COLONY UC-7.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15272.58 Cft | 1065.00%  Cft | 162,653/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| **SUB TOTAL PART-A** | | | | **681,540/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF ROAD DUBBA MOOR AND MUMMADI IRON WORKS AND MAIN ROAD IN MUHAMMAD MUTAFA COLONY UC-7.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2320 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/14**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR OF CC WORK HOUSE NO. 420 AND CATTLE YARD WALI GALI AND HOUSE NO. 411 IN UC-10 ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,47,491 /= + O/R

*BID SECURITY.* Rs. 12,950 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/14**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,47,491 /= + O/R

Earnest Money Rs. 12,950 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **14-REPAIR OF CC WORK HOUSE NO. 420 AND CATTLE YARD WALI GALI AND HOUSE NO. 411 IN UC-10 ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 750  Sft | 4650.00%  Sft | 3,488/= |
| 02 | Excavation of Pipe line in trenches & pits in hard rock by hammering and chieslling i/c alignment & shape leveling and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (64/10) | 1125  Cft | 24150.00%  Cft | 27,574/= |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 250  Rft | 367.00  Rft | 91,750/= |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 11 Nos. | 13064  Each | 143,704/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 22  Rft | 1540.00  Rft | (-)33,880/= |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 750  Cft | 2760.00%0  Cft | 2,070/= |
| 07 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-C) | 1024  Cft | 3327.50%  Cft | 34,074/= |
| 08 | Dismantling of cement concrete flooring 1:3:6 plain. (Ch-2/10/19-b) | 1149  Cft | 1306.80%  Cft | 15,015/= |
| 09 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2022.16  Cft | 1065.04%  Cft | 21,536/= |
| 10 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 9000  Sft | 526.28%  Sft | 47,365/= |
| 11 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9000  Sft | 3275.50%  Sft | 294,795/= |
| **SUB TOTAL PART-A** | | | | **647,491/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR OF CC WORK HOUSE NO. 420 AND CATTLE YARD WALI GALI AND HOUSE NO. 411 IN UC-10 ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 11 Nos. | Offer Rate | Offer Rate |
| 02 | S/F Imported Earth with in the a radius of 5 miles i/c digging, loading, unloading all lead and lift leveling and water compaction etc complete. | 1125  Cft | Offer Rate | Offer Rate |
| 03 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2660 Cft | Offer Rate | Offer Rate |
| 04 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3780  Cft | Offer Rate | Offer Rate |
| **05** | Using SR Cement in place of OPC | 245 CWT | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/15**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR HOUSE NO. 2652/KS & DIFFERENT PLACE IN UC-2**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,18,635/= + O/R*

*BID SECURITY.* Rs. 12,372/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/15**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,18,635/= + O/R*

Earnest Money RS. 12,372/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR HOUSE NO. 2652/KS & DIFFERENT PLACE IN UC-2**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2530 Cft | 4650.00 %0 CFT | 11,765 |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 460 Rft | 206.00 Rft | 94760/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 21 Nos | 13064 /= Each | 2,74,344/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -47 | 1540.00 RFT | -72,380/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2169 | 2760.00 %0 CFT | 5986/= |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 8000 | 526.28%  Sft | 42120/= |
| 08 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 8000 | 3275.50%  Sft | 262040/= |
| **SUB TOTAL PART-A** | | | | **6,18,635/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR HOUSE NO. 2652/KS & DIFFERENT PLACE IN UC-2**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 5355 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 1008 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2000 Cft | Offer Rate | Offer Rate |
| 04 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 231 Cwt | Offer Rate | Offer Rate |
| 05 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 15 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/16**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR AND MAINTENANCE OF SWEARGE SYSTEM IN SHAH FAISAL MOHALLAH IN UC-13.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,03,448 /= + O/R*

*BID SECURITY.* Rs. *18,069 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/16**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,03,448 /= + O/R*

Earnest Money *RS. 18,069 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR AND MAINTENANCE OF SWEARGE SYSTEM IN SHAH FAISAL MOHALLAH IN UC-13.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2596 Cft | 3327.50 %  Cft | 86382/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2600 Cft | 4650.00 %0 CFT | 12090/= |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2475 Cft | 10770.00 %0 CFT | 26656/= |
| 04 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 800 Rft | 367.00  RFT | 293600/= |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 38 Nos | 13064 /= Each | 496432/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -66.5 Rft | 1540.00 RFT | -102410/= |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1745 Cft | 2760.00 %0 CFT | 4841/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 5917 Cft | 1065.00% CFT | 63016/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 25 Nos | 913.63 | 22841/= |
| **SUB TOTAL PART-A** | | | | **9,03,448/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR AND MAINTENANCE OF SWEARGE SYSTEM IN SHAH FAISAL MOHALLAH IN UC-13.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 15 Nos | Offer Rate | Offer Rate |
| 02 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1650 Cft | Offer Rate Each | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/17**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: REHABILITATION OF CC STREET NEAR HOUSE NO. 887 TAUHEED COLONY IN

**UC-5.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,07,884* /= + O/R

*BID SECURITY.* Rs. *12,158*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/17**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *6,07,884* /= + O/R

Earnest Money Rs. *12,158*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: REHABILITATION OF CC STREET NEAR HOUSE NO. 887 TAUHEED COLONY IN

**UC-5.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 3675 Cft | 3327.50%  Cft | 122,286/= |
| 02 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 1116 Cft | 1306.80%  Cft | 14,584/= |
| 03 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 2160 Cft | 1437.00%0  Cft | 3,104/= |
| 04 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 6951 Cft | 1065.00% CFT | 74,028/= |
| 05 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 10000 Sft | 526.28%  Sft | 52,628/= |
| 06 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10000 Sft | 3275.50%  Sft | 327,550/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 15 Nos. | 913.63  Each | 13,704/= |
| **SUB TOTAL PART-A** | | | | **607,884/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF CC STREET NEAR HOUSE NO. 887 TAUHEED COLONY IN UC-5.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 9000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3300 Cft | Offer Rate | Offer Rate |
| 03 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 289 Cwt | Offer Rate | Offer Rate |
| 04 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 10 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/18**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **SYSTEMIC SALARY SYSTEM NEAR HOUSE OF HAJI GHULAM MUSTAFA KS/2522 KS/2512 IN TOORI BANGHASH COLONY IN UC-7.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 8,91,713/= (+) O/R

*BID SECURITY.* Rs. 17,834/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/18**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 8,91,713/= (+) O/R

Earnest Money Rs. 17,834/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **SYSTEMIC SALARY SYSTEM NEAR HOUSE OF HAJI GHULAM MUSTAFA KS/2522 KS/2512 IN TOORI BANGHASH COLONY IN UC-7.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete 1:2:4 | 2596 Cft | 3327.50 % Cft | 8,985/= |
| 02 | Excavation for pipe line in trenches & pits in all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer incharge | 2600 Cft | 4650.00%0 Cft | 23,543/= |
| 03 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge | 2475 Cft | 24150.00%0 Cft | 89609/= |
| 04 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete.  12” DIA | 800 Rft | 367.00 Rft | 330,300/= |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &bedding cast in situ with fair face steel shuttering i/c excavation, back filling & disposal of surplus stuff etc. complete | 40 No. | 13064/=  Each | 496,432/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -70 Rft | 1540.00Rft | -86,106/= |
| 08 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 1754 ft | 2760.00%0 Cft | 21,015/= |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) |  | 1065.00% CFT | 160538/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia |  | 913.63 |  |
| **SUB TOTAL PART-A** | | | | **9,24,186/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **SYSTEMIC SALARY SYSTEM NEAR HOUSE OF HAJI GHULAM MUSTAFA KS/2522 KS/2512 IN TOORI BANGHASH COLONY IN UC-7.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth within the radius of 5 miles i/c digging, loading, unloading, all lead and lift leveling and watering and compacting etc complete . | 3290 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/19**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF SEWERAGE SYSTEM NEAR MADINA STORE FAIZ-E-AAM COLONY NEAR BILMILLAH STORE MOMINABAD ZIA COLONY UC-1**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,60,324* /= + O/R

*BID SECURITY.* Rs. *17,206*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/19**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,60,324* /= + O/R

Earnest Money Rs. *17,206*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REHABILITATION OF SEWERAGE SYSTEM NEAR MADINA STORE FAIZ-E-AAM COLONY NEAR BILMILLAH STORE MOMINABAD ZIA COLONY UC-1**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement  Concrete plain flooring. (10/19 a-b-c) C.C 1:2:4 | 2133  Cft | 3327.50 % CFT | 70976/= |
| 02 | Dismantling and removing of stone metaling and carpeting etc (13/51) | 630  Cft | 605.00 % CFT | 3812/= |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 270  Cft | 4650.00 %0 CFT | 1256/= |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 1031  Cft | 10770.00 %0 CFT | 11104/= |
| 05 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 2441  Cft | 24150.00%0CFT | 58950/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  15” DIA | 150 Rft  288 Rft | 367.00 RFT  436.00 RFT | 55050/=  125568/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling &complete (app/rate) | 30  Nos | 13064 /= Each | 391920/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 36.25  Rft | 1540.00 RFT | -55825/= |
| 09 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 872  Cft | 2760.00 %0 CFT | 2407/= |
| 10 | P/L 1:3:6 CC using GSB ¾” and down guage i/c consolidation, curing etc complete without shuttering. (16/5-h) | 90  Cft | 12595.00 % CFT | 11336/= |
| PAGE NO.2 | | | | |
| 11 | Earth work excavation in irrigation channels irrigation draiaetc dressed to designed section and profile excavated material disposed off and dressed with in 50 ft lead. (Ordinary Soil) (ch-1-1/5) | 9600  Cft | 2420.00 %0 CFT | 23232/= |
| 12 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 15074  Cft | 1065.00% CFT | 160538/= |
| **SUB TOTAL PART-A** | | | | 860324/= |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF SEWERAGE SYSTEM NEAR MADINA STORE FAIZ-E-AAM COLONY NEAR BILMILLAH STORE MOMINABAD ZIA COLONY UC-1**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 2000  Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 1000  Cft | Offer Rate | Offer Rate |
| 03 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 05 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/20**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,60,816/= + O/R

*BID SECURITY.* Rs. 15,216 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/20**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,60,816/= + O/R

Earnest Money Rs. 15,216 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7200 Sft | 773.86%  Sft | 55718/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 28013 Cft | 1065.00%  Cft | 298338/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **7,60,816/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 |  |  |  |  |
|  | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 800 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/21**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIRING / IMPROVEMENT OF CARPET SUBHAN BLOCK WORKS AND SHAHANI HALL IN UC-10.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,76,854*/= (+) O/R

*BID SECURITY.* Rs. *13,537*/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/21**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *6,76,854*/= (+) O/R

Earnest Money Rs. *13,537*/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **REPAIRING / IMPROVEMENT OF CARPET SUBHAN BLOCK WORKS AND SHAHANI HALL IN UC-10.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material of designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming it banks or putting the same on combankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12354 Cft | 1437.00%0  Cft | 17,753/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 14822.5 Cft | 1065.00%  Cft | 157,860/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| **SUB TOTAL PART-A** | | | | **676,854/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIRING / IMPROVEMENT OF CARPET SUBHAN BLOCK WORKS AND SHAHANI HALL IN UC-10.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2576 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3656 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/22**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPE GALI NO. 11 GHAZIABAD IN UC-6 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,77,659/= + O/R*

*BID SECURITY.* Rs. 17,553 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/22**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,77,659/= + O/R*

Earnest Money RS. 17,553 /= + O/R

Tender Cost Rs. 1,0,00.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPE GALI NO. 11 GHAZIABAD IN UC-6 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 368 Cft | 1306.80%  Cft | 4,809/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 3000 Cft | 4650.00 %0 CFT | 13950/= |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2000 | 10770.00 %0 CFT | 21540/= |
| 04 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA  12” DIA | 200 Rft  800 Rft | 206.00 RFT  367.00 RFT | 41,200/=  2,93,600 |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 45 Nos | 13064 /= Each | 5,87,880/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -82.5 | 1540.00 RFT | -1,27,050 |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1957 | 2760.00 %0 CFT | 5401/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3411 | 1065.00% CFT | 36329/= |
| **SUB TOTAL PART-A** | | | | **8,77,659/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING RCC PIPE GALI NO. 11 GHAZIABAD IN UC-6 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 2000 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/23**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIRING OF CC STREET AND ROAD NEAR SHAKIR PAN SHOP AND OTHER PLACES IN UC-4.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,64,390* /= + O/R

*BID SECURITY.* Rs. *11,288*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/23**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,64,390* /= + O/R

Earnest Money Rs. *11,288*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REPAIRING OF CC STREET AND ROAD NEAR SHAKIR PAN SHOP AND OTHER PLACES IN UC-4.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 13632 Cft | 1437.00%0  Cft | 19,589/= |
| 02 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 13632 Cft | 1065.00% CFT | 145,181/= |
| 03 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 25550 Sft | 526.28%  Sft | 134,465/= |
| 04 | P/L 1.5” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 3000 Sft | 2548.29%  Sft | 76,449/= |
| 05 | Premixed Patch Repair 1” thick including cleaning cutting scattered patches in proper shapes laying premixed chips, rolling etc complete (Rate i/c all cost of materials T&P and carriage upto 3 chains) P-09/19 using Crushed Bajri laying premixed carpet | 3500 Sft | 4765.11%  Sft | 166,779/= |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame usingm GSB 3/4” and down gauge etc complete (ch-16/31-1)  21” Dia | 24 Nos. | 913.63 Each | 21,927/= |
| **SUB TOTAL PART-A** | | | | **564,390/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIRING OF CC STREET AND ROAD NEAR NEAR SHAKIR PAN SHOP & OTHER PLACES IN UC-4.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 6953 Cft | Offer Rate | Offer Rate |
| 02 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 18 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/24**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **MOTORABLE MAIN LINK ROAD IN FRONT OF TOORI BANGASH POLICE CHOWKI 1-D BUS STOP ROUTE & NISAR ISMAIL KHAN BLOCK WORKS IN UC-7, NEAR DARUL-SADIQABAD, ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.1,24,202* /= + O/R

*BID SECURITY.* Rs. *2484* /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/24**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *1,24,202* /= + O/R

Earnest Money Rs. *2484* /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **MOTORABLE MAIN LINK ROAD IN FRONT OF TOORI BANGASH POLICE CHOWKI 1-D BUS STOP ROUTE & NISAR ISMAIL KHAN BLOCK WORKS IN UC-7, NEAR DARUL-SADIQABAD, ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-c) | 1834  Cft | 3327.50 %  Cft | 61048/= |
| 02 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 12000  Sft | 526.28%  Sft | 63154/= |
| **SUB TOTAL PART-A** | | | | **124202/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **MOTORABLE MAIN LINK ROAD IN FRONT OF TOORI BANGASH POLICE CHOWKI 1-D BUS STOP ROUTE & NISAR ISMAIL KHAN BLOCK WORKS IN UC-7, NEAR DARUL-SADIQABAD, ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 6250  Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 11319  Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/25**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,51,672/= + O/R

*BID SECURITY.* Rs. 15,033 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/25**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,51,672/= + O/R

Earnest Money Rs. 15,033 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6500 Sft | 773.86%  Sft | 50301/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 27663 Cft | 1065.00%  Cft | 294611/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **7,51,672/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 800 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/26**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND CC TOPPING IN GALI # 5 SHAHFAISAL MOHALLAH IN UC-13**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,27,353 /= + O/R*

*BID SECURITY.* Rs. *16,547/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/26**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,27,353 /= + O/R*

Earnest Money *RS. 16,547/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND CC TOPPING IN GALI # 5 SHAHFAISAL MOHALLAH IN UC-13**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer incharge | 3300 Cft | 4650.00%0 Cft | 15345/- |
| 02 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 600 Cft | 10770.00 % 0  1000 CFT | 220200/- |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 30 Nos | 13064 /= Each | 391920/- |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -45.139 Rft | 1540.00 RFT | (-)69514/- |
| 05 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2565 Cft | 2760.00 %0 CFT | 7079 |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 6900 Sft | 526.28%  Sft | 36313/- |
| 07 | P/L 1 ½” thick topping cc 1:2:4 i/c surface finishing & dividing in to panels (42/16-b-c-d) 2” thick cc 1:2:4 topping | 6900 Cft | 1065.00% CFT | 226010/- |
| **SUB TOTAL PART-A** | | | | **8,27,353/=**  **+O/R** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND CC TOPPING IN GALI # 5 SHAHFAISAL MOHALLAH IN UC-13**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 1250  Cft | Offer Rate | Offer Rate |
| 02 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 06 Nos. | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 1725 Cft | Offer Rate | Offer Rate |
| 04 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 199 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/27**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **MAINTENANCE AND REPAIR OF PIPE AND CC STREET NEAR MASJID BAB-E-REHMAT MOMINABAD IN UC-1.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,03,958 /= + O/R*

*BID SECURITY.* Rs. *16,079 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/27**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.8,03,958 /= + O/R*

Earnest Money *RS.16,079 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **MAINTENANCE AND REPAIR OF PIPE AND CC STREET NEAR MASJID BAB-E-REHMAT MOMINABAD IN UC-1.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | Excavation for pipe line in trenches & pits in hard rock by hammering and chieslling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge | 1375 Cft | 10770.00%0  Cft | 14,809/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 200 Rft | 367.00 RFT | 73,400/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 9 Nos. | 13064 /= Each | 1,17,576/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -15.76 Rft | 1540.00 RFT | -24,255/= |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1164 Cft | 2760.00 %0 CFT | 3,213/= |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 2777 Cft | 1065.00% CFT | 29575/= |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2296 Cft | 3327.50 %  Cft | 76,399/= |
| 10 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 13,500  Sft | 526.28%  Sft | 71,048/= |
| 11 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 13500  Sft | 3275.50%  Sft | 4,42,193/= |
| **SUB TOTAL PART-A** | | | | **8,03,958/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **MAINTENANCE AND REPAIR OF PIPE AND CC STREET NEAR MASJID BAB-E-REHMAT MOMINABAD IN UC-1.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 960  Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3950  Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/28**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIRING & CLEANING OF NALLAH & OTHER WORK IN SECTOR 11 ½ PAKISTAN BAZAR ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,15,000 /= + O/R*

*BID SECURITY.* Rs. *14,300 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/28**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.7,15,000 /= + O/R*

Earnest Money *RS. 14,300 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIRING & CLEANING OF NALLAH & OTHER WORK IN SECTOR 11 ½ PAKISTAN BAZAR ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of RCC concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 950 Cft | 5445.0% Cft | 51728/- |
| 02 | Dismantling of CC flooring. 1:2:4 plain (Ch-2/10/19c) | 938 Cft | 3327.50 %  Cft | 31212/- |
| 03 | Earth work excavation in irrigation channels, irrigation drain etc dressed to designed section and profile excavated. | 9970 Cft | 2420.00%0  Cft | 24127/- |
| 04 | Cement Concrete plan 1:2:4 i/c placing, compacting, curing etc complete i/c screening & washing of stone aggregate without shuttering. (17/5-1) | 840 Cft | 14429.25% Cft | 121206/- |
| 05 | Erection and removal of centering for RCC or plane CC Work in partal wood (Vertical) 18/19-b-ii | 2520 Sft | 3127.41 % Sft | 78811/- |
| 06 | Fabrication of steel reinforcement for cement concrete i/c cutting, bending, binding & laying in postion, making joints & fastening i/c the cost of binding works and removal of rust from bars. | 15.36 Wct | 5001.70 per  Cwt | 76826/- |
| 07 | RCC work i/c all labor & material except the cost of reinforcement and its labor for bending binding which will be paid separately. This rate also i/c all kinds of forms, molds, lifting, shuttering, cutting, rendering & finishing the expose surface i/c screening & wishing of shingles. Ratio 1:2:4 | 600 Cft | 337.00 Cft | 202200/- |
| 08 | Bailing or pumping out sub soil water during excavation concrete cast in situ or masonry work in foundation. Only three operation allowed.  (ch-11-75/181) | 479.20 Cft | 543.00 % Cft | 2602/- |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11858 Cft | 1065.00% CFT | 1,26288/= |
| **SUB TOTAL PART-A** | | | | **7,15,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIRING & CLEANING OF NALLAH & OTHER WORK IN SECTOR 11 ½ PAKISTAN BAZAR ORANGI ZONE**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
|  | P/F RCC pre cast slab or i/c linter (I-beam) of required size and shape and and racking out joints with CM curing etc complete as per direction of engineer incharge  (Each 1x3.5x2.0) | 1050 Sft | Offer Rate  (Per Sft ) | Offer Rate |
|  | P/F RCC pre cast slab or linter of required size and shape and racking out joints with CM curing etc complete as per direction of engineer inchargev  48x3.5x1.25x0.33 | 69 Cft | Offer Rate  (per Cft) | Offer Rate |
|  |  |  |  |  |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/29**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PATCH REPAIR OF ROAD MULANA SHOUKAT ALI ROAD / OTHER WORK AND OTHER AREA IN UC-05 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,25,000*/= (+) O/R

*BID SECURITY.* Rs. *12,500*/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/29**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *6,25,000*/= (+) O/R

Earnest Money Rs. *12,500*/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

SUBJECT: **PATCH REPAIR OF ROAD MULANA SHOUKAT ALI ROAD / OTHER WORK AND OTHER AREA IN UC-05 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete 1:2:4 | 1868 Cft | 3327.50 % Cft | 62158/- |
| 02 | Earth work excavation of road side nalis forming it banks or putting the same on combankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 5713 Cft | 1437.00%0  Cft | 8210/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 7692Cft | 1065.00%  Cft | 81920/- |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 7550 Sft | 526.28%  Sft | 39734/- |
| 05 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8500 Sft | 5093.86%  Sft | 432978/- |
| 06 |  |  |  |  |
| **SUB TOTAL PART-A** | | | | **6,25,000/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **PATCH REPAIR OF ROAD MULANA SHOUKAT ALI ROAD / OTHER WORK AND OTHER AREA IN UC-05 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2500 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 4250 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 18 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/30**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING RING OF DIFFERENT DIA AND OTHER WORK IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.Offer Rate*

*BID SECURITY.* Rs. 2% *Offer Rate*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/30**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *O/R*

Earnest Money *2% + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING RING OF DIFFERENT DIA AND OTHER WORK IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 280 Nos. | Offer Rate | Offer Rate |
| 02 | Providing RCC Precast slab.etc. | 400 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

Cell # / PTCL #.

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/31**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **PROVIDING & LYAING RCC PIPE NEAR MONGA CHOWK & BLOCK B MPR COLONY UC-13 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 9,13,817/= (+) O/R

*BID SECURITY.* Rs. 18,276/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/31**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 9,13,817/= (+) O/R

Earnest Money Rs. 18,276/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

Subject: **PROVIDING & LYAING RCC PIPE NEAR MONGA CHOWK & BLOCK B MPR COLONY UC-13 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) | 2596 Cft | 3327.50 % CFT | 86382/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2600 Cft | 4650.00%  Sft | 12090/- |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2475 Cft | 10770.00 %0 CFT | 26656/= |
| 04 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 800  Rft | 367.00  Rft | 2,93,600/- |
| 05 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 39 Nos. | 13064  Each | 5,09,496/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 68.25  Rft | 1540.00  Rft | -105105/- |
| 07 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 1754  Cft | 2760.00%0  Cft | 4841/- |
| 08 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 5917  Cft | 1065.04%  Cft | 63016/- |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 25 Nos. | 913.63  Each | 22841/- |
| **SUB TOTAL PART-A** | | | | **9,13,817/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **PROVIDING & LYAING RCC PIPE NEAR MONGA CHOWK & BLOCK B MPR COLONY UC-13 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Supplying and Filling Imported Earth with in the redius of Five Miles i/c digging laoding and unloading all lead and lift leveling and compacting e.t.c. | 1650 | Offer Rate | Offer Rate |
| 02 | P/F Per Cost RCC Ring Slab 39” dia with R.C.C Manhole cover of 21” dia as per direction of engineer incharge | 11 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/32**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION SEWERAGE SYSTEM BY RCC PIPE 12” DIA ZIA COLONY BIJLI NAGAR SECTOR 4 MOMINABAD IN ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,98,211 /=*

*BID SECURITY.* Rs. *19,964 /=*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/32**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,98,211 /=*

Earnest Money *RS. 19,964 /=*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION SEWERAGE SYSTEM BY RCC PIPE 12” DIA ZIA COLONY BIJLI NAGAR SECTOR 4 MOMINABAD IN ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete 1:2:4 | 2206 Cft | 3327.50 % Cft | 73,405/- |
| 02 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 7938.70 Cft | 1065.00% CFT | 84547/- |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 4310 Cft | 4650.00 %0 CFT | 20042/- |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammering and chieslling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge | 1248 Cft | 10770.00 % 0  Cft | 13441/- |
| 05 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  8” DIA | 500 Rft  624Rft | 367.00  RFT  206Rft | 183500/-  128544/- |
| 06 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 48 Nos | 13064 /= Each | 627072/- |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-)103.50 Rft | 1540.00 RFT | (-)159390/- |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 4540 Cft | 2760.00 %0 CFT | 12530/- |
| 09 | Earth work excavation in irrigation channels irrigation draiaect dressed to designed section and profile excavated material disposed off and dressed with in 50 ft lead. (Ordinary Soil) (ch-1-1/5) | 600Cft | 2420.0% 0Cft | 14520/- |
| **SUB TOTAL PART-A** | | | | **9,98,211 /=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/33**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR OF RCC PIPE NEAR MADARSA EJJAZ UL QURAN GALI NO. 36 NEAR REHMAT CHOWK IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,22,125 /= + O/R*

*BID SECURITY.* Rs. *18,443/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/33**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,22,125 /= + O/R*

Earnest Money *RS. 18,443/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR OF RCC PIPE NEAR MADARSA EJJAZ UL QURAN GALI NO. 36 NEAR REHMAT CHOWK IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1880 Cft  418Cft | 3327.50 %  Cft  5445.0 % | 62,557/=  22760/= |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2100 Cft | 4650.00 %0 CFT | 9765/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA  15” DIA | 800 Rft | 367.00 RTF | 293600/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall & beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 38 Nos | 13064 /= Each | 496432 |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -61.75 Rft | 1540.00 RFT | -95095 |
| 09 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1120 Cft | 2760.00 %0 CFT | 3091/= |
| 10 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 10478 Rft | 1065.00% CFT | 111591/= |
| 11 | Earth work excavation in irrigation channels irrigation draiaetc dressed to designed section and profile excavated material disposed off and dressed with in 50 ft lead. (Ordinary Soil) (ch-1-1/5) | 7200  Cft | 2420.00 %0 CFT | 17424/= |
| **SUB TOTAL PART-A** | | | | **9,22,125/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR OF RCC PIPE NEAR MADARSA EJJAZ UL QURAN GALI NO. 36 NEAR REHMAT CHOWK IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F RCC pre cast slab or linter of required size and shape and shape as per given design and racking out joints with CM curing etc complete as per direction of engineer incharge | 153 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/34**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION SEWERAGE SYSTEM IN BALOUCH PARA AND ALIABAD IN UC-13 ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,24,186 /= + O/R*

*BID SECURITY.* Rs. *18,484 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/34**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,24,186 /= + O/R*

Earnest Money *RS. 18,484 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION SEWERAGE SYSTEM IN BALOUCH PARA AND ALIABAD IN UC-13 ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete 1:2:4 | 2596 Cft | 3327.50 % Cft | 86382/= |
| 02 | Excavation for pipe line in trenches & pits in all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer incharge | 2600 Cft | 4650.00%0 Cft | 12090/= |
| 03 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 2475 Cft | 10770.00 % 0  1000 CFT | 26657/= |
| 04 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 800 Rft | 367.00  RFT | 293600/= |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 40 Nos | 13064 /= Each | 522560/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -70 Rft | 1540.00 RFT | -107800 |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1757 Cft | 2760.00 %0 CFT | 4841/= |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 5917 Cft | 1065.00% CFT | 63016/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 25 Nos | 913.63 | 22841/= |
| **SUB TOTAL PART-A** | | | | **9,24,186/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION SEWERAGE SYSTEM IN BALOUCH PARA AND ALIABAD IN UC-13 ORANGI ZONE.**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1650 Cft | Offer Rate | Offer Rate |
|  | Providing & Laying RCC Ring Slab 39” Dia with RCC Cover 21” Dia as per direction. | 8 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

DISTRICT MUNICIPAL CORPORATION, KARACHI WEST. 04/35

SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.

PTCL # 366697869 /36660102& FAX # 36762519

TENDER REFERENCE # NIT/\_\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: RENOVATION OF BUILDING I/C ELECTRIC WORKS AND FITTING, TILLING PLASTERING

ON WALLS AND OTHER SIMILAR WORKS.

BILL OF QUANTITIES.

*ESTIMATED COST. RS: 3,35,400/=(+) O/R.*

*BID SECURITY. RS. 6,708 /= (+) O/R.*

*TENDER COST. RS. 1,000/=*

*PENALTY. RS. 1,000/= PER DAY.*

Issued to M/S.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp.

DISTRICT MUNICIPAL CORPORATION, KARACHI WEST. 04/35

SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.

PTCL # 366697869 /36660102& FAX # 36762519

Estimated Cost Rs: 3,35, 400/=(+) O/R

Earnest Money Rs. 6,708/= (+) O/R

Tender Cost. Rs. 1,,000/=

Time Limit.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Penalty Rs. 1,000/= Per Day.

SUBJECT: RENOVATION OF BUILDING I/C ELECTRIC WORKS AND FITTING, TILLING PLASTERING

ON WALLS AND OTHER SIMILAR WORKS.

PART-A ITEM BASED ON SCHEDULE RATES

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.# | DESCRIPTION | QUANTITY | RATE/UNIT | AMOUNT. |
| 01 | P/L. Tiles glared 6”x6” x ¼” on floor or wall in required clour or Pdettren jointed in white cement, and pigment i/c washing and filling of joints with salary of white cement etc complete. | 1099.33 SFT | 30509.77 % SFT | 3,35,400/= |
| SUB TOTAL PART-A. RS: | | | | 3,35,400/=(+) O/R |

SIGNATURE OF CONTRACTOR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

DISTRICT MUNICIPAL CORPORATION, KARACHI WEST. 04/35

SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.

PTCL # 366697869 /36660102& FAX # 36762519

SUBJECT: RENOVATION OF BUILDING I/C ELECTRIC WORKS AND FITTING, TILLING PLASTERING

ON WALLS AND OTHER SIMILAR WORKS.

PART-B ITEM BASED ON OFFER RATES.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SL.# | DESCRIPTION | QUANTITY | RATES | AMOUNT |
| 01 | Distempering on walls with approved shade and make i/c scraping old surface etc. | 6940 SFT | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 02 | Cement plaster on walls up to 20ft height and ¾” thick i/c edges and genera and curing etc. | 100 SFT | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 03 | P/F. Electric pints with switch and socket and wiring with best quality electric wire. Etc. complete. | 200 Nos | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 04 | P/F. Wiring for mic system in Hall. , with best quality wire. | 01 No.  Complete Job | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 05 | P/S. Office chairs of iron rod. | 04 Nos. | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 06 | P/F. English commode with all fitting and seat cover. | 04 Nos | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 07 | P/F. Door lock best quality | 10 Nos. | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 08 | P/F. Best quality brass bib cock. | 08 Nos. | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 09 | P/S. Dispensar water. | 02 Nos | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 10 | Toilet Set complete. | 04 Nos | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

SIGNATURE OF CONTRACTOR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ADDRESS: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

I/WE HEREBY QUOTED RATES AS FOLLOWS:-

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (ITEM RATES BASES ON SR)  @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ % ABOVE / BELOW SR I/C THE COST OF CARRIAGE OF MATERIALS AND DIFFERENCE OF COST OF BITUMEN. | RS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 02 | PART-B (ITEM RATE BASES ON OFFER RATES/ITEM RATES THE ITEMS OTHER THEN SCHEDULE RATES | RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| GRAND TOTAL PART-A & B | | RS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

TOTAL RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ RUPEES\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature of contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Cell #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/ PTCL #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/36**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING SUPPLYING RCC COVER OF DIFFERENT DIA IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.2,74,089 /= + O/R*

*BID SECURITY.* Rs. *5,482/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/36**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 2,74,089 /= + O/R*

Earnest Money *RS. 5,482/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING SUPPLYING RCC COVER OF DIFFERENT DIA IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Providing & Laying 1:2:4 RCC Main Hole Cover including Toorbar Framing using GSB ¾ “ and down gauge 21” Dia etc. | 300 Nos | 913.63 Each | 274089/= |
|  | | | | **274089/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING SUPPLYING RCC COVER OF DIFFERENT DIA IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 12 | P/L 1:2:4 RCC Ring Slab including 21” Dia manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) | 228 Nos. | Offer Rate | Offer Rate |
|  | Providing & Fixing RCC Slab CC 1:2:4 | 75 CFT | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/37**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PAINTING CURB STONE ON FOOTPATH ON DIFFERENT ROADS AND OTHER WORK IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.2,15,600 /= + O/R*

*BID SECURITY.* Rs. *4,312/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/37**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 2,15,600 /= + O/R*

Earnest Money *RS. 4,312/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PAINTING CURB STONE ON FOOTPATH ON DIFFERENT ROADS AND OTHER WORK IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 10.60 Cft | 3327.50 %  Cft | 353/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1)  21” Dia  24” Dia | 63 Nos.  150 Nos. | 913.63 Each  1051.25 Each | 57,559/=  157,688/= |
| **SUB TOTAL PART-A** | | | | **215,600/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/38**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **FILLING OF POT HOLES UNEVEN SURFACE AND OTHERRELATEDWORK IN DIFFERENT MAIN ROAD IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.3,25,200 /= + O/R*

*BID SECURITY.* Rs. *6,504/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/38**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.3,25,200 /= + O/R*

Earnest Money *RS.6,504/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **FILLING OF POT HOLES UNEVEN SURFACE AND OTHERRELATEDWORK IN DIFFERENT MAIN ROAD IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 370.22 Cft | 773.86%  Cft | 2,865/= |
| 03 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 11550 Cft | 1437.00%0  Cft | 16,597/= |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11550 Cft | 1065.00%  Cft | 123,012/= |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 200 Nos. | 913.63 | 182,726/= |
| **SUB TOTAL PART-A** | | | | **325,200/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **FILLING OF POT HOLES UN EVEN SURFACE AND OTHERRELATEDWORK IN DIFFERENT MAIN ROAD IN ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 3600 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 7920 Cft | Offer Rate | Offer Rate |
| 03 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 33 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/40**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR / IMPROVEMENT OF RCC PIPE AND MAIN HOLE NEAR SIDDIQUI AKBER MASJID IN UC-1. BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,84,547 /= + O/R*

*BID SECURITY.* Rs. *19,691 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/40**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.9,84,547 /= + O/R*

Earnest Money *RS.19,691 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

Subject: **REPAIR / IMPROVEMENT OF RCC PIPE AND MAIN HOLE NEAR SIDDIQUI AKBER MASJID IN UC-1.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1608 Cft | 3327.50 %  Cft | 53,506/= |
| 02 | Dismantling and removing of stone metaling and carpeting etc (13/51) | 1750 Cft | 605.00 % CFT | 10,588/= |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammering and chieslling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge | 4594 Cft | 24150.00%0  Cft | 1,10,945/= |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2188 Cft | 4650.00 %0 CFT | 10,174/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 15” DIA | 700 Rft | 436.00 RFT | 3,05,200/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 35 Nos. | 13064 /= Each | 4,57,240/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -59.093 Rft | 1540.00 RFT | -91,003/= |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 951 Cft | 2760.00 %0 CFT | 2625/= |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 9189 Cft | 1065.00% CFT | 97,863/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 30 Nos. | 913.63 Each | 27,409/= |
| **SUB TOTAL PART-A** | | | | **9,84,547/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR / IMPROVEMENT OF RCC PIPE AND MAIN HOLE NEAR SIDDIQUI AKBER MASJID IN UC-1.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 380  Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/41**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIRING OF FOOTPATH AND PAINTING AND OTHER WORKS IN IMAM BARGAH HYDER E QARAR IN ORANGE ZONE.**

*ESTIMATED COST. RS.Offer Rate*

*BID SECURITY.* Rs. *2% Offer Rate*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/41**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *O/R*

Earnest Money *2% + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIRING OF FOOTPATH AND PAINTING AND OTHER WORKS IN IMAM BARGAH HYDER E QARAR IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 3840 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2304 Cft | Offer Rate | Offer Rate |
| 03 | P/F kerb stone etc complete | 800 Nos. | Offer Rate | Offer Rate |
| 04 | Painting plaster surface i/c cleaning scraping i/c complete etc | 24000 Sqft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/42**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE NEAR MOMIN MASJID IN MUSLIMABAD, UC-2**

*ESTIMATED COST. RS.9,64,632/= + O/R*

*BID SECURITY.* Rs. 19,293/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/42**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,64,632/= + O/R*

Earnest Money RS.19,293/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE NEAR MOMIN MASJID IN MUSLIMABAD, UC-2**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 3850 Cft | 24150.00 %0 CFT | 92978/= |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 600 Rft  200 Rft | 206.00 Rft  367.00 Rft | 1,23,600/=  73400/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 35 Nos | 13064 /= Each | 4,57,240/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -79 | 1540.00 RFT | -121660/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 7600 | 526.28%  Sft | 39,997/= |
| 07 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 7600 | 3275.50%  Sft | 2,48,938/= |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 10 Nos | 913.63 | 9,136 |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3850 | 1065.00% CFT | 41003/= |
| **SUB TOTAL PART-A** | | | | **9,64,632/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE NEAR MOMIN MASJID IN MUSLIMABAD, UC-2**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 1900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/43**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM BY PROVIDING RCC PIPE AND CONSTRUCTION OF MAIN HOLES IN UC-13 ORANGI ZONE**

*ESTIMATED COST. RS.* 6,75,500/= (+) O/R

*BID SECURITY.* Rs. 13,510/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/43**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,75,500/= (+) O/R

Earnest Money Rs. 13,510/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

Subject: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM BY PROVIDING RCC PIPE AND CONSTRUCTION OF MAIN HOLES IN UC-13 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:3:6 plain. (Ch-2/10/19-b) | 4840 Cft | 1306.80 % CFT | 63,249/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1208 Cft | 4650.00%  Sft | 5,617/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 230  Rft | 206.00  Rft | 47380/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 20 Nos. | 13064  Each | 261280/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 30.75  Rft | 1540.00  Rft | -47355/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 1027  Cft | 2760.00%0  Cft | 2835/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 10592  Cft | 1065.04%  Cft | 112805/- |
| 08 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 5200  Sft | 526.28%  Sft | 27367/- |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 5200  Sft | 3275.50%  Sft | 170326/- |
| 10 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 35 Nos. | 913.63  Each | 31977/- |
| **SUB TOTAL PART-A** | | | | **6,75,500/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM BY PROVIDING RCC PIPE AND CONSTRUCTION OF MAIN HOLES IN UC-13 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3600 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 1300 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 40 Nos. | Offer Rate | Offer Rate |
| 04 | Using SR Cement in Place of OPC | 150 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/44**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **RE-CONSTRUCTION OF ROAD, FILLING OF POT HOLES & TRENCHES NEAR NOORANI AL FATEH GRAVEYARD AND OTHER PLACES IN ORANGE ZONE.**

*ESTIMATED COST. RS.3,40,000*/= (+) O/R

*BID SECURITY.* Rs. *6,800*/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/44**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *3,40,000*/= (+) O/R

Earnest Money Rs. *6,800*/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **RE-CONSTRUCTION OF ROAD, FILLING OF POT HOLES & TRENCHES NEAR NOORANI AL FATEH GRAVEYARD AND OTHER PLACES IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 9000 Sft | 773.86%  Sft | 69,647/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 15960 Cft | 1437.00%0  Cft | 22935/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 20460 Cft | 1065.00%  Cft | 217899/- |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 5609 Sft | 526.28%  Sft | 29519/- |
| **SUB TOTAL PART-A** | | | | **3,40,000/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **RE-CONSTRUCTION OF ROAD, FILLING OF POT HOLES & TRENCHES NEAR NOORANI AL FATEH GRAVEYARD AND OTHER PLACES IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 4500 Cft | Offer Rate | Offer Rate |
| 03 | Providing & Fixing pre cost RCC Ring Slab 39” Dia with RCC Main hole Cover 21” Dia as per direction of engineer incharge. | 75 Nos | Offer Rate | Offer Rate |
| 04 | Painting on footpath, karb stone side situ, p/Wall etc by using oil paint approvwed make and shaid. Two coat i/c one primary coat and removal of dust etc as pe direction of Engineer incharge etc complete. | 4000 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/45**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **SUPPLY & FIXING OF MAIN HOLES COVER AND OTHER MAINTENANCE WORK IN SECTOR 11 ½ ORANGE ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,50,600 /= + O/R*

*BID SECURITY.* Rs. *17,012 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/45**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,50,600 /= + O/R*

Earnest Money *RS. 17,012/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **SUPPLY & FIXING OF MAIN HOLES COVER AND OTHER MAINTENANCE WORK IN SECTOR 11 ½ ORANGE ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 717 Cft | 3327.50 %  Cft | 23858/- |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1375 Cft | 4650.00 %0 CFT | 6393/- |
| 03 | Earth work excavation in irrigation channels irrigation draiaetc dressed to designed section and profile excavated material disposed off and dressed with in 50 ft lead. (Ordinary Soil) (ch-1-1/5) | 3000  Cft | 2420.00 %0 CFT | 7260/- |
| 04 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 250 Rft | 367.00  RFT | 91750/- |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 12 Nos | 13064 /= Each | 156768/- |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -21 Rft | 1540.00 RFT | (-)32340 |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1,111 Cft | 2760.00 %0 CFT | 3066/- |
| 08 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 4288 Cft | 1065.00% CFT | 45667/- |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 600 Nos. | 913.63  Each | 548178/- |
| **SUB TOTAL PART-A** | | | | **8,50,600/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **SUPPLY & FIXING OF MAIN HOLES COVER AND OTHER MAINTENANCE WORK IN SECTOR 11 ½ ORANGE ZONE**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3,800 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/46**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIRING OF EXISTING PIPE DRAIN I/C SUPPLY & FIXING OF RING SLAB IN MAKHDOOM SHAH COLONY ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 2,70,000/= (+) O/R

*BID SECURITY.* Rs. 5,400 /= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/46**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs.2,70,000/= (+) O/R

Earnest Money Rs.5,400 /= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **REPAIRING OF EXISTING PIPE DRAIN I/C SUPPLY & FIXING OF RING SLAB IN MAKHDOOM SHAH COLONY ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-C) | 459 Cft | 3327.50 % CFT | 15273/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1100 Cft | 4650.00%  Sft | 5115/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 12” Dia, | 200 Rft | 367.00 Rft | 73400/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 12 Nos. | 13064  Each | 156768 |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 21.0  Rft | 1540.00  Rft | -32340/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 889 ft | 2760.00%0 Cft | 2454/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 1801  Cft | 1065.00%  Cft | 19180/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 33 Nos. | 913.63  Each | 30150/- |
| **SUB TOTAL PART-A** | | | | **2,70,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIRING OF EXISTING PIPE DRAIN I/C SUPPLY & FIXING OF RING SLAB IN MAKHDOOM SHAH COLONY ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2000 Cft | Offer Rate | Offer Rate |
| 02 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 180 Nos. | Offer Rate | Offer Rate |
| 03 | Painting on footpath, karb stone side situ, p/Wall etc by using oil paint approvwed make and shaid. Two coat i/c one primary coat and removal of dust etc as pe direction of Engineer incharge etc complete. | 4800 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/47**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **IMP OF ROAD IN UC-04 AND OTHER LOCATION IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 6,30,000/= (+) O/R

*BID SECURITY.* Rs. 12,600/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/47**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs.6,30,000/= (+) O/R

Earnest Money Rs. 12,600/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **IMP OF ROAD IN UC-04 AND OTHER LOCATION IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-C) | 1868 Cft | 3327.50 % CFT | 62158/- |
| 02 | Earth work excavation of road side nalis forming it banks or putting the same on combankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 5713 Cft | 1437.00%0  Cft | 8210/- |
| 03 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 7692  Cft | 1065.00%  Cft | 81920/- |
| 04 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 8500  Sft | 526.28%  Sft | 44734/- |
| 05 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8500 Sft | 5093.86%  Sft | 432978/- |
| **SUB TOTAL PART-A** | | | | **6,30,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **IMP OF ROAD IN UC-04 AND OTHER LOCATION IN ORANGI ZONE .**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth within the radius of 5 miles i/c digging, loading, unloading, all lead and lift leveling and watering and compacting etc complete . | 3500 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 4250 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 18 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/48**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **MAINTENANCE OF BROKEN MAIN HOLES AND PIPE NEAR SHAH ALI CLINIC WALI GALI SENTOR 4/F IN UC-1.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,96,246 /= + O/R*

*BID SECURITY.* Rs. *13,925 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/48**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.6,96,246 /= + O/R*

Earnest Money *RS. 13,925 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

Subject: **MAINTENANCE OF BROKEN MAIN HOLES AND PIPE NEAR SHAH ALI CLINIC WALI GALI SENTOR 4/F IN UC-1.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 459 Cft | 3327.50 %  Cft | 15,2,73/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 4,400 Cft | 4650.00 %0 CFT | 20,460/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  15” DIA | 800 Cft | 367.00 RFT | 2,93,600/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 35 Nos. | 13064 /= Each | 4,57,240 |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -70 Rft | 1540.00 RFT | -10,7800 |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 3554 Cft | 2760.00 %0 CFT | 98,09/= |
| 11 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 720 Cft | 1065.00% CFT | 7,664/= |
| **SUB TOTAL PART-A** | | | | **6,96,246/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **MAINTENANCE OF BROKEN MAIN HOLES AND PIPE NEAR SHAH ALI CLINIC WALI GALI SENTOR 4/F IN UC-1.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S.No. | Description | Quantity | Days | Market Rate | Unit | Amount (Rs) |
| 1 | Hiring of Excavator for desalting and Cleaning of Nallaha Long Boom i/c POL  08 hours per day | 01 | 03 | O/Rate | Per day | O/Rate |
| 2 | Hiring Seal Dumpers for Lifting of Garbage & silt of Nallah i/c loading & unloading in all respect with pool  08 hours per day | 04 | 03 | O/Rate | Per day | O/Rate |
| 3 | Hiring of Loader for lifting of Garbage & silt with POL  08 hours per day | 01 | 03 | O/Rate | Per day | O/Rate |
| 4 | Hiring of Tractor Blade heavy Duty for Cleaning of streets & Roads etc with POL.  08 hours per day | 01 | 03 | O/Rate | Per day | O/Rate |
| 5 | Hiring of Skilled Afghani Labour for Cleaning of Nalah in different points all respect.  08 hours per day | 04 | 03 | O/Rate | Per day | O/Rate |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/49**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF SEWERAGE SYSTEM BY RCC PIPE AND CC STREET GALI NO. 8 AND QUODDUSI MASJID IN KHYBER COLONY UC-01.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,44,911 /= + O/R*

*BID SECURITY.* Rs. *16,898 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/49**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.8,44,911 /= + O/R*

Earnest Money *RS.16,898 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION OF SEWERAGE SYSTEM BY RCC PIPE AND CC STREET GALI NO. 8 AND QUODDUSI MASJID IN KHYBER COLONY UC-1.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1917 Cft | 3327.50 %  Cft | 63,788/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2200 Cft | 4650.00 %0 CFT | 10,230/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 400 Rft | 367.00 RFT | 1,46,800/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 16 Nos. | 13064 /= Each | 2,09,024/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -28Rft | 1540.00 RFT | -43,120/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1777 Cft | 2760.00 %0 CFT | 4,905/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 1864Cft | 1065.00% CFT | 19,852/= |
| 08 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 10,800  Sft | 526.28%  Sft | 56,838/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10,800  Sft | 3275.50%  Sft | 3,53,754/= |
| 10 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 25 Nos. | 913.63 Each | 22,840/= |
| **SUB TOTAL PART-A** | | | | **8,44,911/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION OF SEWERAGE SYSTEM BY RCC PIPE AND CC STREET GALI NO. 8 AND QUODDUSI MASJID IN KHYBER COLONY UC-1.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3000 Cft | Offer Rate | Offer Rate |
| 03 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 05 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/50**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONST / REPAIR OF CC STREET AND OTHER WORKS ON DIFFERENT LOCATION IN UC-05**

**BILL OF QUANTITIES**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 5,80,000/= (+) O/R

*BID SECURITY.* Rs. 11,600/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/50**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs.5,80,000/= (+) O/R

Earnest Money Rs. 11,600/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **CONST / REPAIR OF CC STREET AND OTHER WORKS ON DIFFERENT LOCATION IN UC-05**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-C) | 2604 Cft | 3327.50 % CFT | 86,648/- |
| 02 | Preparing of subgrade i/c earth excavation leveling to an average depth of nine inch dressing to camber e.t.c | 6500 Sft | 526.28 % Sft | 34208/- |
| 03 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 6500  Sft | 3275.50%  Sft | 212908/- |
| 04 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 08 Nos. | 913.63  Each | 7309/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 17.5  Rft | 1540.00  Rft | -26950/- |
| 06 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 4615  Cft | 1065.00%  Cft | 49150/- |
| 07 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 200 Rft | 367.00 Rft | 73400/- |
| 08 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 10 Nos. | 13064  Each | 130640/- |
| 09 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1100 Cft | 4650.00%  Sft | 5115/- |
| 10 | P/F Cost Iron frame for main hole i/c the cost of material. (ch-p/health-J1) | 5.44 kg | 140/- per Kg | 762/- |
| 11 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 889 ft | 2760.00%0 Cft | 2454/- |
| 12 | Earth work excavation in irrigation channels irrigation draiaetc dressed to designed section and profile excavated material disposed off and dressed with in 50 ft lead. (Ordinary Soil) (ch-1-1/5) | 1800  Cft | 2420.00 %0 CFT | 4356/= |
| **SUB TOTAL PART-A** | | | | **5,80,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONST / REPAIR OF CC STREET AND OTHER WORKS ON DIFFERENT LOCATION IN UC-05**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth within the radius of 5 miles i/c digging, loading, unloading, all lead and lift leveling and watering and compacting etc complete . | 3000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1000 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 1900 Cft | Offer Rate | Offer Rate |
| 04 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 75 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/51**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPLECEMENT OF DAMAGE RCC PIPE AND MAIN HOLES IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,88,000*/= (+) O/R

*BID SECURITY.* Rs. 11,760/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/51**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *5,88,000*/= (+) O/R

Earnest Money Rs. 11,760/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

SUBJECT: **REPLECEMENT OF DAMAGE RCC PIPE AND MAIN HOLES IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1749 Cft | 3327.50 %  Cft | 58198/- |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2750 Cft | 4650.00 %0 CFT | 12788/- |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 500 Cft | 367.00 RFT | 183500/- |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 25 No. | 13064 /= Each | 326600/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -43.75 Rft | 1540.00 RFT | -37375/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2,222 Cft | 2760.00 %0 CFT | 6133/- |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 2625 Cft | 1065.00% CFT | 27956/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 130 Nos. | 913.63 | 40200/- |
| **SUB TOTAL PART-A** | | | | **5,88,000/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPLECEMENT OF DAMAGE RCC PIPE AND MAIN HOLES IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 130 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/52**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIRING OF CC WORKS / RCC PIPE DRAIN IN UC-02 AND OTHER PLACES IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,85,000/= (+) O/R

*BID SECURITY.* Rs. 15,700/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/52**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,85,000/= (+) O/R

Earnest Money Rs. 15,700/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **REPAIRING OF CC WORKS / RCC PIPE DRAIN IN UC-02 AND OTHER PLACES IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) | 2300 Cft | 3327.50 % CFT | 76533/- |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2200 Cft | 10770.00 %0 CFT | 23694/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 400 Rft | 367.00 Rft | 146800/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 18 Nos. | 13064  Each | 235152/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 33.968  Rft | 1540.00  Rft | -52311/- |
| 06 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2300  Cft | 1065.04%  Cft | 24495/- |
| 07 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 29 Nos. | 913.63  Each | 26495/- |
| 08 | Preparing of subgrade i/c earth excavation leveling to an average depth of nine inch dressing to camber e.t.c | 8000 Sft | 526.28 % Sft | 42102/- |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 8000  Sft | 3275.50%  Sft | 262040/- |
| **SUB TOTAL PART-A** | | | | **7,85,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIRING OF CC WORKS / RCC PIPE DRAIN IN UC-02 AND OTHER PLACES IN ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 1200 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 2640 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/53**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **FILLING OF DAMAGE ROAD PORTION & CARPETING POT HOLE ALI NAGAR BHOLO MASJID IN UC-09**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,61,202/= + O/R

*BID SECURITY.* Rs. 15,224 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/53**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,61,202/= + O/R

Earnest Money Rs. 15,224 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **FILLING OF DAMAGE ROAD PORTION & CARPETING POT HOLE ALI NAGAR BHOLO MASJID IN UC-09**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6500 Sft | 773.86%  Sft | 50301/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 27663 Cft | 1065.00%  Cft | 294611/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 8000Sft | 4765.11%Sft | 381209/- |
| **SUB TOTAL PART-A** | | | | **7,51,672/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **FILLING OF DAMAGE ROAD PORTION & CARPETING POT HOLE ALI NAGAR BHOLO MASJID IN UC-09**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 800 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/54**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMPROVEMENT OF CC STREET AND OTHER WORKS NEAR SABRI CHOWK AND ON DIFFERENT LOCATION IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,76,000/= (+) O/R

*BID SECURITY.* Rs. 15,520/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/54**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,76,000/= (+) O/R

Earnest Money Rs. 15,520/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

Subject: **IMPROVEMENT OF CC STREET AND OTHER WORKS NEAR SABRI CHOWK AND ON DIFFERENT LOCATION IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) RCC1:2:4 | 3465 Cft  375 Cft | 3327.50 % CFT  5445 % Cft | 1,15,298/-  20419/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 660 Cft | 4650.00%  Sft | 3069/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 8” Dia, 12” Dia, 15” Dia | 120  Rft | 367.00  Rft | 44040/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 06 Nos. | 13064  Each | 78384/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 10.5  Rft | 1540.00  Rft | -16170/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 533  Cft | 2760.00%0  Cft | 1471/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 9240  Cft | 1065.04%  Cft | 98406/- |
| 08 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 10500  Sft | 526.28%  Sft | 55259/- |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10500  Sft | 3275.50%  Sft | 343928/- |
| 10 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia 24” Dia | 20 Nos. | 913.63  Each | 18273/- |
| 11 | Earth Excavation in irrigation channels, and disposal of cerplus staff e.t.c. | 5400 Cft | 2420.00 % 0 Cft | 13068/- |
| 12 | Providing and Fixing Cast iron frame for main hole i/c the cost of material | 3.966 KG | 140 per KG | 555/- |
| **SUB TOTAL PART-A** | | | | **7,76,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMPROVEMENT OF CC STREET AND OTHER WORKS NEAR SABRI CHOWK AND ON DIFFERENT LOCATION IN ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3045 Cft | Offer Rate | Offer Rate |
| 02 | Painting of Footpath Curb Stone and Side SITU with oil pant approve make and shade and remove old surface | 2600 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/55**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE MUSLIM NAGAR GALI NO. 14 IN UC-6**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,57,646/= + O/R*

*BID SECURITY.* Rs. *11,153 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/55**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 5,57,646/= + O/R*

Earnest Money *RS. 11,153 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE MUSLIM NAGAR GALI NO. 14 IN UC-6**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1188 Cft | 4650.00 %0 CFT | 5524/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2)  9” DIA | 250 Rft | 206 RFT | 51500/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 20 Nos | 13064 /= Each | 2,61,280/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -37.5 | 1540.00 RFT | -57750/= |
| 09 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 889 Cft | 2760.00 %0 CFT | 2454/= |
|  | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 7750 Cft | 526.28%  Sft | 40787/= |
|  | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 7750 Cft | 3275.50%  Sft | 2,53,851/= |
| **SUB TOTAL PART-A** | | | | **5,57,646/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPE MUSLIM NAGAR GALI NO. 14 IN UC-6**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 3306 Sft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4148 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/56**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF RCC PIPE AND CC STREET IN JUMMAN DRAWN MOHALLAH IN UC-13 ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,94,337 /= + O/R*

*BID SECURITY.* Rs. *15,887 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/56**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 7,94,337 /= + O/R*

Earnest Money *RS. 15,887 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION OF RCC PIPE AND CC STREET IN JUMMAN DRAWN MOHALLAH IN UC-13 ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2991 Cft | 3327.50 %  Cft | 99526/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1725 Cft | 4650.00 %0 CFT | 8021/= |
| 03 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 300 Rft | 367.00  RFT | 110100/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 15 Nos | 13064 /= Each | 195960/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -22.5 Rft | 1540.00 RFT | -34650/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1408 Cft | 2760.00 %0 CFT | 3886/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 4752 Cft | 1065.00% CFT | 50609/= |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9500 Sft | 526.28%  Sft | 49997/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9500 Sft | 3275.50%  Sft | 310888/= |
| **SUB TOTAL PART-A** | | | | **7,94,337/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION OF RCC PIPE AND CC STREET IN JUMMAN DRAWN MOHALLAH IN UC-13 ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

**I / we hereby quoted rates as follows:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 22 Nos | Offer Rate | Offer Rate |
| 02 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1688 Cft | Offer Rate Each | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2755 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/57**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF RCC PIPE NEAR FARHAN GENERAL STORE IN MOMINABAD**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,98,630*/=

*BID SECURITY.* Rs. *19,973*/=

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/57**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *9,98,630*/=

Earnest Money Rs. *19,973*/=

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **REHABILITATION OF RCC PIPE NEAR FARHAN GENERAL STORE IN MOMINABAD**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1608 Cft | 3327.50 %  Cft | 53,506/= |
| 02 | Dismantling and removing of stone metaling and carpeting etc (13/51) | 1750 Cft | 605.00 % CFT | 10,588/= |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2188 Cft | 4650.00 %0 CFT | 10,174/= |
| 04 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 4594 Cft | 24150.00 %0 CFT | 1,10,945/= |
| 05 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 15” DIA | 700 Cft | 436.00 RFT | 3,05,200/= |
| 06 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 35 No. | 13064 /= Each | 4,57,240/= |
| 07 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -59.44 Rft | 1540.00 RFT | -91,538/= |
| 08 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 951 Cft | 2760.00 %0 CFT | 2625/= |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 9189 Cft | 1065.00% CFT | 97,863/= |
| 10 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 46 Nos. | 913.63 | 42,027/= |
| **SUB TOTAL PART-A** | | | | **9,98,630/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF RCC PIPE NEAR FARHAN GENERAL STORE IN MOMINABAD**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/58**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR OF CC AND SEWERAGE SYSTEM 9” DIA IN RAHIM SHAH COLONY AND TOUHEED COLONY IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,81,834 /= + O/R*

*BID SECURITY.* Rs. *17,637 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/58**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,81,834 /= + O/R*

Earnest Money *RS. 17,637 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR OF CC AND SEWERAGE SYSTEM 9” DIA IN RAHIM SHAH COLONY AND TOUHEED COLONY IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2595 Cft | 10770.00 %0 CFT | 27948/- |
| 02 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1500 Cft | 3327.50 %  Cft | 49913/- |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  8” DIA | 300 Rft  800 Rft | 367.00RFT  206.00 RFT | 1,10,100/=  37080/- |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 22 Nos | 13064 /= Each | 287408/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -35.0 Rft | 1540.00 RFT | -53900/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2137 Cft | 2760.00 %0 CFT | 5898/- |
| 07 | P/L 1:3:6 CC using GSB ¾” and down guage i/c consolidation, curing etc complete without shuttering. (16/5-h) | 60 Cft | 12595.00 % CFT | 7557/- |
| 08 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 7478 Cft | 1437.00%0  Cft | 10746/- |
| 09 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 14499 Cft | 1065.00% CFT | 154414/- |
| 10 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 3000 Sft | 526.28%  Sft | 15788/- |
| 11 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 6000 Sft | 3275.50%  Sft | 196530/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 22 Nos. | 913.63 | 20100/- |
| 13 | Earth work excavation in irrigation channels, irrigation drain etc dressed to designed section and profile excavated. | 5063 Cft | 2420.00%0  Cft | 12252/- |
| **SUB TOTAL PART-A** | | | | **294795/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR OF CC AND SEWERAGE SYSTEM 9” DIA IN RAHIM SHAH COLONY AND TOUHEED COLONY IN ORANGE ZONE.**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per Costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 04 Nos | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2719 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/59**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **PATCH REPAIR OF CARPET NEAR ZAIQA PAKWAN AND 4 STAR LAWN IN SHAH WALIULLAH NAGAR IN UC-7 ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,93,213*/= (+) O/R

*BID SECURITY.* Rs. *13,864*/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/59**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *6,93,213*/= (+) O/R

Earnest Money Rs. *13,864*/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **PATCH REPAIR OF CARPET NEAR ZAIQA PAKWAN AND 4 STAR LAWN IN SHAH WALIULLAH NAGAR IN UC-7 ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15253.42Cft | 1065.00%  Cft | 162,449/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 12 Nos. | 913.63 Each | 11,877/= |
| **SUB TOTAL PART-A** | | | | **693,213/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **PATCH REPAIR OF CARPET NEAR ZAIQA PAKWAN AND 4 STAR LAWN IN SHAH WALIULLAH NAGAR IN UC-7 ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3660 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/60**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIRING AND MAINTENANCE OF SEWERAGE SYSTEM AND CC STREET IN KACHI MOHALLAH AND OTHER PLACE IN UC-13.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,55,131 /= + O/R*

*BID SECURITY.* Rs. *17,103 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/60**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,55,131 /= + O/R*

Earnest Money *RS. 17,103 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIRING AND MAINTENANCE OF SEWERAGE SYSTEM AND CC STREET IN KACHI MOHALLAH AND OTHER PLACE IN UC-13.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 3221 Cft | 3327.50 %  Cft | 107179/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1650 Cft | 4650.00 %0 CFT | 7673/= |
| 03 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 350 Rft | 367.00  RFT | 128450/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 20 Nos | 13064 /= Each | 261280/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -30 Rft | 1540.00 RFT | -46200/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1280 Cft | 2760.00 %0 CFT | 3533/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 4794 Cft | 1065.00% CFT | 51056 |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9000 Sft | 526.28%  Sft | 47365/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9000 Sft | 3275.50%  Sft | 294795/= |
| **SUB TOTAL PART-A** | | | | **294795/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIRING AND MAINTENANCE OF SEWERAGE SYSTEM AND CC STREET IN KACHI MOHALLAH AND OTHER PLACE IN UC-13.**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per Costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 02 Nos | Offer Rate | Offer Rate |
| 02 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1688 Cft | Offer Rate Each | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2250 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/61**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR AND RE-FIXING OF MAIN HOLE COVER AND PRE COST RING SLAB IN THE JURISDICTION OF ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.4,56,815 /= + O/R*

*BID SECURITY.* Rs.*9,136 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/61**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 4,56,815 /= + O/R*

Earnest Money *RS. 9,136 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR AND RE-FIXING OF MAIN HOLE COVER AND PRE COST RING SLAB IN THE JURISDICTION OF ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 500 Nos | 913.63 | 456815 |
| **SUB TOTAL PART-A** | | | | **456815/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR AND RE-FIXING OF MAIN HOLE COVER AND PRE COST RING SLAB IN THE JURISDICTION OF ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per Costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 180 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/62**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND FIXING OF WOODEN PENAL SHEET I/C POLISHING IN AND OTHER WORKS COMINITY HALL IN ORNAGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.Offer Rate*

*BID SECURITY.* Rs.*2% Offer Rate*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/62**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Subject: **PROVIDING AND FIXING OF WOODEN PENAL SHEET I/C POLISHING IN AND OTHER WORKS COMINITY HALL IN ORNAGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F 3/4 “ thick clip board or partex board in pennels i/c 2mm finishing ply wod i/c suppling and fixing and polishing etc. | 1530/- | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/63**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF ROAD BY TRACTOR FOR MOTORABLE OF ROAD IN BIJLI NAGAR IJTIMAHGAH AND OTHER ROAD IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,74,685 /= + O/R*

*BID SECURITY.* Rs.*13,494 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/63**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,74,685 /= + O/R*

Earnest Money *RS. 13,494 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION OF ROAD BY TRACTOR FOR MOTORABLE OF ROAD IN BIJLI NAGAR IJTIMAHGAH AND OTHER ROAD IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 02 | Earth work excavation of road side nalis forming it banks or putting the same on commandment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 21613 Cft | 1437.00%0  Cft | 31,058/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 21613 Cft | 1065.00%  Cft | 2,30,178/= |
| 04 | P/L Aggregate base course material in proper grade and camber having CBR 80% as per AASHO standard specification i/c Vibratory roller, & smooth wheel roller etc) watering to maintain the moisture content the compaction of each layer shall 100% to the max dry density. (Rate i/c all cost of materials T&P and carriage upto 3 chains. | 4163 Cft | 5542.25 % Cft | 2,30,723/= |
| 12 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 200 Nos | 913.63 | 1,8,2726/= |
| **SUB TOTAL PART-A** | | | | **6,74,685/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION OF ROAD BY TRACTOR FOR MOTORABLE OF ROAD IN BIJLI NAGAR IJTIMAHGAH AND OTHER ROAD IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
|  | Providing & Fixing Precost RCC Ring Slab 39” Dia with RCC Main Hole Cover of 21” Dia as per direction | 40 Nos. | Offer Rate | Offer Rate |
|  | Hiring of Tractor Blade Heavy Duty for cleaning of Street or Road etc. with POL (8 Hours) | 10 Days | Offer Rate | Offer Rate |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 3132 | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/64**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **IMPROVEMENT / CONSTRUCTION OF CC STREET NEAR IQRA SCHOOL GULSHAN-E-ZIA ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,31,441/= + O/R*

*BID SECURITY.* Rs.*10,629 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/64**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 5,31,441/= + O/R*

Earnest Money *RS. 10,629 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **IMPROVEMENT / CONSTRUCTION OF CC STREET NEAR IQRA SCHOOL GULSHAN-E-ZIA ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 520 Cft | 1306.80%  Cft | 6,795/= |
| 02 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 13800 Cft | 526.28%  Sft | 72,627/= |
| 03 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 13800Cft | 3275.50%  Sft | 4,52,019/= |
| **SUB TOTAL PART-A** | | | | **5,31,441/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **IMPROVEMENT / CONSTRUCTION OF CC STREET NEAR IQRA SCHOOL GULSHAN-E-ZIA ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 2663 Sft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4002 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/65**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPE & CC STREET IN GALI NO. 3 NEAR JAMIA MEHMODIA MADARSA IN RAJA TAVEER COLONY, IN UC-7**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,74,713 /= + O/R*

*BID SECURITY.* Rs.*13,494 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/65**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,74,713 /= + O/R*

Earnest Money *RS. 13,494 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPE & CC STREET IN GALI NO. 3 NEAR JAMIA MEHMODIA MADARSA IN RAJA TAVEER COLONY, IN UC-7**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1279 Cft | 3327.50 %  Cft | 42,559/= |
| 01 | Dismantling of cementconcrete flooring. 1:3:6 plain (10/19-b) | 1872 Cft | 1306.80%  Cft | 24,464/= |
| 03 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1500 Cft | 4650.00 %0 CFT | 6,975/= |
| 04 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 300 Cft | 10770.00 %0 CFT | 3,231/= |
| 06 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 300 Rft | 367.00RFT | 1,10,100/= |
| 07 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 13 Nos | 13064 /= Each | 1,69,832/= |
| 08 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -21 Rft | 1540.00 RFT | -32340/= |
| 09 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1432 Cft | 2760.00 %0 CFT | 3952/= |
| 10 | P/L 1:3:6 CC using GSB ¾” and down guage i/c consolidation, curing etc complete without shuttering. (16/5-h) | 30 Cft | 12595.00 % CFT | 3779/= |
|  | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9000 Cft | 526.28%  Sft | 47366/= |
|  | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9000 Cft | 3275.50%  Sft | 2,94,795 |
| **SUB TOTAL PART-A** | | | | **6,74,713/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING RCC PIPE & CC STREET IN GALI NO. 3 NEAR JAMIA MEHMODIA MADARSA IN RAJA TAVEER COLONY, IN UC-7**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 6875 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 1230 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3375 Cft | Offer Rate | Offer Rate |
| 04 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 245 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/66**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR & MAINTENANCE OF CC STREET & PIPE DRAIN NEAR MASHA ALLAH LAWN IN UC-9**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,56,420 /= + O/R*

*BID SECURITY.* Rs.*13,128 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/66**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,56,420 /= + O/R*

Earnest Money *RS. 13,128 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR & MAINTENANCE OF CC STREET & PIPE DRAIN NEAR MASHA ALLAH LAWN IN UC-9**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1700 Cft | 4650.00 %0 CFT | 7,905/= |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 400 Cft | 206 RFT | 82,400/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 18 Nos | 13064 /= Each | 2,35,152/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -36 Rft | 1540.00 RFT | -55,440/= |
| 05 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1386 Cft | 2760.00 %0 CFT | 3,823/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 10050 Cft | 526.28%  Sft | 52,891/= |
| 07 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10050 Cft | 3275.50%  Sft | 3,29,188 |
| **SUB TOTAL PART-A** | | | | **6,56,420/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR & MAINTENANCE OF CC STREET & PIPE DRAIN NEAR MASHA ALLAH LAWN IN UC-9**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2513 Cft | Offer Rate | Offer Rate |
| 04 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 290 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/67**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPER GALI NO. 2, IN HAJI HUSSAIN MOHALLAH BISMILLAH COLONY, & DIFFERENT PLACE IN UC 2**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,16,034/= + O/R*

*BID SECURITY.* Rs.18,321/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/67**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,16,034/= + O/R*

Earnest Money RS. 18,321/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPER GALI NO. 2, IN HAJI HUSSAIN MOHALLAH BISMILLAH COLONY, & DIFFERENT PLACE IN UC 2**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 3080 Cft | 24150.00 %0 CFT | 74382/= |
| 02 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1980 | 3327.50 %  Cft | 65885/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 560 Rft | 367.00 Rft | 205520/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 26 Nos | 13064 /= Each | 3,39,664/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -58 | 1540.00 RFT | -89320/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2394 | 2760.00 %0 CFT | 6607/= |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 8000 | 526.28%  Sft | 42120/= |
| 08 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 8000 | 3275.50%  Sft | 262040/= |
| 09 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 10 Nos | 913.63 | 9,136 |
| **SUB TOTAL PART-A** | | | | **9,16,034/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONSTRUCTION OF CC STREET & RCC PIPER GALI NO. 2, IN HAJI HUSSAIN MOHALLAH BISMILLAH COLONY, & DIFFERENT PLACE IN UC 2**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2640 Cft | Offer Rate | Offer Rate |
| 02 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 231 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/68**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM & NALA INCLUDING RCC SLAB AT IMAM COLONY BABA WALIYAT ALI SHAH COLONY AND OTHER COLONY IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,53,751/= + O/R*

*BID SECURITY.* Rs.*11,075 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/68**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 5,53,751/= + O/R*

Earnest Money *RS. 11,075 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM & NALA INCLUDING RCC SLAB AT IMAM COLONY BABA WALIYAT ALI SHAH COLONY AND OTHER COLONY IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of RCC concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1594 Cft | 5445.0% Cft | 86793/= |
| 02 | Dismantling of CC flooring. 1:2:4 plain (Ch-2/10/19c) | 2100 Cft | 3327.50 %  Cft | 69,878/= |
| 03 | Dismantling of cementconcrete flooring. 1:3:6 plain (10/19-b) | 1155 Cft | 1306.80%  Cft | 15,094/= |
| 04 | Earth work excavation in irrigation channels, irrigation drain etc dressed to designed section and profile excavated. | 18985 Cft | 2420.00%0  Cft | 45944/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 23834 | 1065.00% CFT | 2,53,832/= |
| 06 | Fabrication of steel reinforcement for cement concrete i/c cutting, bending, binding & laying in postion, making joints & fastening i/c the cost of binding works and removal of rust from bars. | 3.5 Wct | 5001.70 per  Cwt | 17506/= |
| 07 | RCC work i/c all labor & material except the cost of reinforcement and its labor for bending binding which will be paid separately. This rate also i/c all kinds of forms, molds, lifting, shuttering, cutting, rendering & finishing the expose surface i/c screening & wishing of shingles. Ratio 1:2:4 | 192 Cft | 337.00 Cft | 64,704/= |
| **SUB TOTAL PART-A** | | | | **5,53,751/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR & MAINTENANCE OF SEWERAGE SYSTEM & NALA INCLUDING RCC SLAB AT IMAM COLONY BABA WALIYAT ALI SHAH COLONY AND OTHER COLONY IN ORANGI ZONE**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 05 | P/F RCC pre cast slab 2” thick of required size and shape and racking out joints with CM curing etc complete as per direction of engineer incharge | 252 Sft | Offer Rate | Offer Rate |
| 06 | P/F RCC pre cast slab or i/c linter (I-beam) of required size and shape and and racking out joints with CM curing etc complete as per direction of engineer incharge | 984 Sft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/69**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR AND MAINTENANCE OF CC STREET SALAM BHAI WALI GALI IN UC-2.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,99,809 /= + O/R*

*BID SECURITY.* Rs.*13,996 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/69**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,99,809 /= + O/R*

Earnest Money *RS. 13,996 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR AND MAINTENANCE OF CC STREET SALAM BHAI WALI GALI IN UC-2.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2607  Cft | 3327.50 %  Cft | 86,735/= |
| 02 |  |  |  |  |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 2607 Cft | 1065.00% CFT | 27,765/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 10400 Sft | 526.28%  Sft | 54,733/= |
| 05 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 10400 Sft | 3275.50%  Sft | 3,40,652/= |
| 06 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 120 Cft | 4650.00 %0 CFT | 5580/= |
| 07 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 200 Rft | 367.00  RFT | 73400/= |
| 08 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 09 Nos | 13064 /= Each | 1,17,576/= |
| 09 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -18 Rft | 1540.00 RFT | -27,720/= |
| 10 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1020 Cft | 2760.00 %0 CFT | 2815/= |
| 11 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 20 Nos | 913.63 | 18,273/= |
| **SUB TOTAL PART-A** | | | | **6,99,809/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR AND MAINTENANCE OF CC STREET SALAM BHAI WALI GALI IN UC-2.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3016 Cft | Offer Rate | Offer Rate |
| 02 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 300 Cwt | Offer Rate | Offer Rate |
| 03 | Providing& Fixing pre cost RCC Ring Slab 39” Dia with RCC Main hole Cover 21” Dia as per direction | 45 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/70**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMPROVEMENT OF ROAD BY CARPETING NEAR SABRI CHOWK AND URDU CHOWK & OTHER PLACES IN ORANGE ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,60,816/= + O/R

*BID SECURITY.* Rs.15,216 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/70**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,60,816/= + O/R

Earnest Money Rs. 15,216 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **IMPROVEMENT OF ROAD BY CARPETING NEAR SABRI CHOWK AND URDU CHOWK & OTHER PLACES IN ORANGE ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7200 Sft | 773.86%  Sft | 55718/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 28013Cft | 1065.00%  Cft | 298338/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **7,60,816/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMPROVEMENT OF ROAD BY CARPETING NEAR SABRI CHOWK AND URDU CHOWK & OTHER PLACES IN ORANGE ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 750 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3600 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/71**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR AND MAINTENANCE CC STREET AND PIPE 12” INCH DIA NEAR KHAN NIAZI HOUSE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,16,917 /= + O/R*

*BID SECURITY.* Rs.*16,338 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/71**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,16,917 /= + O/R*

Earnest Money *RS. 16,338 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR AND MAINTENANCE CC STREET AND PIPE 12” INCH DIA NEAR KHAN NIAZI HOUSE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3900  Cft | 10770.00 %0 CFT | 42003/= |
| 02 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 600  RFT | 367.00  RFT | 2,20,200/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 24 Nos | 13064 /= Each | 3,15,536/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -42  Rft | 1540.00 RFT | -64,680/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3900  Cft | 1065.00% CFT | 41,535/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 6900  Sft | 526.28%  Sft | 36,313/= |
| 07 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 6900  Sft | 3275.50%  Sft | 2,26,010/= |
| **SUB TOTAL PART-A** | | | | **8,16,917/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR AND MAINTENANCE CC STREET AND PIPE 12” INCH DIA NEAR KHAN NIAZI HOUSE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 2966 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2001 Cft | Offer Rate | Offer Rate |
| 02 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 199 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/72**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LYING RCC PIPE IN GALI NO.15 GULSHAN-E-ZIA SECTOR 11 ½ SHEET NO.01 NEAR MUSTAFA MASJID AND MUKHTAR HOUSE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.3,34,111 /= + O/R*

*BID SECURITY.* Rs.*6,682 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/72**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 3,34,111 /= + O/R*

Earnest Money *RS. 6,682 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LYING RCC PIPE IN GALI NO.15 GULSHAN-E-ZIA SECTOR 11 ½ SHEET NO.01 NEAR MUSTAFA MASJID AND MUKHTAR HOUSE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:3:6 plain. (Ch-2/10/19-b) | 123  Cft | 1306.80%  Cft | 1607/- |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2250  Sft | 4650.00 %0 CFT | 10463/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 09” DIA | 450  RFT | 206.00 RFT | 92700/- |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 22 Nos | 13064 /= Each | 287408/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -41  Rft | 1540.00 RFT | -63140/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1838  Cft | 2760.00 %0 CFT | 5073/- |
| **SUB TOTAL PART-A** | | | | **3,34,111/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LYING RCC PIPE IN GALI NO.15 GULSHAN-E-ZIA SECTOR 11 ½ SHEET NO.01 NEAR MUSTAFA MASJID AND MUKHTAR HOUSE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Providing& Fixing pre cost RCC Ring Slab 39” Dia with RCC Main hole Cover 21” Dia as per direction of engineer incharge. | 215 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/73**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF ROAD AND RCC PIPE NEAR ALTAF MEMORIAL PUBLIC SCHOOL IN UC-6**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,04,298/= + O/R*

*BID SECURITY.* Rs.18,086/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/73**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,04,298/= + O/R*

Earnest Money RS.18,086/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF ROAD AND RCC PIPE NEAR ALTAF MEMORIAL PUBLIC SCHOOL IN UC-6**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 2000 | 4650.00 %0 CFT | 9,300/= |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 100 Rft  300 Rft | 206.00 Rft  367.00 Rft | 20600/=  1,10,100/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 20 Nos | 13064 /= Each | 2,61,280/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -37.5 | 1540.00 RFT | -57750/= |
| 05 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1585 | 2760.00 %0 CFT | 4,375/= |
| 05 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9900 | 526.28%  Sft | 52,101/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 9900 Sft | 5093.86%  Sft | 5,04292/= |
| **SUB TOTAL PART-A** | | | | **9,04,298/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF ROAD AND RCC PIPE NEAR ALTAF MEMORIAL PUBLIC SCHOOL IN UC-6**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3713 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/74**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

**SUBJECT: REPAIRING OF DAMAGE ROAD / FILLING OF POT HOLES TRANCHES ON DIFFERENT LOCATION NEAR MUSTAFA COLONY BLOCK J ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,50,000/= (+) O/R

*BID SECURITY.* Rs.15,000/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/74**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,50,000/= (+) O/R

Earnest Money Rs. 15,000/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

**SUBJECT: REPAIRING OF DAMAGE ROAD / FILLING OF POT HOLES TRANCHES ON DIFFERENT LOCATION NEAR MUSTAFA COLONY BLOCK J ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-b) | 1542 Cft | 3327.50 % CFT | 51310/- |
| 02 | Earth Work Excavation of Road Sides Nails forming its Banks of putting the same on embakment as directed braking clods & Dressing e.t.c | 5490 Cft | 1437.00%0  Cft | 7889/- |
| 03 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 7035  Cft | 1065.04%  Cft | 74923/- |
| 04 | Preparing of subgrade i/c earth excavation leveling to an average depth of nine inch dressing to camber e.t.c | 8000 Sft | 526.28 % Sft | 42102/- |
| 05 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3000 Cft | 5542.24 % Cft | 166267/- |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| **SUB TOTAL PART-A** | | | | **7,50,000/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

**SUBJECT: REPAIRING OF DAMAGE ROAD / FILLING OF POT HOLES TRANCHES ON DIFFERENT LOCATION NEAR MUSTAFA COLONY BLOCK J ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 3000 Cft | Offer Rate | Offer Rate |
| 03 | P/F RCC 1:2:4 Slab pre cost lintle shap as per direction | 103 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/75**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LYING RCC PIPE AND CONSTRUCTION OF CC STREET GHAZIABAD UC-6 NEAR HOUSE NO. 1167 ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,50,781 /= + O/R*

*BID SECURITY.* Rs.*15,016 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/75**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 7,50,781 /= + O/R*

Earnest Money *RS. 15,016 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LYING RCC PIPE AND CONSTRUCTION OF CC STREET GHAZIABAD UC-6 NEAR HOUSE NO. 1167 ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cementconcrete flooring. 1:3:6 plain (10/19-b) | 289 Cft | 1306.80%  Cft | 3777/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1230 Cft | 4650.00 %0 CFT | 5720/= |
| 03 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 550 Rft | 206.00  RFT | 113300/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 25 Nos | 13064 /= Each | 3,26,600/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -50 Rft | 1540.00 RFT | -77000/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 727 Cft | 2760.00 %0 CFT | 2007/= |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9900 Sft | 526.28%  Sft | 52102/= |
| 08 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9900 Sft | 3275.50%  Sft | 3,24,275/= |
| **SUB TOTAL PART-A** | | | | **7,50,781/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LYING RCC PIPE AND CONSTRUCTION OF CC STREET GHAZIABAD UC-6 NEAR HOUSE NO. 1167 ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 2761 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3300 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/76**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPIE STREET NO. 1 BLOCK-N IN CHUSHTI NAGAR**

**IN UC-7**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.2,24,803/=*

*BID SECURITY.* Rs.4,496/=

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/76**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 2,24,803/= + O/R*

Earnest Money RS. 4,496/=*+ O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPIE STREET NO. 1 BLOCK-N IN CHUSHTI NAGAR**

**IN UC-7**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1650 | 4650.00 %0 CFT | 7673/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 300 | 10770.00 %0 CFT | 3231/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2)  9” DIA | 300 | 206.00 RFT | 61800/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 14 Nos | 13064 /= Each | 1,82,896/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -23 | 1540.00 RFT | -35420/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1675 | 2760.00 %0 CFT | 4,623/= |
| **SUB TOTAL PART-A** | | | | **2,24,803/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING RCC PIPIE STREET NO. 1 BLOCK-N IN CHUSHTI NAGAR**

**IN UC-7**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 250 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/77**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMPROVEMENT OF CARPETING AZHARA ACADEMY PLAYGROUND NEAR MASOOMABAD IN UC-7.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*6,94,847 /= + O/R

*BID SECURITY.* Rs.13,897 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/77**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 6,94,847 /= + O/R

Earnest Money Rs. 13,897 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **IMPROVEMENT OF CARPETING AZHARA ACADEMY PLAYGROUND NEAR MASOOMABAD IN UC-7.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6000 Sft | 773.86%  Sft | 46,432/= |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 12280 Cft | 1437.00%0  Cft | 17,646/= |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 15235.33Cft | 1065.00%  Cft | 162,256/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8000 Sft | 526.28%  Sft | 42,103/= |
| 05 | Applying Priming Coat or Tack Coat with approved binder at the required rate i/c cleaning the road surface thoroughly heating to the required temperature and spraying the binder with pressure as directed etc, complete (ch H/ways 12/31) | 8000 Sft | 64.96 %  Sft | 5,197/= |
| 06 | Providing 1” thick (consolidated) premixed carpet in proper camber and grade including supplying 10 CftBajri 4 cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the roads surface (rate i/c all cost of materials T & P and carriage upto 3 chains)  Using Crushed Bajri (8/12)  Laying Premixed Carpet (12/32) | 8000 Sft | 5093.86%  Sft | 407,509/= |
| 07 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 15 Nos. | 913.63 Each | 13,704/= |
| **SUB TOTAL PART-A** | | | | **694,847/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMPROVEMENT OF CARPETING AZHARA ACADEMY PLAYGROUND NEAR MASOOMABAD IN UC-7.**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 2000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3360 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/78**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **FILLING OF SINK DOWN TRENCHES POT HOLES BY FILLING STAFF LINK ROAD JOIN ALI NAGAR ROAD ZIA UL HAQ CHOWN AND OTHER WORK IN ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.2,45,480 /= + O/R*

*BID SECURITY.* Rs.*4,910/= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/78**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.2,45,480 /= + O/R*

Earnest Money *RS.4,910/= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **FILLING OF SINK DOWN TRENCHES POT HOLES BY FILLING STAFF LINK ROAD JOIN ALI NAGAR ROAD ZIA UL HAQ CHOWN AND OTHER WORK IN ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 11550 Cft | 1437.00%0  Cft | 16,597/= |
| 02 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 11550 Cft | 1065.00%  Cft | 123,012/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 5 Nos. | 13064 /= Each | 65,320/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | 15486 Rft | 1540.00 RFT | 8,449/= |
| 05 | P/F Cost Iron frame for main hole i/c the cost of material (Ch-p/health 35-J/1) | 350 Kga | 140/Kg | 49,000/= |
| **SUB TOTAL PART-A** | | | | **245,480/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **FILLING OF SINK DOWN TRENCHES POT HOLES BY FILLING STAFF LINK ROAD JOIN ALI NAGAR ROAD ZIA UL HAQ CHOWN AND OTHER WORK IN ORANGI ZONE.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 8000 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 7680 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/79**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR QADIR HOUSE IN SHAH MUHALLAH D STREET NO. 2**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,18,474/= + O/R*

*BID SECURITY.* Rs.16,369/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/79**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,18,474/= + O/R*

Earnest Money RS.16,369/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR QADIR HOUSE IN SHAH MUHALLAH D STREET NO. 2**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 3052 Cft | 24150.00 %0 CFT | 73706/= |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 555 Rft | 367.00 Rft | 2,03,685/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 24 Nos | 13064 /= Each | 3,13,536/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -54 | 1540.00 RFT | -83160/= |
| 05 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2372 | 2760.00 %0 CFT | 6547/= |
| 06 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 8000 | 526.28%  Sft | 42120/= |
| 07 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 8000 | 3275.50%  Sft | 262040/= |
| **SUB TOTAL PART-A** | | | | **8,18,474/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING & LAYING RCC PIPE AND CC STREET NEAR QADIR HOUSE IN SHAH MUHALLAH D STREET NO. 2**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 5355 Cft | Offer Rate | Offer Rate |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 1008 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2000 Cft | Offer Rate | Offer Rate |
| 04 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 231 Cwt | Offer Rate | Offer Rate |
| 05 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 15 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/80**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIRING OF DAMAGE PORTION OF RAOD, TRANCHES , POT HOLES BY CARPETING NEAR HABIB BANK QUARTER, DABBA MORE IN UC-09**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,51,672/= + O/R

*BID SECURITY.* Rs.15,033 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/80**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 7,51,672/= + O/R

Earnest Money Rs. 15,033 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REPAIRING OF DAMAGE PORTION OF RAOD, TRANCHES , POT HOLES BY CARPETING NEAR HABIB BANK QUARTER, DABBA MORE IN UC-09**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 6500 Sft | 773.86%  Sft | 50301/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 24413 Cft | 1437.00%0  Cft | 35081/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 27663 Cft | 1065.00%  Cft | 294611/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **7,51,672/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **CARPETING OF ROAD / DAMAGE PORTION AND SINK DOWN TRANCHES NEAR IRANI CAMP IMAM BARGAH PUNJATAN HOUSE IN UC-04**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Granular Sub Base Course material over prepared sub grade in conformity with lines, grade, thickness and typical cross sections for grade / widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer incharge. | 800 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3900 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/81**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **IMPROVEMENT OF RCC SLAB / NALA AT MUSTAFA COLONY MUHAMMAD NAGAR COLONY & OTHER PRESS IN ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.4,14,374 /= + O/R*

*BID SECURITY.* Rs.*8,287 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/81**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 4,14,374 /= + O/R*

Earnest Money *RS. 8,287 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **IMPROVEMENT OF RCC SLAB / NALA AT MUSTAFA COLONY MUHAMMAD NAGAR COLONY & OTHER PRESS IN ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of RCC concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1125 Cft | 5445.0% Cft | 61256/= |
| 02 | Dismantling of CC flooring. 1:2:4 plain (Ch-2/10/19c) | 2100 Cft | 3327.50 %  Cft | 69,878/= |
| 03 | Dismantling of cementconcrete flooring. 1:3:6 plain (10/19-b) | 1155 Cft | 1306.80%  Cft | 15,094/= |
| 04 | Earth work excavation in irrigation channels, irrigation drain etc dressed to designed section and profile excavated. | 5951 Cft | 2420.00%0  Cft | 14,401/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 16,282 | 1065.00% CFT | 1,73,403/= |
| 06 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 528 Cft | 4650.00 %0 CFT | 2455/= |
| 07 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 96Cft | 367.00 RFT | 35,232/= |
| 08 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 04 Nos | 13064 /= Each | 52,2,56/= |
| 09 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -7 Rft | 1540.00 RFT | -10,780/= |
| 10 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 427Cft | 2760.00 %0 CFT | 1179/= |
| **SUB TOTAL PART-A** | | | | **4,14,374/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **IMPROVEMENT OF RCC SLAB / NALA AT MUSTAFA COLONY MUHAMMAD NAGAR COLONY & OTHER PRESS IN ORANGI ZONE**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F RCC pre cast slab or linter of required size and shape and shape as per given design and racking out joints with CM curing etc complete as per direction of engineer incharge | 1181 Cft | Offer Rate | Offer Rate |
| 02 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 25 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/82**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPER GALI NO. 8 NEAR JAMIA MASJID SADA-E-MADINA GULSHAN-E-BEHAR IN UC-6 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,02,495/= + O/R*

*BID SECURITY.* Rs.18,050 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/82**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,02,495/= + O/R*

Earnest Money RS. 18,050 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPER GALI NO. 8 NEAR JAMIA MASJID SADA-E-MADINA GULSHAN-E-BEHAR IN UC-6 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 3000 Cft | 4650.00 %0 CFT | 13950/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2000 | 10770.00 %0 CFT | 21540/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA  12” DIA | 100 Rft  900 Rft | 206.00 RFT  367.00 RFT | 20600/=  3,30,300/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 45 Nos | 13064 /= Each | 5,87,880/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -67.5 | 1540.00 RFT | -103950/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 3940 | 2760.00 %0 CFT | 10874/= |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 2000 | 1065.00% CFT | 21301/= |
| **SUB TOTAL PART-A** | | | | **9,02,495/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING RCC PIPER GALI NO. 8 NEAR JAMIA MASJID SADA-E-MADINA GULSHAN-E-BEHAR IN UC-6 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 2000 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/83**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF CC STREET IN MAGSI MOHALLAH UC-13 IN ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,35,045 /= + O/R*

*BID SECURITY.* Rs.*16,701 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/83**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 8,35,045 /= + O/R*

Earnest Money *RS. 16,701 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REHABILITATION OF CC STREET IN MAGSI MOHALLAH UC-13 IN ORANGI ZONE.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 1641 Cft | 3327.50 %  Cft | 54604/= |
| 02 | Excavation for pipe line in trenches & pits in hard rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 7000 Cft | 25936.00 %0 CFT | 1,81,552/= |
| 03 | Dressing stone (Hammer dressed) | 3000 Sft | 2390.00% Sft | 71,700/= |
| 04 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 8000 Sft | 526.28%  Sft | 42,102/= |
| 05 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 12000 Sqf | 3275.50%  Sft | 3,93,060/= |
| 06 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 8641 Cft | 1065.00% CFT | 92,027/= |
| **SUB TOTAL PART-A** | | | | **8,35,045/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION OF CC STREET IN MAGSAY MOHALLAH UC-13 IN ORANGI ZONE.**

**.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3500 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/84**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPER & CC STREET GULSHAN-E-ZIA SHEET NO. 3, GALI NO.2 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.5,75,959/= + O/R*

*BID SECURITY.* Rs.11,519 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/84**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 5,75,959/= + O/R*

Earnest Money RS. 11,519 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPER & CC STREET GULSHAN-E-ZIA SHEET NO. 3, GALI NO.2 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:3:6 plain (10/19-b) | 578 Cft | 1306.80%  Cft | 7553/= |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1200 Cft | 4650.00 %0 CFT | 5580/= |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 800 | 10770.00 %0 CFT | 8616/= |
| 04 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 400 Rft | 206.00 RFT | 82400/= |
| 05 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 18 Nos | 13064 /= Each | 2,35,152/= |
| 06 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -27 | 1540.00 RFT | -41580/= |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 1634 | 2760.00 %0 CFT | 4510/= |
| 08 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 7200 | 526.28%  Sft | 37892/= |
| 09 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 7200 | 3275.50%  Sft | 2,35,836/= |
| **SUB TOTAL PART-A** | | | | **5,75,959/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **PROVIDING AND LAYING RCC PIPER & CC STREET GULSHAN-E-ZIA SHEET NO. 3, GALI NO.2 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 2139 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2088 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/85**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **PROVIDING AND LAYING RCC PIPER & NEAR PEHALWAN HOTAL SECTOR 11 ½ ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.9,31,936/=*

*BID SECURITY.* Rs.18,639 /=

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/85**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 9,31,936/=*

Earnest Money RS. 18,639 /=

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **PROVIDING AND LAYING RCC PIPER & NEAR PEHALWAN HOTAL SECTOR 11 ½ ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 3000 Cft | 4650.00 %0 CFT | 13950/= |
| 02 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2000 | 10770.00 %0 CFT | 21540/= |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 9” DIA | 100 Rft  900 Rft | 206.00 RFT  367.00 Rft | 20600/=  330300/= |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 48 Nos | 13064 /= Each | 627072/= |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -60 | 1540.00 RFT | -92400/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 3940 | 2760.00 %0 CFT | 10874/= |
| **SUB TOTAL PART-A** | | | | **9,31,936/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/86**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR AND REHABILITATIOBN OF ROAF IN GALI NO. 30 AND DIFFERENT PLACES IN UC-05**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*8,04,739/= + O/R

*BID SECURITY.* Rs.16,095/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/86**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 8,04,739/= + O/R

Earnest Money Rs. 16,095/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REPAIR AND REHABILITATIOBN OF ROAF IN GALI NO. 30 AND DIFFERENT PLACES IN UC-05**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 7000 Sft | 773.86%  Sft | 54170/- |
| 02 | Earth work excavation of road side nalis forming its banks or putting the same on embankment as directed breaking clods dressing etc complete in ordinary soil (1/4-H/ways) | 28263 Cft | 1437.00%0  Cft | 40614/- |
| 03 | Cartage of sand, bajri, lime, sukhi, murrum and building rubbish i/c loading unloading and stacking at site (10 miles) (Ch 1/1-1) | 31763Cft | 1065.00%  Cft | 338276/- |
| 04 | Premixed patch repair 1” thick including cleaning cutting scattered patches in proper shape laying premixed chips rolling etc complete (rate i/c all cost of materials T&P and carriage up to 3 chains) P-09/19 using crushed bajri laying premixed carpet | 7800Sft | 4765.11%Sft | 371679/- |
| **SUB TOTAL PART-A** | | | | **8,04,739/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR AND REHABILITATIOBN OF ROAF IN GALI NO. 30 AND DIFFERENT PLACES IN UC-05**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/F per costed RCC Ring Slab 39” Dia with RCC manhole cover of 21” dia as per direction of engineer incharge | 12 Nos | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 2925 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/87**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF CARPETING GALI NO. 8 NEAR GRAVEYARD IN GHAZIABAD UC-6**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.6,95,425/= + O/R*

*BID SECURITY.* Rs.13,909 /= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/87**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 6,95,425/= + O/R*

Earnest Money RS. 13,909 /= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF CARPETING GALI NO. 8 NEAR GRAVEYARD IN GHAZIABAD UC-6**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of existing asphalt concrete road i/c base, sub base and disposal of dismantled material to designated placed (15/11-H/ways) | 536 Cft | 773.86%  Cft | 4148/= |
| 02 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 12,300 Sft | 526.28%  Sft | 64,732/= |
| 03 | Providing 1” thick (consolidate) premixed carpet in proper camber and grade including supplying 10 Cft: Bajri. 4 Cft hill sand (of approved quality and grade) bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the road surface (Rate i/c all cost of materials T&P and carriage upto 3 chains, Using Crushed Bajri.  Laying premixed. | 12300 Sft | 5093.86 % CFT | 6,26545/= |
| **SUB TOTAL PART-A** | | | | **6,95,425/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **CONSTRUCTION / IMPROVEMENT OF CARPETING GALI NO. 8 NEAR GRAVEYARD IN GHAZIABAD UC-6**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 02 | P/L Granular sub base course material over prepared sub grade in conformity with lines, grade, thickness and typical cross section for grade/ widening well graded granular stone with sand and silt having a smooth gradation I as per AASHTO-M 147-65(1980) and compacting dry density approved mechanical means of i/c watering with all lead and lift as per directed by engineer in charge. | 2505 Cft | Offer Rate | Offer Rate |
| 03 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4613 Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/88**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR AND MAINTENANCE OF RCC PIPE 12” DIA AND CC STREET NEAR RAFI HOUSE BISMMILAH COLONY IN UC-2.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,53,774 /= + O/R*

*BID SECURITY.* Rs.*15,075 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/88**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS. 7,53,774 /= + O/R*

Earnest Money *RS. 15,075 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR AND MAINTENANCE OF RCC PIPE 12” DIA AND CC STREET NEAR RAFI HOUSE BISMMILAH COLONY IN UC-2.**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 2600 Cft | 10770.00 %0 CFT | 28002/= |
| 02 | P/L RCC Rubber rig pipe of Class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 400  RFT | 367.00  RFT | 1,46,800/= |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 17 Nos | 13064 /= Each | 2,22,088/= |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -27.25 | 1540.00 RFT | -41965/= |
| 05 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 2210 Cft | 2760.00 %0 CFT | 6100/= |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 20 Nos | 913.63 Each  1051.25 Each | 18,273/= |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (H/ways-2/9) | 9850 Sft | 526.28%  Sft | 51,839/= |
| 08 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 9850 Sft | 3275.50%  Sft | 3,22,637/= |
| **SUB TOTAL PART-A** | | | | **7,53,774/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR AND MAINTENANCE OF RCC PIPE 12” DIA AND CC STREET NEAR RAFI HOUSE BISMMILAH COLONY IN UC-2.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
|  | Supply & Filling of imported earth with in the radios of 5 miles including load, unloading & all lead & lift leveling & compacting etc. | 2500 Cft | Offer Rate | Offer Rate |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2857 Cft | Offer Rate | Offer Rate |
| 02 | Extra for using (SR Cement) sulphate resistant cement in place of ordinary Portland cement. | 285 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/89**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF SEWERAGE SYSTEM BY RCC 12” DIA NEAR MUHAMMADI MASJID ORANGI ZONE.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*9, 24,186/= (+) O/R.

*BID SECURITY.* Rs.18,484/= (+) O/R.

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION, KARACHI WEST. 4/89**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 9, 24,186/= (+) O/R.

Earnest Money Rs. 18,484/= (+) O/R.

Tender Cost. Rs. 1,000.00

Time Limit.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Penalty. Rs. 1,000.00 Per Day.

SUBJECT: REHABILITATION OF SEWERAGE SYSTEM BY RCC 12” DIA NEAR MUHAMMADI MASJID ORANGI ZONE.

PART-A ITEM BASED ON SCHEDULE RATES.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SL. # | DESCRIPTION | QUANTITY | RATE/UNIT | AMOUNT |
| 01 | Dismantling of cement concrete plain flooring.  (10/19 a-b-c) C.C. 1:2:4. | 2,596 CFT | 3327.50 % cft | 86,382/= |
| 02 | Excavation for pipe li ne in trenches & pits in all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge.(62/5) | 2600 CFT | 4650.00 0% 0 cft | 12,090/= |
| 03 | Excavation for pipe line in trenches & pits in soft rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer kin charge (62/6) | 2,475 CFT | 10770.00 0 CFT | 26,656/= |
| 04 | P/L. RCC rubber ring pie of class A and fixing in trenches i/c cutting, fitting and jointing with rubber ring etc complete.  12” dia | 800 RFT | 367.00 RFT | 2,93,600/= |
| 05 | Construction of manhole 4’ dia inside i/c RCC ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 in 9” thick wall and bedding cast in situ with fair face steel shuttering i/c excavation back filling and dispose of surplus stuff up to one chain etc complete. (app/rate) | 40 Nos | 13064.00 EACH | 5,22,560/= |
| 06 | Add for extra depth beyond 5 ft depth less the 5 ft deduct the same rate. | (-)70 RFT | 1540.00 RFT | (-)1,07,800/= |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete.(ch-11/77-24) | 1754 CFT | 2760.00 0% cft | 4,841/= |
| 08 | Cartage of sand, bajri, lime surki murum building rubbish i/c loading and unloading and stacking at site. All lide & lift ( Ch 1/1-1) | 5917 Cft | 1065.00% cft | 63,016/= |
| 09 | P/L. 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete.  (ch-16/31-1) | 25 Nos. | 913.63 EACH | 22,841/= |
| SUB TOTAL PART-A | | | | 9,24,186/= (+)O/R |

SIGNATURE OF CONTRACTOR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

SUBJECT: REHABILITATION OF SEWERAGE SYSTEM BY RCC 12” DIA NEAR

MUHAMMADI MASJID ORANGI ZONE.

PART-B ITEM BASED ON OFFER RATES.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SL.# | DESCRIPTION | QUANTITY | RATES/UNIT | AMOUNT |
| 01 | P/F. Per Coasted R.C.C. Ring slab 39” dia with R.C.C. Manhole C over of 21” dia as per direction of engineer in charge. | 15 Nos. | OFFER RATES  RS:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 02 | S/F. Imported Earth with in the a radius of 5 miles i/c digging, lodging, un lodging all lead and lift leveling and water compaction etc complete. | 1650 CFT | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | OFFER RATE  RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

SIGNATURE OF CONTRACTOR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ADDRESS: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

I/WE HEREBY QUOTED RATES AS FOLLOWS:-

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (ITEM RATES BASES ON SR)  @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ % ABOVE / BELOW SR I/C THE COST OF CARRIAGE OF MATERIALS AND DIFFERENCE OF COST OF BITUMEN. | RS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 02 | PART-B (ITEM RATE BASES ON OFFER RATES/ITEM RATES THE ITEMS OTHER THEN SCHEDULE RATES | RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| GRAND TOTAL PART-A & B | | RS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

TOTAL RS.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_RUPEES\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature of contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Cell #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ PTCL # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/90**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND C.C. TOPPING IN GALI # 3 AND 4 NEAR NAJORI HOUSE ,UC-13.**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.*8, 18,550/= (+) O/R.

*BID SECURITY.* Rs.16,371/= (+) O/R.

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION, KARACHI WEST. 4/90**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. 8, 18,550/= (+) O/R.

Earnest Money Rs. 16,371/= (+) O/R.

Tender Cost. Rs. 1,000.00

Time Limit.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Penalty. Rs. 1,000.00 Per Day.

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND C.C. TOPPING IN GALI # 3 AND 4 NEAR NAJORI HOUSE ,UC-13.**

PART-A ITEM BASED ON SCHEDULE RATES.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SL. # | DESCRIPTION | QUANTITY | RATE/UNIT | AMOUNT |
| 01 | Dismantling of cement concrete plain flooring.  (10/19 a-b-c) C.C. 1:2:4. | 2991 CFT | 3327.50 % cft | 99,526/= |
| 02 | Excavation for pipe li ne in trenches & pits in all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge.(62/5) | 1650 CFT | 4650.00 0% 0 cft | 7,673/= |
| 03 | Preparing of sub grade i/c earth excavation leveling to an average depthof 9’ dressing to camber and consolidation with power roller.(2/9-H/ways) | 10,000 SFT | 526.28 % SFT | 52,628/= |
| 04 | P/L. RCC rubber ring pie of class A and fixing in trenches i/c cutting, fitting and jointing with rubber ring etc complete.  12” dia | 300 RFT | 367.00 RFT | 1,10,100/= |
| 05 | Construction of manhole 4’ dia inside i/c RCC ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 in 9” thick wall and bedding cast in situ with fair face steel shuttering i/c excavation back filling and dispose of surplus stuff up to one chain etc complete. (app/rate) | 15 Nos | 13064.00 EACH | 1,95,960/= |
| 06 | Add for extra depth beyond 5 ft depth less the 5 ft deduct the same rate. | (-)18.75 RFT | 1540.00 RFT | (-)28,875/= |
| 07 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete.(ch-11/77-24) | 1333 CFT | 2760.00 0% cft | 3,677/= |
| 08 | Cartage of sand, bajri, lime surki murum building rubbish i/c loading and unloading and stacking at site. All lide & lift ( Ch 1/1-1) | 4752 Cft | 1065.00% cft | 50,609/= |
| 09 | P/L. 1 ½” THICK TOPPING c.c. (1:2:4) i/c surface finishing & dividing into panels (42/16-b-c-d) | 10,000 SFT | 3275.50 % SFT | 3,27,550/= |
| SUB TOTAL PART-A | | | | 8,18,550/= (+)O/R |

SIGNATURE OF CONTRACTOR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ؎

SUBJECT: **IMPROVEMENT OF SEWERAGE SYSTEM BY REPAIRING / REPLACEMENT OF DAMAGE PORTION OF PIPE AND C.C. TOPPING IN GALI # 3 AND 4 NEAR NAJORI HOUSE ,UC-13.**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 12 | P/L 1:2:4 RCC Ring Slab including 21” Dia manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) | 30 Nos. | Offer Rate | Offer Rate |
|  | S/F. Imported Earth with in the a radius of 5 miles i/c digging, lodging, un lodging all lead and lift leveling and water compaction etc complete. | 1650 CFT | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/91**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REHABILITATION OF RCC PIPE AT ILAHIABAD ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,16,522*/= + O/R

*BID SECURITY.* Rs.*14,330*/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/91**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *7,16,522*/= + O/R

Earnest Money Rs. *14,330*/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs.

Subject: **REHABILITATION OF RCC PIPE AT ILAHIABAD ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in hard rock by hammering and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge  (64/10) | 3900 Cft | 24150.00 %0 CFT | 94185/- |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 600 Rft | 367.00 RFT | 220200/- |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 30 No. | 13064 /= Each | 391920/- |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -508 Rft | 1540.00 RFT | -77000/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3900 Cft | 1065.00% CFT | 41535/- |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 50 Nos. | 913.63 | 45682/- |
| **SUB TOTAL PART-A** | | | | **7,16,522/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REHABILITATION OF RCC PIPE AT ILAHIABAD ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness and typical widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according to AASHTO-T-180 method D using approved mechanical means of i/c watering with all lead and lift as per specification and as per directed by engineer incharge | 3300 Cft | Offer Rate | Offer Rate |
| 02 | Providing & Fixing RCC Ring Slab 39” Dia with RCC Main hole Cover 21” Dia as per direction of engineer incharge. | 50 Nos | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/92**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **REPAIR AND MAINTINANCE OF SEWERAGE SYSTEM AND CC STREET NEAR MASJID UMER FAROOQ SHEET NO. 10 ORANGI ZONE**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,91,088* /= + O/R

*BID SECURITY.* Rs.17,822/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/92**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,91,088* /= + O/R

Earnest Money Rs.17,822/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **REPAIR AND MAINTINANCE OF SEWERAGE SYSTEM AND CC STREET NEAR MASJID UMER FAROOQ SHEET NO. 10 ORANGI ZONE**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 3900  Cft | 10770.00 %0 CFT | 42003/- |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA  15” DIA | 600 Rft | 367.00 RFT | 220200/- |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling &complete (app/rate) | 26  Nos | 13064 /= Each | 339664/- |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 52  Rft | 1540.00 RFT | -80080/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3900  Cft | 1065.00% CFT | 41535/- |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 10 No. | 913.63 Each | 9136/- |
| 07 | Preparing of sub grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller (2/9) | 8400 Sft | 526.28%  Sft | 44208/- |
| 08 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 8400  Sft | 3275.50%  Sft | 275142/- |
| **SUB TOTAL PART-A** | | | | **8,91,088/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **REPAIR AND MAINTINANCE OF SEWERAGE SYSTEM AND CC STREET NEAR MASJID UMER FAROOQ SHEET NO. 10 ORANGI ZONE**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 2772  Cft | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/93**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REPAIR OF BROKEN PIPE & MAIN HOLE AND CC FLOORING IN TOUHEEDI MUHALLAH IN UC-02 .**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.7,73,318 /= + O/R*

*BID SECURITY.* Rs.*15,466 /= + O/R*

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/93**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost *RS.7,73,318 /= + O/R*

Earnest Money *RS.15,466 /= + O/R*

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000

SUBJECT: **REPAIR OF BROKEN PIPE & MAIN HOLE AND CC FLOORING IN TOUHEEDI MUHALLAH IN UC-02 .**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring. 1:2:4 plain (Ch-2/10/19c) | 2302 Cft | 3327.50 %  Cft | 76599/- |
| 02 | Excavation for pipe line in trenches & pits all kind of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level & shape leveling of beds of trenches to correct level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1100 Cft | 4650.00 %0 CFT | 5115/- |
| 03 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 12” DIA | 200 Rft | 367.00 RFT | 73400/- |
| 04 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling & complete (app/rate) | 10 Nos. | 13064 /= Each | 130640/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | -17.5 Rft | 1540.00 RFT | -26950/= |
| 06 | Refilling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete (ch-11/77-24) | 889 Cft | 2760.00 %0 CFT | 2454/- |
| 07 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 3957Cft | 1065.00% CFT | 42142/- |
| 08 | P/L 1:2:4 RCC Manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete. (Ch-16/31-1) 21” Dia | 15 Nos. | 913.63 Each | 13704/= |
| 09 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 12000  Sft | 526.28%  Sft | 63154/- |
| 10 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 12000  Sft | 3275.50%  Sft | 393060/- |
| **SUB TOTAL PART-A** | | | | **7,73,318/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REPAIR OF BROKEN PIPE & MAIN HOLE AND CC FLOORING IN TOUHEEDI MUHALLAH IN UC-02 .**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1688 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3500 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/94**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

SUBJECT: **REHABILITATION OF PIEP DRAIN & CC FLOORING AT MUSQATI MUHALLAH IN**

**UC-02 .**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.* 7,45,894/= (+) O/R

*BID SECURITY.* Rs.14,918/= (+) O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST. 4/94**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs.7,45,894/= (+) O/R

Earnest Money Rs. 14,918/= (+) O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000/-

SUBJECT: **REHABILITATION OF PIEP DRAIN & CC FLOORING AT MUSQATI MUHALLAH IN**

**UC-02 .**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Dismantling of cement concrete flooring 1:2:4 plain. (Ch-2/10/19-C) | 1890 Cft | 3327.50 % CFT | 62890/- |
| 02 | Excavation of Pipe line in trenches & pits in all kinds of soils of murum i/c trimming and dressing sides to true alignment & shape leveling of beds of trenches to correct level and grade cutting joint holes and disposal of surplus earth within one chain as directed by engineer in charge (62/5) | 1300 Cft | 4650.00%  Sft | 6045/- |
| 03 | P/L RCC Rubber ring pipe of class “A” and fixing in trenches i/c cutting, fitting & jointing with rubber ring etc complete. (18/2) 12” Dia, | 200 Rft | 367.00 Rft | 73400/- |
| 04 | Construction of manholes 4” dia inside i/c RCC Ring Slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling and disposal of surplus stuff etc complete. | 10 Nos. | 13064  Each | 130640/- |
| 05 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 17.5  Rft | 1540.00  Rft | -26950/- |
| 06 | Re filling of excavated stuff in trenches 6”th layer i/c watering ramming to full compaction etc complete. | 1089 ft | 2760.00%0 Cft | 3006/- |
| 07 | Cartage of sand, Bajri, lime, sukhi, murrum& building rubbish i/c loading unloading & stacking at site. (10 miles) (Ch 1/1-1) | 2101  Cft | 1065.00%  Cft | 22376/- |
| 08 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia  24” Dia | 20 Nos. | 913.63  Each | 18273/- |
| 09 | Preparing of Sub-Grade i/c earth excavation leveling to an average depth of 9” dressing to camber and consolidation with power roller. | 12000  Sft | 526.28%  Sft | 63154/- |
| 10 | P/L 2” thick topping C.C (1:2:4) i/c surface finishing & dividing in to panels. | 12000  Sft | 3275.50%  Sft | 393060/- |
| **SUB TOTAL PART-A** | | | | **7,45,894/-** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

SUBJECT: **REHABILITATION OF PIEP DRAIN & CC FLOORING AT MUSQATI MUHALLAH IN**

**UC-02 .**

**PART-B ITEM BASED ON SCHEDULE RATES**

***Address***

I / we hereby quoted rates as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | S/F Imported Earth with in the a radius of 5 miles i/c digging, lodging un-lodging all lead and lift leveling and water compaction etc complete (A/rate) | 1688 Cft | Offer Rate | Offer Rate |
| 02 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 3480 Cft | Offer Rate | Offer Rate |
| 03 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos. | Offer Rate | Offer Rate |
| 04 | Extra for using (S.R Cement) Sulphate resistant cement on place of ordinary portland cement | 347 Cwt | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST.**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI. 4/95**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

TENDER REFERENCE # NIT /\_\_\_\_/2016. Dated: \_\_\_\_\_\_\_\_\_\_\_\_/2016.

Subject: **IMP OF SEWERAGE SYSTEM BY RCC PIPE AT UMER BALOCH MUHALLAH (PHASE-II) IN UC-02**

**BILL OF QUANTITIES**

*ESTIMATED COST. RS.8,09,424* /= + O/R

*BID SECURITY.* Rs.16,188/= + O/R

*TENDER COST. RS.1000/=*

*PENALTY. RS.1000/=Per Day*

Issued to M/s. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Video pay order / Challan # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ dated:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature and Stamp

**DISTRICT MUNICIPAL CORPORATION , KARACHI WEST 4/95**

**SECTOR 11-E SHAHRAH-E-ORANGI, ORANGI TOWN, KARACHI.**

**PTCL # 366697869 / 36660102 & FAX # 36762519**

Estimated Cost Rs. *8,09,424* /= + O/R

Earnest Money Rs.16,188/= + O/R

Tender Cost Rs. 1,000.00

Time Limit : \_\_\_\_\_\_\_\_\_

Penalty Rs. 1000.00

Subject: **IMP OF SEWERAGE SYSTEM BY RCC PIPE AT UMER BALOCH MUHALLAH (PHASE-II) IN UC-02**

**PART-A ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | Excavation for pipe line in trenches & pits in soft rock by hammerings and chiseling i/c alignment & shape level & grade cutting joint holes & disposal of surplus earth within one chain as directed by engineer in charge (62/6) | 9450  Cft | 10770.00 %0 CFT | 101777/- |
| 02 | P/L RCC Rubber ring Pipe of class “A” and fixing in trenches i/c cutting fitting & jointing with rubber ring etc complete. (18/2) 15” DIA | 700 Rft | 436.00 RFT | 305200/- |
| 03 | Construction of manholes 4’ dia inside i/c RCC Ring slab 39” dia with manhole cover 21” dia of 5’ clear depth in 1:2:4 CC in 9” thick wall &beding cast in situ with fair face steel shuttering i/c excavation, back filling &complete (app/rate) | 25  Nos | 13064 /= Each | 326600/- |
| 04 | Add for extra depth beyond 5 feet depth, lass then 5 ft depth deduct the same rate. | (-) 25  Rft | 1540.00 RFT | -38500/= |
| 05 | Cartage of sand, bajri, lime, sukhi, murrum, bulding rubbish i/c loading unloading stacking at site. All lide& lift (Ch 1/1-1) | 9450  Cft | 1065.00% CFT | 100643/- |
| 06 | P/L 1:2:4 RCC manhole cover i/c tor bars frame using GSB ¾” and down gauge etc complete  (CH-16/31-1) 21” Dia | 15 No. | 913.63 Each | 13704/- |
| **SUB TOTAL PART-A** | | | | **8,09,424/=** |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

Subject: **IMP OF SEWERAGE SYSTEM BY RCC PIPE AT UMER BALOCH MUHALLAH (PHASE-II) IN UC-02**

**PART-B ITEM BASED ON SCHEDULE RATES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION** | **QUANTITY** | **RATE/UNIT** | **AMOUNT** |
| 01 | P/L Aggregate base course material over prepared sub grade in conformity with lines, grade, thickness, and typical cross sections fir grade/ widening existing pavement using well graded granular crushed stone with sand and silt having a smooth gradation curve with in the limit for grading A or B as per AASHTO-M 142-65(1985) and compacting to 100% of the minimum dry density according means of i/c watering with all lead and lift as per specification and as per directed by engineer in charge. | 4900  Cft | Offer Rate | Offer Rate |
| 02 | P/F R.C.C. Ring Slab 39” Dia with R.C.C. manhole cover of 21” dia as per direction of engineer incharge. | 15 Nos. | Offer Rate | Offer Rate |
| **SUB TOTAL PART-B** | | | |  |

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Signature of Contractor***

***Address***

I / we hereby quoted rates as follows:

|  |  |  |
| --- | --- | --- |
| 01 | PART-A (Item Rates Based on SR)  @ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% above / below SR i/c the cost of carriage of materials and difference of cost of bitumen | Rs. |
| 02 | PART-B (Item Rates Based on Offer Rates / Item Rates the items other then schedule rates) | Rs. |
| **GRAND TOTAL PART-A & B** | | **Rs.** |

Total Rs. Rupees

***Signature of Contractor***

***Address :***

***Cell # / PTCL #.***