PART-A

Name of work: CONSTRUCTION C.C.PAVER BLOCK & SURFACE DRAIN FOR UC- DRIB, TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Supplying and filling sand under floor and plugging in walls. (S.I. NO. 29, P-26) | 25220.0 | 1141.25 | % CFT | 287823.0 |
| 02 | Dressing & leveling and earth work to designed section etc complete, (a) Ashes, sand and silt of soft soil. | 25220.0 | 96.80 | % CFT | 24413.0 |
| 03 | Cement Concrete Plain i/c placing compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering. (CSI NO: 5, P. No: 15)(b)Ratio 1 : 4 : 8 | 6305.0 | 11288.75 | % CFT | 711756.0 |
| 04 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 16393.0 | 223.97 | P.SFT | 16393.0 |
| 05 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 8827.0 | 248.10 | P.SFT | 2189979.0 |
| 06 | Erection & Removal of centering for RCC or plain Cement Concrete works of deodar wood “ 2nd class”. | 5044.0 | 3127.41 | % SFT | 157747.0 |
| 07 | Cement concrete plain placing, compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering(CSI NO: 5, P. No: 15) (b) Ratio 1 : 2 : 4 | 2522.0 | 14429.25 | % CFT | RS.363906.0 |
|  |  |  | TOTAL | RS. | 7407164.0 |
|  | Above/ Below % on the rates of CSR |  |  | RS. |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

PART – B

NAME OF WORK :- CONSTRUCTION OF SURFACE DRAIN FOR UC- DRIB,TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Excavation in foundation of Building, Bridges & other structures i/c dag belling dressing, refilling around structure with excavated earth watering & ramming lead up to 5ft. (CSI-18 (b) P-04) | 375.0 | 3176.25 | %0 CFT | 1191.0 |
| 02 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:4:8 (CSI-05 (i) P-15 | 62.50 | 11288.75 | % CFT | 7055.0 |
| 03 | Erection & removal of centering for RCC or plain Cement Concrete works of Deodar wood ( 2nd Class) ii-Vertical. (CSI-19 (ii) P-18) | 375.0 | 3127.41 | % SFT | 11728.0 |
| 04 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:2:4 (CSI-05 (f) P-16) | 175.0 | 14429.25 | % CFT | 25251.0 |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels & other structural members laid in situ or precast laid in position complete in all respects, Ratio (1:2:4) 90 Lbs, cement 2Cft Sand 4 Cft. Shingle 1/8” to ¼” guage.(CSI-06 (i) P-16) | 15.84 | 337.0 | P. CFT | 5338.0 |
| 06 | Fabrication of Mild Steel reinforcement for cement concrete i/c cutting, bending, laying in position, making joints & fastening i/c cost of building wire (also i/c removeal of) (b) Using Tor bars. (CSI-08 (b) P-17 | 0.636 | 5001.70 | P. CWT | 3181.0 |
|  |  |  | TOTAL | RS. | 53744.0 |
|  | Add Above/ Below on the rate of CSR |  | TOTAL | RS |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

**PART-A**

Name of work: CONSTRUCTION C.C.PAVER BLOCK & SURFACE DRAIN FOR UC- HINGORO & UC- SANGI, TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Supplying and filling sand under floor and plugging in walls. (S.I. NO. 29, P-26) | 25220.0 | 1141.25 | % CFT | 287823.0 |
| 02 | Dressing & leveling and earth work to designed section etc complete, (a) Ashes, sand and silt of soft soil. | 25220.0 | 96.80 | % CFT | 24413.0 |
| 03 | Cement Concrete Plain i/c placing compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering. (CSI NO: 5, P. No: 15)(b)Ratio 1 : 4 : 8 | 6305.0 | 11288.75 | % CFT | 711756.0 |
| 04 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 16393.0 | 223.97 | P.SFT | 16393.0 |
| 05 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 8827.0 | 248.10 | P.SFT | 2189979.0 |
| 06 | Erection & Removal of centering for RCC or plain Cement Concrete works of deodar wood “ 2nd class”. | 5044.0 | 3127.41 | % SFT | 157747.0 |
| 07 | Cement concrete plain placing, compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering(CSI NO: 5, P. No: 15) (b) Ratio 1 : 2 : 4 | 2522.0 | 14429.25 | % CFT | RS.363906.0 |
|  |  |  | TOTAL | RS. | 7407164.0 |
|  | Above/ Below % on the rates of CSR |  |  | RS. |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

PART – B

NAME OF WORK :-CONSTRUCTION OF SURFACE DRAIN FOR UC- HINGORO & UC- SANGI,TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Excavation in foundation of Building, Bridges & other structures i/c dag belling dressing, refilling around structure with excavated earth watering & ramming lead up to 5ft. (CSI-18 (b) P-04) | 375.0 | 3176.25 | %0 CFT | 1191.0 |
| 02 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:4:8 (CSI-05 (i) P-15 | 62.50 | 11288.75 | % CFT | 7055.0 |
| 03 | Erection & removal of centering for RCC or plain Cement Concrete works of Deodar wood ( 2nd Class) ii-Vertical. (CSI-19 (ii) P-18) | 375.0 | 3127.41 | % SFT | 11728.0 |
| 04 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:2:4 (CSI-05 (f) P-16) | 175.0 | 14429.25 | % CFT | 25251.0 |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels & other structural members laid in situ or precast laid in position complete in all respects, Ratio (1:2:4) 90 Lbs, cement 2Cft Sand 4 Cft. Shingle 1/8” to ¼” guage.(CSI-06 (i) P-16) | 15.84 | 337.0 | P. CFT | 5338.0 |
| 06 | Fabrication of Mild Steel reinforcement for cement concrete i/c cutting, bending, laying in position, making joints & fastening i/c cost of building wire (also i/c removal of) (b) Using Tor bars. (CSI-08 (b) P-17 | 0.636 | 5001.70 | P. CWT | 3181.0 |
|  |  |  | TOTAL | RS. | 53744.0 |
|  | Add Above/ Below on the rate of CSR |  | TOTAL | RS |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

**PART -A**

Name of work: CONSTRUCTION C.C.PAVER BLOCK & SURFACE DRAIN FOR UC- PANO GHULAM ALI & UC-BAIJI, TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Supplying and filling sand under floor and plugging in walls. (S.I. NO. 29, P-26) | 25220.0 | 1141.25 | % CFT | 287823.0 |
| 02 | Dressing & leveling and earth work to designed section etc complete, (a) Ashes, sand and silt of soft soil. | 25220.0 | 96.80 | % CFT | 24413.0 |
| 03 | Cement Concrete Plain i/c placing compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering. (CSI NO: 5, P. No: 15)(b)Ratio 1 : 4 : 8 | 6305.0 | 11288.75 | % CFT | 711756.0 |
| 04 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 16393.0 | 223.97 | P.SFT | 16393.0 |
| 05 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 8827.0 | 248.10 | P.SFT | 2189979.0 |
| 06 | Erection & Removal of centering for RCC or plain Cement Concrete works of deodar wood “ 2nd class”. | 5044.0 | 3127.41 | % SFT | 157747.0 |
| 07 | Cement concrete plain placing, compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering(CSI NO: 5, P. No: 15) (b) Ratio 1 : 2 : 4 | 2522.0 | 14429.25 | % CFT | RS.363906.0 |
|  |  |  | TOTAL | RS. | 7407164.0 |
|  | Above/ Below % on the rates of CSR |  |  | RS. |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

PART – B

NAME OF WORK :- CONSTRUCTION OF SURFACE DRAIN FOR UC- PANO GHULAM ALI & UC- BAIJI,

TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Excavation in foundation of Building, Bridges & other structures i/c dag belling dressing, refilling around structure with excavated earth watering & ramming lead up to 5ft. (CSI-18 (b) P-04) | 375.0 | 3176.25 | %0 CFT | 1191.0 |
| 02 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:4:8 (CSI-05 (i) P-15 | 62.50 | 11288.75 | % CFT | 7055.0 |
| 03 | Erection & removal of centering for RCC or plain Cement Concrete works of Deodar wood ( 2nd Class) ii-Vertical. (CSI-19 (ii) P-18) | 375.0 | 3127.41 | % SFT | 11728.0 |
| 04 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:2:4 (CSI-05 (f) P-16) | 175.0 | 14429.25 | % CFT | 25251.0 |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels & other structural members laid in situ or precast laid in position complete in all respects, Ratio (1:2:4) 90 Lbs, cement 2Cft Sand 4 Cft. Shingle 1/8” to ¼” guage.(CSI-06 (i) P-16) | 15.84 | 337.0 | P. CFT | 5338.0 |
| 06 | Fabrication of Mild Steel reinforcement for cement concrete i/c cutting, bending, laying in position, making joints & fastening i/c cost of building wire (also i/c removal of) (b) Using Tor bars. (CSI-08 (b) P-17 | 0.636 | 5001.70 | P. CWT | 3181.0 |
|  |  |  | TOTAL | RS. | 53744.0 |
|  | Add Above/ Below on the rate of CSR |  | TOTAL | RS |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

**PART -A**

Name of work: CONSTRUCTION C.C.PAVER BLOCK & SURFACE DRAIN FOR UC-JUNAS & UC-NIRCH, TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Supplying and filling sand under floor and plugging in walls. (S.I. NO. 29, P-26) | 25220.0 | 1141.25 | % CFT | 287823.0 |
| 02 | Dressing & leveling and earth work to designed section etc complete, (a) Ashes, sand and silt of soft soil. | 25220.0 | 96.80 | % CFT | 24413.0 |
| 03 | Cement Concrete Plain i/c placing compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering. (CSI NO: 5, P. No: 15)(b)Ratio 1 : 4 : 8 | 6305.0 | 11288.75 | % CFT | 711756.0 |
| 04 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 16393.0 | 223.97 | P.SFT | 16393.0 |
| 05 | Providing and fixing cement paving block flooring having size 197 x 97 x 80 (mm) of city / Quadra / cobble shape with pigmented having strength b/w 5000 psi to 8500 psi including filling joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I.NO. 73, P.NO.50 | 8827.0 | 248.10 | P.SFT | 2189979.0 |
| 06 | Erection & Removal of centering for RCC or plain Cement Concrete works of deodar wood “ 2nd class”. | 5044.0 | 3127.41 | % SFT | 157747.0 |
| 07 | Cement concrete plain placing, compacting finishing and curing Complete i/c screening and washing of stone aggregate without Shuttering(CSI NO: 5, P. No: 15) (b) Ratio 1 : 2 : 4 | 2522.0 | 14429.25 | % CFT | RS.363906.0 |
|  |  |  | TOTAL | RS. | 7407164.0 |
|  | Above/ Below % on the rates of CSR |  |  | RS. |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION

PART – B

NAME OF WORK :- CONSTRUCTION OF SURFACE DRAIN FOR UC- JUNAS & UC-NIRCH,

TALUKA PANO AKIL.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO | DESCRIPTION | QTY | RATE | UNIT | AMOUNT |
| 01 | Excavation in foundation of Building, Bridges & other structures i/c dag belling dressing, refilling around structure with excavated earth watering & ramming lead up to 5ft. (CSI-18 (b) P-04) | 375.0 | 3176.25 | %0 CFT | 1191.0 |
| 02 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:4:8 (CSI-05 (i) P-15 | 62.50 | 11288.75 | % CFT | 7055.0 |
| 03 | Erection & removal of centering for RCC or plain Cement Concrete works of Deodar wood ( 2nd Class) ii-Vertical. (CSI-19 (ii) P-18) | 375.0 | 3127.41 | % SFT | 11728.0 |
| 04 | Cement Concrete plain i/c placing compacting, finishing & curing / complete ( including screening & washing at stone aggregate without shuttering). Ratio: 1:2:4 (CSI-05 (f) P-16) | 175.0 | 14429.25 | % CFT | 25251.0 |
| 05 | R.C.C work in roof slab, beams columns rafts, lintels & other structural members laid in situ or precast laid in position complete in all respects, Ratio (1:2:4) 90 Lbs, cement 2Cft Sand 4 Cft. Shingle 1/8” to ¼” guage.(CSI-06 (i) P-16) | 15.84 | 337.0 | P. CFT | 5338.0 |
| 06 | Fabrication of Mild Steel reinforcement for cement concrete i/c cutting, bending, laying in position, making joints & fastening i/c cost of building wire (also i/c removal of) (b) Using Tor bars. (CSI-08 (b) P-17 | 0.636 | 5001.70 | P. CWT | 3181.0 |
|  |  |  | TOTAL | RS. | 53744.0 |
|  | Add Above/ Below on the rate of CSR |  | TOTAL | RS |  |
|  |  | GRANT | TOTAL | RS. |  |

RUPEES IN WORK\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACTOR’S EXECUTIVE ENGINEER

SIGNATURE RURAL DEVELOPMENT DEPARTMENT

SUKKUR DIVISION