**SCHEDULE B.**

Name of work:- **M/R to Secretary Bungalow No. 20, At GOR-1,Bath Island Karachi.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.NO.** | **DESCRAPTION OF ITEMS** | **QUTY** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | P/L fancy type porcelain floor & dadotiles24”x24”x3/8”thickasapproved size specified approved quality/make / design & color i/c laying with bond solution sand mortar i/c jointing with white cement/matching grouted i/c washing of tiles i/c cutting of tile to proper profile i/c all respect labor & required necessary material as directed by the Engineer In charge etc complete.(Imported make ) | 957.25 |  | P. Sft |  |
| 2 | P/F giralda one pe commode approved quality color design etc, complete. | 3-Nos |  | Each |  |
| 3 | P/F giralda seat cover approved quality etc, complete as directed by the E.I. | 3-nos |  | Each |  |
| 4 | P/F screw for vitorim approved quality etc, complete as directed by the E.I. | 3-nos |  | Each |  |
| 5 | P/F thimble S/s approved quality as directed by the E.I. etc, complete. | 3-nos |  | Each |  |
| 6 | P/F timber wash basin approved quality etc, complete as directed by the E.I. | 3-nos |  | Each |  |
| 7 | P/F euro cube basin mixture grohi approved quality as directed by the E.I. | 3-nos |  | Each |  |
| 8 | P/F double bib cock ½” dia plastic / powder coated master “A” class as directed by the E.I. | 3-nos |  | Each |  |
| 9 | P/F bath room min concealed body dial main w/diver approved quality etc, complete. | 3-nos |  | Each |  |
| 10 | P/F euro cube s/l exposed past w/diverter approved quality as directed by the E.I. | 3-nos |  | Each |  |
| 11 | P/F rain shower rod vintage approved quality etc, complete. | 3-nos |  | Each |  |
| 12 | P/F rain shower F. series approved quality as directed by the E.I. | 3-nos |  | Each |  |
| 13 | P/F euro cube bath spot approved quality color design etc, complete. | 3-nos |  | Each |  |
| 14 | P/F angle valve ½”x1/2” stop cock approved quality etc, complete. | 9-nos |  | Each |  |
| 15 | P/F stainless steel floor trap jalli imported make etc, complete. | 9-nos |  | Each |  |
| 16 | P/F viega bottle trap 1.25 cp approved quality & design etc, complete. | 3-nos |  | Each |  |
| 17 | P/F Bath Accessories imported make as approved quality etc complete. | 3-nos |  | Each |  |
| 18 | S/F Muslim shower with double bib cock approved quality etc complete (Imported make) | 3-nos |  | Each |  |
| 19 | P/F of looking mirror on wall Belgium mirror lass etc complete as directed by the Engineer in charge. | 3-Nos |  | Each |  |
| 20 | P/F vanity top of granite approved quality etc, complete. | 3-Nos |  | Each |  |
| 21 | P/F Glass potion of 8mm tamper for shower area with fitting arrangement of S.S. complete. | 3-Nos |  | Each |  |
| 22 | Providing and fixing CPVC pipe 1” dia pak arab of AGM make including cutting making and jointing with imported solution including necessary PVC fitting with approved quality including all cost of labour material cartage as directed by the engineer incharge etc complete | 246.00 |  | p. Rft |  |
| 23 | P/F elbow 1” 90 schd, 80(AGM) approved quality etc, complete. | 96.00 |  | Each |  |
| 24 | P/F Tee 1” sched, 80 (AGM) as approved quality etc, complete. | 14-nos |  | Each |  |
| 25 | P/F socket 1” schd, 80 (AGM) approved quality etc, complete. | 16-Nos |  | Each |  |
| 26 | P/F Upvc valve ball 1” dia approved quality etc, complete. | 4-Nos |  | Each |  |
| 27 | P/F bush 1”x3/4” schd 80 (AGM) approved quality etc, complete. | 8-Nos |  | Each |  |
| 28 | P/F cpvc cross over 1” dia approved quality as directed by the E.I. | 4-Nos |  | Each |  |
| 29 | P/F GI gass clip 1”(heavy duty imported) etc, complete | 120-Nos |  | Each |  |
| 30 | P/F cpvc pipe ¾” schd, 80 (AGM) approved quality etc, complete. | 158-Nos |  | p. Rft |  |
| 31 | P/f cpvc elbow ¾” 90” schd, 80 (AGM) approved quality etc, complete. | 48-Nos |  | Each |  |
| 32 | P/F cpvc Tee ¾” dia. Approved quality & design etc, complete. | 12-Nos |  | Each |  |
| 33 | P/F cpvc socket ¾” dia schd, 80(AGM) approved quality etc, complete. | 14-Nos |  | Each |  |
| 34 | P/F cpvc bush ¾”x1/2” schd, 80(AGM) approved quality etc, complete as directed by the E.I. | 10-Nos |  | Each |  |
| 35 | P/F upvc valve ball ¾” dia approved quality as directed by the E.I. | 2-Nos |  | Each |  |
| 36 | P/F GI gass clip ¾” (heavy duty imported) etc, complete as directed by the E.I. | 51-Nos |  | Each |  |
| 37 | P/F cpvc pipe ½” dia schd, 80(AGM) approved quality etc, complete as directed by the E.I. | 220.0 Rft |  | P. Rft |  |
| 38 | P/F cpvc ½” Elbow 90” schd, 80 (AGM) approved quality as directed by the E.I. | 48-Nos |  | Each |  |
| 39 | P/F cpvc ½”x1/2” brass thrd elbow (AGM) approved quality etc, complete. | 18-Nos |  | Each |  |
| 40 | P/F cpvc ½” dia Tee schd, 80 (AGM) approved quality etc, complete. | 36-Nos |  | Each |  |
| 41 | P/F cpvc ½” dia croos over schd, 80(AGM) approved quality as directed by the E.I. | 6-Nos |  | Each |  |
| 42 | P/F cpvc 1/2” socket schd, 80 (AGM) approved quality etc, complete. | 12-Nos |  | Each |  |
| 43 | P/F cpvc ½” x1/2” brass thrd tee approved quality etc, complete. | 3-Nos |  | Each |  |
| 44 | P/F cpvc ½” dia brass valve socket (AGM) approved quality etc, complete. | 14-Nos |  | Each |  |
| 45 | P/F cpvc ½” end cap schd, 80 (AGM) approved quality etc, complete as directed by the E.I. | 28-Nos |  | Each |  |
| 46 | P/F upvc pipe 1- ¼” schd, 40 (AGM) approved quality etc, complete. | 22.0 Rft |  | P. Rft |  |
| 47 | P/F upvc 1-1/4” 90 elbow schd, 40(AGM) approved quality etc, complete as directed by the E.I. | 3-Nos |  | Each |  |
| 48 | P/F upvc 1-1/4”x2” bush sehd, 40 (AGM) approved quality etc, complete. | 6-Nos |  | Each |  |
| 49 | P/F cpvc 3” pipe SDR 32.5(AGM) approved quality etc, complete. | 155.0 Rft |  | P. Rft |  |
| 50 | P/F upvc 3” dia socket shed, 40 (AGM) approved quality as directed by the E.I. | 3-Nos |  | Each |  |
| 51 | P/F upvc 3”x4” socket schd, 40 (AGM) approved quality etc, complete. | 5-Nos |  | Each |  |
| 52 | P/F upvc 3” wye schd, 40 (AGM) approved quality etc, complete. | 7-Nos |  | Each |  |
| 53 | P/F 3” 45 elbow sched, 40 (AGM) approved quality etc, complete. | 13-Nos |  | Each |  |
| 54 | P/F upvc 3” elbow 90 schd, 40 (AGM) approved quality etc, complete as directed by the E.I. | 12-Nos |  | Each |  |
| 55 | P/F upvc 3” dia P-trap schd, 40 (AGM) approved quality etc, complete. | 8-Nos |  | Each |  |
| 56 | P/F upvc 3”x2” floor trap w/o top tile (AGM) approved quality etc, complete. | 12-Nos |  | Each |  |
| 57 | P/F upvc 4” dia pipe SDR 41 (AGM) approved quality etc, complete. | 28.0 Rft |  | P. Rft |  |
| 58 | P/F upvc 4” dia elbow 90 sched, 40 (AGM) approved quality etc, complete as directed by the E.I. | 6-Nos |  | Each |  |
| 59 | P/F upvc 4” dia plug tee schd, 40 (AGM) approved quality etc, complete. | 3-Nos |  | Each |  |
| 60 | P/F upvc cleaner 237 ml (AGM) approved quality etc, complete as directed by the E.I. | 3-Nos |  | Each |  |
| 61 | P/F cpvc solvent 237 ml (AGM) approved quality etc, complete. | 14-Nos |  | Each |  |
| 62 | P/F upvc taflon tap (imported) approved quality etc, complete as directed by the E.I. | 18-Nos |  | Each |  |
| 63 | Making and fixing kitchen arrangement complete including cabinet, counter top (granite) kitchen accessories, fittings & appliances . | 1-job |  | P. job |  |
|  | **‘G’ Total Rs,** |  |  |  |  |

**TERMS AND CONDITION**

1. Any typographical errors in the schedule B are subject to the correction with

Reference to the Schedule of rate General 2012 enforced from 12.07.2012 as

Approved by the S R C, Sindh Karachi

1. Arbitration clause stands deleted from the agreement.
2. No premium shall be paid on a Non schedule items.
3. 100% WELL Graded crushed bajri shall be used in items of work without any

extra payment

1. No Any items of exvceed then the Quantity Provided in the Schedule B without

Prior of the Executive Engineer.

6. All sample of items should be got approved by the Executive Engineer.

CONTRACTOR ASSISTANT ENGINEER

PROVINCIAL BUILDINGS SUB DIVISION-I

KARACHI