|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R SINDH SECRETARIAT BUILDINGS NO.I (OFFICE OF THE SECRETARY (I&C) SGA&CD ROOM NO. 517, 5TH FLOOR (COLOURING, POLISHING, ALUMINUM WINDOW ).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | | **UNIT** | **AMOUNT** |
|  | **PART-“A” SCHEDULE ITEMS ( CIVIL WORK )** | |  | |  |  |
| **1.** | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 1608.00-Sft | 226/88 | | %Sft | 3648/- |
|  | Rupees. Two hundred twenty six. And. Eighty eight. Paisa | | | | | |
| **2.** | Distempering.( b ) Two coats.( SI.24(b) / P-54 ). | 665.00 Sft | 1043/90 | | %Sft | 6942/- |
|  | Rupees. One thousand & forty three. And. Ninety. Paisa | | | | | |
| **3.** | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 1608.00-Sft | 1772/38 | | %Sft | 28500/- |
|  | Rupees. One thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | | |
| **4.** | Removing window and sky light with Chowkats (33-b P/12). | 03-Nois | 102/85 | | P. No. | 309/- |
|  | Rupees. One hundred & two. And. Two. And. Eighty five. Paisa | | | | | |
| **5.** | French polishing complete. (b) On old work.( SI. 7(b)/P-71 ). | 282.00-Sft | 1952/50 | | %Sft | 5506/- |
|  | Rupees. One thousand nine hundred fifty two. And. Fifty. Paisa | | | | | |
| **6.** | Supplying & fixing in position Aluminum channels framing for sliding windows & ventilators of Alcop made with 5 mm thick tinted glass glazing ( Belgium ) & Aluminum fly screen in/c handles stoppers & locking arrangement etc. complete. ( b ) Deluxe model ( Bronze ).  ( SI.84-b / P-108 ) | 82.43-Sft | 1647/69 | | P.Sft | 135820/- |
|  | Rupees. One thousand six hundred forty seven. And. Sixty nine. Paisa | | | | | |
| **7.** | Providing and laying tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and apttern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing, clearing and cost of wax polish etc. complete including cutting tiles to proper profile.  ( SI.60/P-47 ). | 94.88-Sft | 30509/77 | | %Sft | 28948/- |
|  | Rupees. Thirty thousand five hundred & nine. And. Seventy seven. Paisa | | | | | |
|  |  |  | **Total Rs.** | | | **209673/-** |
|  | **Less % below on Item No. 6 & 7 Rs.** | | | | |  |
|  |  | **(A). Total Rs.** | | | |  |
|  | **PART ‘B’ WATER SUPPLY SANITARY.** |  |  | |  |  |
| **1.** | Supplying & fixing Bath room accessories set  ( 7-piece ) in/c towel rod, brush holder soaptray shelf of approved design in/c cost of screws, nuts etc complete.  ( Master Brand ). ( SI.23 / P-19 ). | 01-No | 10322/40 | | Each | 10322/- |
|  | Rupees. Ten thousand three hundred twenty two. And. Forty. Paisa | | | | | |
| **2.** | ( a ). S/Fixing canceled tee-stop cock of superior quality with C.P head ½” dia. ( SI.12-a / P-18 ). | 04-Nos | 843/92 | | Each | 3376/- |
|  | Rupees. Eight hundred forty three. And. Ninety two. Paisa | | | | | |
|  | **Total Rs.** | | | | | **13698/-** |
|  |  | | | | |  |
|  | **(B). Total Rs.** | | | | |  |
|  | **PART-“B” NON SCHEDULE ITEMS.** |  | |  |  |  |
| **1** | Making jambs of window of size 6” to 9” and repairing the surface by 1:4 cement plaster making edges, maintaining right angle in/c finishing curing etc complete & working upto height of 90’-0 using etc complete. | 65.00-Rft | |  | PRft |  |
| **2** | P/F Aluminum partition with fixed glass (frosted) 5mm thick using 4” lucky section in champion color as frame on floor or block masonry fixed with necessary fixtures rubber packings etc. The cost in/c tools & plants used in making and carriage from shop to site as directed by the Engineer Incharge. | 40.00-Sft | |  | PSft |  |
| **3** | P/F fine quality roller type blind with approved design false & in/c steel angle fixing with steel screws as per window as required @ site as directed by the Engineer Incharge. | 102.50 Sft | |  | P/Sft |  |
| **4** | P/F wooden cabinet with shutter and back shelves by using laminated lassani sheet 3/4" thick and frame work of 1st class partal wood 2”x1” with 18” deep box in/c providing & fixing wooden leaping or gola around lassani shutter or making gola by router in approved design & shape & polishing it. The cost in/c necessary hinges, catchers, handles, sliding wheels in draws, nails, screws, draws locks etc. The cost also in/c necessary tools and plants to be used in making etc complete as directed by the Engineer Incharge. | 25.84 Sft | |  | P/Sft |  |
| **5** | P/F marble top 1” thick (botesina or teravera or equivalent) having size upto 8’-0x2’-0 in/c cutting into proper size, making round gola & cutting for fixing vanity basin or sink bowl and filling joints with white cement or jelly in/c grinding and chemical polishing etc complete as directed by the Engineer Incharge. | 25.84-Sft | |  | PSft |  |
| **6** | P/F Double Bib Cock / Long Bib Cock 1/2” dia plastic coated A Class as directed by the Engineer Incharge. (Irfan Make) | 02-Nos | |  | Each |  |
| **7** | P/F exhaust fan 18” dia size plastic / metal body in/c making hole in wall to required size in/c cutting, chiseling, & making corner with cement sand mortar 1:4 (Pak/Millat/Royal) make in/c removing dismantled material from site to out side of premises in proper place as directed by the Engineer Incharge. | 01-No | |  | Each |  |
| **8** | P/F sanitary fitting chrome plated heavy gauge of approved quality (Master / Sonex make) fitted with completed accessories as directed by the Engineer Incharge. **Side pillar cock . ½” dia** | 01-No | |  | Each |  |
| **9** | P/F false ceiling spot light fancy type round shape with glass and 2 holder and energy saver of approved make & quality including fixing in false ceiling by cutting hole as directed by the Engineer Incharge. | 13-Nos | |  | Each |  |
| **10** | S/F TBS 2-40 / 36 watts TLW complete fancy tube light shade 4’-0 length with fancy cover light reflector sheet, 02 Nos rods, chocks, starters of approved quality base fitted on wall / ceiling in/c connected with 40/.076 flexible wire to existing ceiling rose as directed by the Engineer Incharge. (Phillips make) or equivalent. | 02-Nos | |  | Each |  |
| **11** | P/F door lock with triplicate key of approved make & quality as directed by the Engineer Incharge. | 08-Nos | |  | Each |  |
|  |  |  | | **(C). Total Rs.** | |  |
|  |  | **(B). Total Rs.** | | | |  |
|  |  |  | | **(A). Total Rs.** | |  |
|  |  | **G. Total ( A + B + C ) Rs:** | | | |  |
|  |  | **Say Rs.** | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |