|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO.II ( TUGHLAQ HOUSE ) KARACHI**  **( REPLACEMENT OF DAMAGED GI & UPVC PIPE & FITTINGS OVER ROOF & BATH ROOM DUCTS, REPAIR / REWINDING OF MOTORS PUMP ETC. )** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **NON-SCHEDULE ITEMS PART** |  |  |  |  |
| 1 | P/F GI pipe of IIL (L) or equivalent with fittings of TG or equivalent recessed in wall or columns in/c cutting pipe, the threading,, fixing and wrapping bitumen tape all around and making required No. of holes in wall, floor or plinth for pipe connection and making good in CC 1:2:4 as directed by Engineer Incharge., **1-1/2” dia pipe** | 302.00 Rft |  | P/Rft |  |
| 2 | Providing GI pipe with out fittings IIL (L) in/c cutting, fitting and threading also cost of breaking through walls or slab making good with 1:2:4 C.C. finishing with cement plaster etc. The cost also in/c wrapping plastic or bitumen tape fitted on surface testing with a pressure head of 200'-0 etc complete in all respect as directed by the Engineer Incharge.  **2" dia pipe** | 204.47 Rft. |  | P/Rft. |  |
| 3 | S/F GI fitting of approved quality & gauge fitted on existing pipe as directed by the Engineer Incharge |  |  |  |  |
| a. | **2" dia Tee** | 02 Nos |  | Each. |  |
| b. | **2" dia Elbow** | 09 Nos |  | Each |  |
| c. | **2" dia Nipple** | 30 Nos |  | Each. |  |
| 4 | P/F UPVC fittings valve socket 1” dia of approved quality make as directed by the Engineer Incharge. | 18 Nos |  | Each. |  |
| 5 | P/F ball l cock of approved quality make as directed by the Engineer Incharge. | 02 Nos |  | Each. |  |
| 6 | P/F UPVC water supply pipe of AGM or Pak Arab make schedule 40(E) ASTM standard D-1785 with all necessary fittings like elbow, bend, tee etc. This includes fixing on walls with clamps or Jubilee clips upto height of 50’-0 in vertical or horizontal position using Jhoola or long ladder or scaffolding and jointing pipe & fittings with approved solvent / JTG solution. The rate includes all cost of labour, material, and cartage, as directed by Engineer Incharge |  |  |  |  |
| a. | **1-1/4” dia.** | 127.00 Rft. |  | P/Rft. |  |
| b. | **1” dia.** | 80.00 Rft. |  | P/Rft |  |
| c. | **1/2” dia.** | 80.00 Rft. |  | P/Rft. |  |
| d. | **3/4” dia.** | 40.00 Rft. |  | P/Rft |  |
| 7 | Removing debries from Sindh Secretariat Buildings in/c collecting from different floors, throwing to stair to ground floor at proper place and then loading on truck and throwing out of city government premises, fuel & hire charges of truck, loading & unloading etc complete. | 04 Truck |  | P/Truck |  |
| 18 | Removing 2-HP motor pump and carryout side shop to repair motor P/f new bearing winding oil, greasing in/c all cost of labour material cartage etc complete. | 01 Nos |  | Each |  |
| 9 | S/F piston motor pump set (Bottle type) three phase 1450 RPM 440-volts with (Siemens motor & NICE pump) 2”x1-1/2” suction & delivery as directed by the Engineer Incharge | 02 No |  | Each. |  |
|  |  | **Total Rs.** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |