|  |  |
| --- | --- |
| **NAME OF WORK :-** | **M/R TO SINDH SECRETARIAT NO-I (FALSE CEILING WITH LIGHTS, FILE CABINETS, MATT FINISH COLOURING OF OFFICE OF FOCAL PERSON TO CHIEF-SECRETARY 2ND FLOOR** |

**“ SCHEDULE “B “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS (A** |  |  |  |  |
| 1. | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 2930.0-Sft | 226/88 | %Sft | 6648/- |
|  | Rupees (Two hundred twenty six & Ps. Eighty eight) only. | | | | |
| 2 | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 4185.0-Sft | 1772/38 | %Sft | 74174/- |
|  | Rupees (One thousand seven hundred seventy two & Ps. Eighty eight) only. | | | | |
| 3 | French polishing complete. (b) On old work. ( SI. 7(b)/P-71 ). | 486.0-Sft | 1952/50 | %Sft | 9489/- |
|  | Rupees (One thousand nine hundred fifty two & Ps. Fifty) only. | | | | |
| 4 | Distempering (b) Two cots. (SI.24-B/P-54) | 1435.0-Sft | 1043/90 | %Sft | 14980/- |
|  | Rupees (One thousand forty three & Ps. Ninety) only. | | | | |
| 5 | Providing and fixing approved quality mortice lock. ( SI.21 / P-60 ). | 05 Nos | 1786/13 | Each | 8930/- |
|  | Rupees (One thousand seven hundred eighty six & Ps. Thirteen) only. | | | | |
|  |  |  | **(A) Total** | | **114221/-** |
|  | **NON-SCHEDULE ITEMS (B)** |  |  |  |  |
| 1 | P/F false ceiling of Gypsum board panels of required design & size in/c frame work of aluminum T-Section hanged with nail wire to ceiling etc complete. | 355.0  Sft |  | P.Sft |  |
| 2 | P/F false ceiling spot light fancy type round shape with glass and 2 holder and energy saver of approved make & quality including fixing in false ceiling by cutting hole as directed by the Engineer Incharge. | 18 Nos |  | Each |  |
| 3 | P/F wooden cabinet / Almirah with shutter and back shelves by using laminated lassani sheet 3/4" thick and frame work of 1st class partal wood 2”x1” with 18” deep box in/c providing & fixing wooden leaping or gola around lassani shutter or making gola by router in approved design & shape & polishing it. The cost in/c necessary hinges, catchers, handles, sliding wheels in draws, nails, screws, draws locks etc. The cost also in/c necessary tools and plants to be used in making etc complete as directed by the Engineer Incharge. | 48.00  Sft |  | P.Sft |  |
| 4 | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 16’x16”x1/4”.** | 218.00Sft |  | P.Sft |  |
| 5 | Wiring for light point to point with 1.5 3/.029 PVC insulated wire in 3/4” PVC conduit recessed in wall columns as required. | 18 Nos |  | Each |  |
|  |  |  | **(B). Total** | |  |
|  |  |  | **(A) Total** | |  |
|  |  | **G. Total ( A + B ) Rs.** | | |  |
|  |  | **Say** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate (Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-I,**  **KARACHI.** |