|  |  |
| --- | --- |
| **NAME OF WORK :-** | **M/R TO SINDH SECRETARIAT NO. VI (OLD STATE BANK) OFFICE OF THE PUBLIC SERVICE COMMISSION & OTHER OFFICES (FLOOR TILES, RENOVATION OF KITCHEN).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS** |  |  |  |  |
| 1 | Providing and laying tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and apttern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slaurry of white cement and pigment in desired shape with finishing, clearing and cost of wax polish etc. complete including cutting tiles to proper profile. ( SI.60/P-47 ). | 282.00-Sft | 30509/77 | %Sft | 86038/- |
|  | Rupees. Thirty thousand five hundred & nine. And. Seventy seven. Paisa | | | | |
| 2 | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 733.00-Sft | 226/88 | %Sft | 1663/- |
|  | Rupees. Two hundred twenty six. And. Eighty eight. Paisa | | | | |
| 3 | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 1047.00-Sft | 1772/38 | %Sft | 18557/- |
|  | Rupees. One thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | |
|  |  |  | **(A). Total** | |  |
|  | **Above / Below Rs.** | | | |  |
|  |  |  |  | |  |
|  | **NON-SCHEDULE ITEMS** |  |  |  |  |
| 1 | P/L Porcelain tiles glazed or matt glazed Master or equivalent jointed in white cement and laid over 1:2 grey cement sand mortar ¾” thick in/c finishing & filling of joints with slurry of white cement or tile grout in desired shape in/c cutting of tiles to proper profile (on floor or facing) **size 16”x16”x1/4”** | 715.0 Sft |  | P.Sft |  |
| 2 | P/F Gypsum board pelmet to be hanged from ceiling in specified shape and design as approved by the consultant. This in/c cutting the existing Gypsum board false ceiling in proper shape, hanging the structure by aluminum angle 1’x1” @ 3’-0 apart drilled and screwed in RCC slab, making hanging frame by using aluminum U-channel section 1-1/2” wide in 18”x18” rafters and fixing Gypsum board sheet with plastic mesh and plaster of paris and making surface smooth as directed by the Engineer incharge. | 652.00-Sft |  | PSft |  |
|  |  | **(B). Total** | | |  |
|  |  | **(A). Total** | | |  |
|  |  | **G. Total (A+B) Rs:** | | |  |
|  |  | **Say** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |