|  |  |  |
| --- | --- | --- |
| **NAME OF WORK:** | **M/R TO SINDH SECRETARIAT NO.III OLD K.D.A BUILDING KARACHI BACKSIDE P/LAYING DRANAGE LINE, PAVING BLOCKS & MISC: WORKS.** |  |

**“SCHEDULE “B“**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEM** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS (A)** |  |  |  |  |
| 1 | Dismantling cement block masonry. ( SI.14 / P-10 ). | 75.07 Sft | 1134/38 | %Sft | 852/- |
|  | Rupees (One thousand one hundred thirty four & Ps. Thirty eight) only. | | | | |
| 2 | Providing and laying 1: 3: 6 cement concrete solid block masonry wall 6” and below in thickness set in 1:6 cement mortar in ground floor Super Structure including raking out joints & curing etc, complete.( SI.24 / P-19 ). | 28.74 Sft | 15771/01 | % Cft | 4533/- |
|  | Rupees (Fifteen thousand seven hundred seventy one & Ps one ) only. | | | | |
| 3 | Cement Plaster 1:5 upto 12’ height.( a ) 3/8” thick ( SI.12-a / P-52 ). | 132.44 Sft | 2166/72 | %Sft | 2870/- |
|  | Rupees (Twenty one thousand sixty six & Ps. Seventy two ) only. | | | | |
| 4 | Providing & fixing cement paving blocks flooring having size of 197x97x60 (mm) of city / Quadra / cobble shape with natural colors, having strength b/w 5000 psi to 8500 psi Including filling the joints with hill sand and laying in specified manner / pattern and design etc complete.(SI.71 / P-49 ). | 1504.52 Sft | 199/77 | P.Sft | 300558/- |
|  | Rupees (One hundred ninety nine & Ps. Seventy seven) only. | | | | |
| 5 | Making & fixing steel grated door with 1/16” thick sheeting including angle iron frame 2”x2” 3/8” and ¾” square bars 4” centre to centre with locking arrangement.( SI.24 / P-92 ). | 17.08-Sft | 726/72 | P.Sft | 12412/- |
|  | Rupees (Seven hundred twenty six & Ps. Seventy two) only. | | | | |
|  |  | **Total** | | | **321225/-** |
|  | **Above / Below Rs:** | | | |  |
|  |  |  | | |  |
|  |  | **Total Rs. A** | | |  |
|  | **NON-SCHEDULE ITEMS** |  |  |  |  |
| 1 | P/M Graffito paint to wall surface to provide durable & aesthetic surface having thickness between 1.6 – 2.0mm in specified color / shade & working up to height of 90-0’ using scaffolding as directed by the Engineer Incharge. | 1196.28 P.Sft |  | P.Sft |  |
| 2 | Removing debries from Sindh Secretariat Buildings in/c collecting from different floors, throwing to stair to ground floor at proper place and then loading on truck and throwing out of city government premises, fuel & hire charges of truck, loading & unloading etc complete. | 13 Nos |  | P.Truck |  |
| 3 | P/F RCC pipe 12” dia with collar of class \*B\* for sewerage line in/c excavating the trench of required dia and depth and then laying pipe in trench jointing and refilling excavated stuff as directed by the Engineer Incharge. | 144.00 Rft |  | P.Rft |  |
| 4 | P/F RCC pipe 6” dia with collar of class \*B\* for sewerage line in/c excavating the trench of required dia and depth and then laying pipe in trench jointing and refilling excavated stuff as directed by the Engineer Incharge. | 19.50-Rft |  | P.Rft |  |
| 5 | Construction of manhole or inspection chamber 2’-0x2’-0 & upto 3’-0” inside dimension for required dia of circular sewer with walls of solid block masonry 1:3:6 set in 1:6 cement sand mortar 6” thick with 6” thick C.C. 1:4:8 in foundation, ½” thick plaster in 1:4 ratio to all inside wall surface & to top 1” thick C.C. flooring etc including, curing, excavation, back filling & disposal of surplus earth as directed by the Engineer Incharge. size 2’-0x2’-0x2’-0 to 3’-0 | 01-No |  | Each |  |
| 6 | P/F RCC main hole cover of 3” thickness embedded with angle iron frame 1-1/2”x1-1/2”x1-1/4” and bars of 3/8” dia mild steel placed at 6” i/c both way i/c handle in centre for lifting poured with C.C. 1:2:4 in/c curing, finishing etc complete. | 8.00-Sft |  | PSft |  |
|  | **Total Rs. (B)** | | | |  |
|  | **G. Total (A) (+) (B) Total Rs.** | | | |  |
|  | **Say RS.** | | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

**CONTRACTOR.**

|  |  |
| --- | --- |
| **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |