***BIDDING DATA***

***Work No:* Tender No.(6)/ (2015-2016)**

(This section should be filled by the Engineer/Procuring Agency before issuance of the Bidding Documents).

**(a).Name of Procuring Agency** Deputy Commissioner, District Central-Karachi

**(b).Brief Description of Works** Improvement / Repair (Beautification) of Foot Paths / Central Island in the area of District Central Karachi.

**(c).Procuring Agency’s address:-** Near Sakhi Hassan, North Nazimabad Karachi

**(d).Estimated Cost:- ­­­­­­­­­­­­­­­­­­­­­­­­\_\_**10.000**\_**Million**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**(e).Amount of Bid Security:-** Rs.4,00,000/- \_(Fill in lump sum amount or in % age of bid amount/estimated cost, but not exceeding 5%

**(f).Period of Bid Validity (days):- \_\_\_\_\_\_\_\_**90 Days\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(g).Security Deposit :-( including bid security):-** \_\_\_\_\_\_\_\_10%\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(in % age of bid amount/estimated cost equal to 10%)

**(h).Percentage, if any, tobe deducted from bills:-** 7.5% Income Tax for filer\_\_\_\_\_\_\_\_\_\_\_\_

**(i).Deadline for Submission of Bids along with time:-** Dated: 01-06-2016\_2:00 PM\_\_

**(j).Venue, Time, and Date of Bid Opening:-** Office of the Deputy Commissioner, Karachi-Central Near Sakhi Hassan, North Nazimabad Karachi. At 3:00 PM Dated:-\_01-06-2016

**(k).Time for Completion from written order of commence:-** 40 Days\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(l).Liquidity damages:-\_\_\_\_\_\_**0.10%**\_\_\_\_\_\_\_\_**0.05 of Estimated Cost of Bid cost per day of delay, but total not exceeding 10%).

**(m)Tender Cost Receipt Pay Order No:\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_Amount:\_\_\_\_\_\_\_**

**(n).Deposit Receipt Pay Order No:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_Amount:\_\_\_\_\_\_\_**

Name of Bank\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**(o).Bidding Documents issued to:M/s.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**ISSUING AUTHORITY**

**DISTRICT MUNICIPAL CORPORATION (CENTRAL) KARACHI**

**BILL OF QUANTITIES**

NAME OF WORK:- Improvement / Repair (Beautification) of Foot Paths / Central Island in the area of District Central Karachi.

**Tender No.(6)/ (2015-2016)**

**(PART-A: ITEM BASED ON SCHEDULE RATE)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **Description of Item** | **Qty** | **Rate** | **Unit** | **Amount** |
|  | **DISMANTLING CEMENT CONCRETE PLAIN 1:2:4**  **PG10 / 19 C** | **1500 CFT** | **3327.50** | **% CFT** | **49912 /=** |
|  | **EXCAVATION IN FOUNDATION OF BUILDING BRIDGES AND OTHER STRUCTURES I/C DABELLING DRESSING REFILLING ROUND STRUCTURE WITH EXCAVATED EARH WATERING AND RAMMING LEAD UP TO 05’ PG 04/18 (b),** | **1875 CFT** | **3176.25** | **%0 CFT** | **5955/=** |
|  | **CEMENT CONCRETE BRICK STONE OR STONE BALLAST 1 ½ “ TO 2” 1:4:8 PG 15/04** | **825 CFT** | **9416.28** | **% CFT** | **77684 /=** |
|  | **CEMENT CONCRETE PLAIN I/C PLACING COMPACTING FINISHING AND QUEERING CONCRETE (I/C SCREENING AND WASHING AND STONE AGGREGATE WITHOUT SHUTTERING) 1:2:4. PG16/05 F** | **3112 CFT** | **14429.25** | **% CFT** | **449038 /=** |
|  | **CEMENT CONCRETE PLAIN I/C PLACING COMPACTING FINISHING AND QUEERING CONCRETE (I/C SCREENING AND WASHING AND STONE AGGREGATE WITHOUT SHUTTERING) 1:3:6. PG16/05 H** | **1875 CFT** | **12595.00** | **% CFT** | **236156 /=** |
|  | **ERRECTION AND REMOVAL OF CENTERING FOR RCC OR PLAIN CC WORK FOR PARTAL WOOD PG 18/19 B.** | **7500 SFT** | **3588.48** | **% SFT** | **269136/=** |
|  | **CE,EMT PLASTER 1:4 UP TO 12’ FOOT HIEGHT ½ “ THICK PG 52/11 (b).** | **7075 SFT** | **2283.93** | **% SFT** | **161588 /=** |
|  | **CEMENT CONCRETE PLAIN I/C PLACING COMPACTING FINISHING AND QUEERING CONCRETE (I/C SCREENING AND WASHING AND STONE AGGREGATE WITHOUT SHUTTERING) 1:4:8. PG16/05 I** | **3125 CFT** | **11288.75** | **% CFT** | **352773 /=** |
|  | **P/L 2” THICK TOPPING CEMENT CONCRETE 1:2:4 I/C SURFACE FINISHING AND DIVIDING IN TO PANELS PG-42/16 (C).** | **8500 SFT** | **3275.50** | **% SFT** | **278417/=** |
|  | **PROVIDING AND LAYING COLOURED CEMENT TILES (PATTERN) 12”X12”X01” OF APPROVED SHADE AND PATTERN LAID FLAT IN 1:2 GREY CEMENT MORTOR OVER A BED OF ¾ “ THICK GREY CEMENT MORTOR 1:2 PG -47/59.** | **18550 SFT** | **9427.84** | **% SFT** | **1748864/=** |
|  | **P/F CEMENT PAVING BLOCKS FLOORING HAVING SIZE OF 197X197X60 (mm) OF CITY / QUDDRA / COBBEL SHAPE WITH NATURAL COLOUR, HAVING STRENGTH B/W 5000 PSI TO 8500 PSI I/C FILLING THE JOINTS WITH HILL SAND AND LAYING IN SPECIFIED MANNER /PATTERN AND DESIGN ETC COMPLETE PG 59/71.** | **13578 SFT** | **199.77** | **P.SFT** | **2712477/=** |
|  | **PAINTING WITH ENAMEL PAINT ON MASONRY WALL**  **2ND AND SUBSEQUENT COAT PG 73/30 (A,B).** | **39000 SFT** | **837.10+**  **584.65**  **1421.75** | **% SFT**  **% SFT**  **% SFT** | **554482/=** |
|  | **SCRAPPING RUST FROM OLD RAIL OR GIRDERS PG72/24** | **15050 SFT** | **473.75** | **% SFT** | **71299 /=** |
|  | **PREPARING SURFACE AND PAINTING GUARD BARS, GETS OF IRON BARS , GRATTING , RAILNGS (I/C STANDARD BRACES ETC END SIMILAR OPEN WORK) PG 69/5 (D12).**  **PRIMING COAT.**  **EACH SUBSEQUENT COAT OF PAINT.** | **15050 SFT** | **521.95**  **374.44**  **896.39** | **% SFT** | **134907/=** |
|  | **PREPARING SURFACE AND PAINTING GUARD BARS, GETS OF IRON BARS , GRATTING , RAILNGS (I/C STANDARD BRACES ETC END SIMILAR OPEN WORK) PG 68/4 (D).**  **FIRST COAT.**  **EACH SUBSEQUENT COAT OF PAINT** | **17500 SFT** | **371.80**  **302.80**  **674.60** | **% SFT** | **118055** |
|  | **WHITE WASHING**  **TWO COATS PG54/26 (b)** | **30000 SFT** | **425.84** | **% SFT** | **127752 /=** |
|  | **COLOUR WASHING**  **TWO COATS PG 54/25 (B)** | **15000 SFT** | **859.90** | **% SFT** | **128985 /=** |
|  | **CARTAGE OF % CFT 5 TONS ALL MATERIALS LIKE STONE AGGREGATE SPAWL COAL LIME SURKHI EARTH ETC COMPLETE 7 MILES LEAD.** | **3375 CFT** | **804.52** | **% CFT** | **27153 /=** |
|  | **TOTAL COST OF SCHEDULE ITEMS RS:-** | | | | **7504633/-** |

NAME OF WORK:- Improvement / Repair (Beautification) of Foot Paths / Central Island in the area of District Central Karachi.

**Tender No.(6)/ (2015-2016)**

**(PART-B: ITEM BASED ON NON SCHEDULE ITEM APPROVED RATE)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SR#** | **Description of Item** | **Qty** | **Rate** | **Unit** | **Amount** |
|  | **P/L DRY STONE METAL WITH COMPACTION UNDER FLOOR I/C CRUSH STONE DUST.** | **8500 SFT** | **16.00** | **P.SFT** | **136000/=** |
|  | **P/F PRECAST KERB BLOCK 3750 PSI MADE SIZE 06”THICK 12” LONG 18” HIEGHT I/C THE COST OF EXCAVATION, 1:3:6 LEAN I/C CARTAGE RACKING OUT JOINTS 1:4 CEMENT SAND MORTOR.** | **3000 RFT** | **220.00** | **P.RFT** | **660000/=**  **796000/=** |
|  | **PROVIDING FIXING DIFFERENT TYPES OF PLANTS I/C THE COST OF 1” THICK DIA WOODEN STICK AS PER DIRECTED BY THE ENGINEER INCHARGE.**   1. **PALM PLANT 5’FT HEIGHT** 2. **LIGNUM PLANTS 5’FT HEIGHT** 3. **U FORBIA PLANT 1-1/2 FT HEIGHT** 4. **FEYCUS PLANT 5’ FT HEIGHT** 5. **BUGAN BELA PLANT 4’FT HEIGHT** 6. **KANGI PALM PALNT ( 12 LEAFS)** | **25.NOS**  **25.NOS**  **25.NOS**  **25.NOS**  **25.NOS**  **25.NOS** | **1300/-**  **1600/-**  **700/-**  **1300/-**  **1200/-**  **5000/-** | **EACH**  **EACH**  **EACH**  **EACH**  **EACH**  **EACH** | **32500/-**  **40000/-**  **17500/-**  **32500/-**  **30000/-**  **125000/-** |
|  | **PROVIDING FIXING RCC POTS SIZE 30”X 24”X02” THICK I/C THE COST OF LOADING AND UNLOADING AND COLORING AND ERRECTING I/C FORM WORK DISTRICT CENTRAL KARACHI AS PER DIRECTED BY THE EINGINEER INCHARGE** | **05 NOS** | **10000.00** | **EACH** | **50000/-** |
|  | **PROVIDING FIXING RCC POTS SIZE 36” X 10” X 12” 2” THICK I/C THE COST OF LOADING UNLOADING COLORING AND ERRECTING I/C FORM WORK DISTRICT CENTRAL KARACHI AS PER DIRECTED BY THE ENGINEER INCHARGE.** | **12 nos** | **1800.00** | **EACH** | **21600/-** |
|  | **SUPPLYING / STACKING AND SPREEADING GARDEN SOIL (SWEET EARTH) FREE FROM SALTS AND PEBBLES AND GRASS ROOT I/C THE COST OF LOADING UNLOADING AND LEAD UPTO 10 MILES.** | **900 CFT** | **25.00** | **P.CFT** | **22500/-** |
|  | **SUPPLYING STACKING ANDN SPREADING COWDUNG MANURE FROM APPROVED SOURCE I/C THE COST OF LOADING UNLOADING AND LEAD UPTO 10 MILES./** | **225.CFT** | **28.00** | **P.CFT** | **4050/-** |
|  | **TOTAL COST OF NON SCHEDULE ITEMS RS:-** | | | | **1171650/-** |

Nomenclature quantities and

Rates have been checked by us

ASSTT:EX:ENGINEER EXECUTIVE ENGINEER

DMC (CENTRAL) DMC(CENTRAL)

NAME OF WORK:- Improvement / Repair (Beautification) of Foot Paths / Central Island in the area of District Central Karachi.

**Tender No.(6)/ (2015-2016)**

**QUOTED BID SUMMERY**

I/We hereby quoted as follows.

|  |  |  |  |
| --- | --- | --- | --- |
|  | | **In Figures** | **In Words** |
| 1. | PART-A (Item Based on S/R) amounting Rs **7504633/-** \_\_\_\_\_\_\_\_%Above/Below of the S/R | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |
| 2. | PART-**B** (Item Based on Non S/I Approved Rate) amounting Rs. **1171650/-** \_\_\_\_\_\_\_\_%Above/Below of the A/R | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |
| 3. | **GRAND TOTAL (A+B)** | Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_ |  |

**NOTE:**

* Tender must be quoted in figure & in work both otherwise liable to be cancelled.
* All over writing & correction if any must be initialed & stamped by the bidder.
* I / We read the Standard Bidding Documents available in SPPRA website ([www.pprasindh.govt.pk](http://www.pprasindh.govt.pk)) and agreed to abide all of them and also provide all these documents with our signatures as & when directed.

Signature of the Contractor

with Stamp\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_