Peoples University

of Medical & Health Sciences for women

Nawabshah, Shaheed Benazirabad, Sindh, Pakistan

**Phone: 0244-9370427, Fax No: 0244-9370263**

**Web:** [**www.pumhs.edu.pk**](http://www.pumhs.edu.pk) **Email:** [**pd@pumhs.edu.pk**](mailto:pd@pumhs.edu.pk)

**TENDER ENQUIRY NO.PUMHSW/P.D/2016/ 2416 DATED: 28th -November -2016**



**FINANCIAL PROPOSALS (PACKAGE-A)**

**FURNITURE ITEMS FOR PHARMACEUTICAL INSTITUTE AND PUBLIC HEALTH INSTITUTE AT NEW CAMPUS OF PUMHSW**

**SUPPLY OF FURNITURE & FIXTURE**

**FOR THE YEAR 2016-2017**

**DATE OF SUBMISSION & OPENING**

**MONDAY 19th DECEMBER, 2016**

TIME OF RECEIVING TENDER 01:30 P.M

TIME OF OPENING TENDER 02:30 P.M

TENDER FEE Rs. 2,000/- (Non-Refundable)

**TERMS & CONDITIONS**

**SUPPLY OF FURNITURE & FIXTURE**

**FOR THE YEAR 2016-2017**

1. Supplier will have to provide **call deposit @ 2% of bid amount** in the favor of the **Vice Chancellor Peoples University of Medical & Health Sciences for Women Shaheed Benazirabad**, in case of failure the tender document will not be entertained
2. Quantity at any time can be increased / decreased or can deleted at any time.
3. The Supplier will have to produce evidence in respect of their registration with income tax and sales tax department.
4. The original brochure /catalogue must accompany with offer.
5. The bid shall comprise a single stage one envelope procedure. The envelope marked as “FINANCIAL PROPOSAL” and mentioned clearly address of the Bidder / Supplier
6. In case of failure on the part of Supplier to Supply as per specification or within the stipulated time without getting extension, penalty of 3% of the supply order per month or part thereof up to maximum limit of 10% will be imposed on the supplier.
7. The Successful bidders will be bound to carry out job according to specification provided in the BOQ with in specified time given in the supply order, failing which his earnest money shall be forfeited. The successful bidder has to furnish such undertaking in writing on the stamp paper of Rs: 100/-
8. The rates should be given inclusive of GST, Income Tax & any other government duty.
9. Income tax, G.S.T, Stamp duty & other applicable taxes and duties at the government prescribed rates are deductible from the bill.
10. The item(s) which is/are exempted from GST, the rates for the same must be quoted accordingly, stating clearly in BOQ, the cost of all those item(s) excluding G.S.T at the time of payment, no claim for GST shall be paid.
11. All those Suppliers who have been blacklisted by any Government Department, their bids shall not be entertained.
12. Suppliers must produce eligibility as per SPPRA rules. In case of non-production of eligibility tender forms will not be issued.
13. Conditional tenders will not be accepted.
14. Payment will be made on availability of funds, if delayed due to any reason; no extra interest / mark-up will be accepted / paid.
15. Rejected consignment shall be returned back to dealers / suppliers at their own cost.
16. An amount equivalent to 10 % of security deposit shall be withheld from the bills which will be refunded on satisfactory completion of the job, as per Clause-12 of General Conditions of the Contract of this bidding document.
17. The bid validity period shall be for 90 days after opening of tender.
18. Bid money to unsuccessful bidder shall be refunded after one week of tender opening on receipt of application on official letter pad.

**GENERAL CONDITIONS OF THE CONTRACT**

**CLAUSE 1. INSTRUCTIONS TO THE BIDDERS**

1. The tenders shall be submitted with all documents and drawing literature & catalogue (in furniture & fixture) in sealed envelopes with sealing wax / gum. The envelope must contained tender enquiry No. on the top. The name of manufacturer and the supplier should be affixed on the face of envelope at the left side.
2. Tenders must be filled in with blue or black ink in the columns provided in BOQ documents duly signed.
3. The tenders must be free from erasing cutting and over writing. In case of erasing, cutting and over writing, authorized person should initial it.
4. The rates of each item should be written in figures as well as in words. In case of discrepancy the price in works will be taken as authenticate and final.
5. Conditional Tenders will be ignored and will not be considered/entertained/accepted.
6. Original purchase receipt of tender fee or in shape of Pay order / DD original as tender form fee in favour of V.C PUMHS must be enclose with the tender form.
7. The tendered rate should be inclusive of all taxes, Income & Sales Tax etc payable to Federal & Provincial Govt or Local bodies and no claims on this account shall be entertained.
8. The bidder shall furnish General sales tax (GST) Registration Certificate of the firm failing which the offer will be ignored. In case the item is exempted from GST either documentary evident or certificate from competent authority shall be attached with the offer.
9. The bidder shall furnish copy of valid professional Tax (Excise & Taxation)Certificate
10. List of similar assignments with cost under-taken over the past (05) years.

**CLAUSE 2. SPECIAL CONDITIONS:**

1. Store is required immediately. The tenders may, however, give their short guaranteed delivery period by which the supply will be completed positively.
2. Tenders are required to specify make, country of origin and furnish detailed technical Description literature / catalogue along with their offer.
3. The Bidders shall quote their firm and final price both in figures & words on “Free Delivery basis to Consignee end
4. Tenderer shall submit guarantee letter that the supplied Furniture are the original / brand new product / latest model none of the part is replaced, old or refurbished.
5. No manufacturer shall authorize their distributor/agent/any firm or person to quote the same item which manufacturer is quoting it in any tender. Failing that offers of both the manufacturer, which the manufacturer as well as other bidder shall be ignored.
6. Tenderer shall purchase separate tender document furnish purchases receipts for each alternate offer in case they want to submit alternate offer for any items. All the bids with alternate offer without separate purchases receipt (original) are supposed to be rejected. Also, choice to select/ignore any their alternate offer shall rest with the purchase committee
7. The bidder shall confirm the refund of cost difference if the same goods is/was supplied at lower rates to any other Govt./Semi Government institution or Armed Forces in the province or outside in the same fiscal year.
8. The successful supplier / bidder must be bound to supply the awarded items mentioned dated supply orders on the quoted rates.

**CLAUSE: 3. PURCHASER’S RIGHT TO VARY QUANTITIES.**

The Purchase Committee reserves the right to increase/decrease or delete the quantities of any items at the time of award of contract and also reserves the right to enhance the quantities of goods/service originally specified in the Schedule of Requirement without any change in unit price or other terms and conditions of goods at any time during contract period.

**CLAUSE: 4. PURCHASERS RIGHT TO ACCEPT ANY BID AND TO REJECT ANY OR ALL BIDS:**

The Purchase Committee reserves the right to accept or reject any bid in accordance with the provision provided in SPPRA rules and to annual the bidding process and rejects all bids at any time prior to contract award without thereby incurring any liability to the affected bidder or bidders, on the grounds for the Purchaser’s action.

**CLAUSE 5. ELIGIBLE BIDDERS**

This Invitation for Bids is open to all original Manufacturers, within Pakistan and abroad, and their Authorized Agents/Importers/Suppliers subject to the conditions that:

1. In the case of foreign Manufacturers, they shall offer the product Certified by the ISO-CE-FDA;
2. Original technical broacher is mandatory

The Agents/Suppliers/Importers must possess valid authorization from the Manufacturer. In case of Manufacturers, they should have documentary proof to the effect that they are the original Manufacturers of the required specifications.

Bidders shall not be under a declaration of ineligibility for corrupt and fraudulent practices issued by any Government (Federal or Provincial), a local body or a public sector organization.

The bidders should have operational office(s) in Pakistan and possess financial sustainability to meet timely supply of items.

**CLAUSE 6. CRITERIA FOR EVALUATION OF BIDS.**

1. Registration with income tax & sales tax departments
2. Earnest money
3. Quoted prices.
4. Operational cost
5. Specification compliance.
6. Submission of catalogue,
7. Original brochure of product
8. Past performance of manufacturer/sole distributor in terms of supply and after sale service.
9. Delivery schedule

**CLAUSE: 7. NOTIFICATION OF AWARD**

1. Prior to the expiration of the period of bid validity, the Purchaser will notify the successful bidder in writing about the acceptance of the offer delivery by hand or by registered letter, to confirmed in writing that the bid has been accepted.
2. The notification of award will constitute the formation of the contract.

**CLAUSE: 8. AWARD OF CONTRACT & CONTRACT AGREEMENT.**

Subject to the fulfillment of all formalities, the Purchaser will award the contract the successful Bidder whose bid has been determined to be qualified to perform the contract satisfactory.

**CLAUSE: 9. PAYMENTS.**

**(A) Interim/Running Bill.**

The competent authority of procuring agency shall pass/certify the amount to be paid to the contractor, which he considers due and payable in respect thereof, subject to deduction of security deposit, advance payment if any made to him and taxes. All such intermediate payment shall be regarded as payments by way of advance against the final payment only and not as payments for supply actually done and completed, and shall not preclude the competent authority from recoveries from final bill and rectification of defects and unsatisfactory items of works pointed out to him during defect liability period.

**(B) The Final Bill.**

A bill shall be submitted by the contractor within one month of the date fixed for the completion of the work otherwise Purchase & Store Officer’s certificate of the total amount payable for the supply shall be final and binding on all parties.

**CLAUSE 10**. **PERFORMANCE SECURITY**

An amount equivalent to 10 % of security deposit shall be withheld from the bills of the successful tenderers / bidders which will be refunded on satisfactory completion of the job, as per clause 12 of general conditions of the contract of this bidding document.

**CLAUSE: 11. REDUCED RATES**

In cases where the items of supply are not accepted as so completed, the competent authority may make payment on account of such items at such reduced rates as he may consider reasonable in the preparation of final or on running account bills with reasons recorded in writing.

**CLAUSE: 12. REFUND OF SECURITY DEPOSIT / PERFORMANCE SECURITY.**

On completion of the whole of the works (a work should be considered as complete for the purpose of refund of security deposit to a contractor from the last date on which its final supplies and installation has been made by a competent authority, the defects notice period has also passed and the competent authority has certified that all defects notified to the contractor before the end of this period have been corrected, the security deposit lodged by a contractor (in cash or recovered in installments from his bills) shall be refunded to him after the expiry of three months from the date on which the supplies & installation are completed.

**CLAUSE: 13. UNDERTAKING:**

* That I/We agree whether our tender accepted for total, partial or enhanced quantity for all or any single item. I/We also agreed to supply and accept the said item at the rates for the supply of contracted quantity within the stipulated period shown in the contract.
* I/We understand and confirm the refund of cost difference if the same goods is/was supplied at lower rates to any other Govt/Semi Govt: Institution, Armed Forces, in the province in the same fiscal year.
* I/We undertake that, if any of the information submitted in accordance to this tender enquiry found incorrect, our contract may be cancelled at any stage on our cost and risk.

|  |  |
| --- | --- |
| **Contractor**  Sign with stamp | **Engr. Dur Muhammad Mangi**  Project Director  PUMHSW, Shaheed Benazirabad |

**TENDER FORM**

**SUPPLY OF FURNITURE & FIXTURE’S**

**FINANCIAL YEAR 2015-2016**

(BILL OF QUANTITY) B.O.Q

(Such quantity can be Reduced / Increased at any time)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **FURNITURE ITEMS FOR PHARMACEUTICAL INSTITUTE AND PUBLIC HEALTH INSTITUTE AT NEW CAMPUS OF PUMHSW** | | | | | | | |
| **B.O.Q (Non-Scheduled Items)** | | | | | | | |
| **S NO** | **TYPE** | **DESCRIPTION** | **UNIT** | **QTY** | **RATES** | **RATE IN WORDS** | **AMOUNT** |
| **A** | **FURNITURE FOR THE OFFICE OF PROFESSOR / CHAIRMAN** | |  |  |  |  |  |
| 1 | **ET-1** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 6'-0" X 3'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK OAK VINEER BOARD 700 DENSITY WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 2 | **CH-1** | PROVIDING AND MAKING REVOLVING CHAIR HIGH BACK, WITH WOODEN ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 3 | **CH-7** | PROVIDING AND MAKING EXECUTIVE VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 3 |  |  |  |
| 4 | **BS-2** | PROVIDING AND MAKING EXECUTIVE BOOK SHELF OF SIZE 6'-0" X 6'-6" HAVING TWO PORTION, BOTTOM PORTION HAVING 4 NOS PARTITIONS, BACK AND OPEN ABLE SHUTTERS MADE OF 3/4'' THICK AND 1'' THICK OAK VINEER BOARD 700 DENSITY ON TOP WITH OAK WOOD LIPPING ON ALL EDGES, UPPER PORTION 15'' DEEP, HAVING 4 NOS PARTITIONS AND 3 NOS SHELVES AND BACK ALSO MADE OF 3/4'' THICK CHIP BOARD AND LIPPING WITH OAK WOOD, 1'' THICK GLAZED OPEN ABLE SHUTTERS MADE OF 5MM THICK GLASS PLAIN LOCALLY MADE FIXED IN OAK WOOD FARMING ALL OAK WOOD POLISHED, ALL FITTING LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 5 | **ES-1** | PROVIDING AND MAKING EXECUTIVE SOFA SINGLE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 6 | **ES-3** | PROVIDING AND MAKING EXECUTIVE SOFA THREE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 7 | **CST-1** | PROVIDING AND MAKING CENTER AND SIDE TABLE SET OF SIZE 4'-0" X 2'-0" X 18" HIGH, AND 18" X 18" X 18" HIGH, MADE OF SHESHAM WOOD FRAME AND LEGS INCLUDING 8MM THICK TINTED GLASS FIXED IN 1 1/2'' X 3'' SHESHAM WOOD TOP FINISHED WITH SPRIT POLISH AND ALL SHESHAM COMPLETELY SEASONED AND TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SET | 1 |  |  |  |
| **B** | **FURNITURE FOR PA STAFF** | |  |  |  | - | - |
| 1 | **T-4** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 5'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 2 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 3 | **CH-8** | PROVIDING AND MAKING VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 8 |  |  |  |
| 4 | **FC-2** | PROVIDING AND MAKING FILLING CABINET OF SIZE 7'-0" X 3'-0" X 20" DEEP, HAVING TWO PORTION, BOTTOM PORTION HAVING 4 NOS PARTITIONS, BACK AND OPEN ABLE SHUTTERS MADE OF 3/4'' THICK AND 1'' THICK LAMINATION CHIP BOARD 700 DENSITY ON TOP WITH SHESHAM WOOD LIPPING ON ALL EDGES, UPPER PORTION, HAVING 4 NOS PARTITIONS AND 3 NOS SHELVES AND BACK ALSO MADE OF 3/4'' THICK CHIP BOARD AND LIPPING WITH SHESHAM WOOD, 3/4" THICK LAMINATION CHIPBOARD OF 700 DENSITY OPEN ABLE SHUTTERS, ALL SHESHAM WOOD POLISHED, ALL FITTING LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 3 |  |  |  |
| 5 | **FC-5** | PROVIDING AND MAKING FILLING CABINET OF REQUIRED SIZE AND 2' - 0'' DEEP HAVING 2 OR 3 PORTIONS WITH 4 NOS SHELVES WITH OPEN ABLE SHUTTERS MADE OF HIGH QUALITY LAMINATION BOARD 3/4'' AND THICK OF 750 DENSITY INCLUDING ALL EXPOSED SURFACES FINISHED WITH BEST QUALITY FORMICA OF APPROVED COLOR FIXED WITH GERMAN GLUE, ALL FITTINGS LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECTS AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SFT | 120 |  |  |  |
| 6 | **NB-1** | PROVIDING AND SUPPLYING SOFT BOARD NOTICE BOARD AS PER APPROVED DRAWING AND DESIGN. | NOS | 2 |  |  |  |
| **C** | **FURNITURE FOR THE OFFICES OF ASSOCIATES PROFESSOR / LECTURERS** | |  |  |  | - | - |
| 1 | **T-2** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 5'-0" X 3'-0" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 2 | **T-3** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 5'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 3 | **CH-2** | PROVIDING AND MAKING REVOLVING CHAIR HIGH BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 10 |  |  |  |
| 4 | **CH-8** | PROVIDING AND MAKING VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 30 |  |  |  |
| 5 | **S-1** | PROVIDING AND MAKING SOFA SINGLE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 20 |  |  |  |
| 6 | **ST-1** | PROVIDING AND MAKING SIDE TABLE OF SIZE 18" X 18" X 18" HIGH, MADE OF SHESHAM WOOD FRAME AND LEGS INCLUDING 8MM THICK TINTED GLASS FIXED IN 1 1/2'' X 3'' SHESHAM WOOD TOP FINISHED WITH SPRIT POLISH AND ALL SHESHAM COMPLETELY SEASONED AND TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 10 |  |  |  |
| 7 | **BS-3** | PROVIDING AND MAKING BOOK SHELF OF SIZE 6'-0" X 6'-6" HAVING TWO PORTION, BOTTOM PORTION HAVING 4 NOS PARTITIONS, BACK AND OPEN ABLE SHUTTERS MADE OF 3/4'' THICK AND 1'' THICK LAMINATION CHIP BOARD 700 DENSITY ON TOP WITH SHESHAM WOOD LIPPING ON ALL EDGES, UPPER PORTION 15'' DEEP, HAVING 4 NOS PARTITIONS AND 3 NOS SHELVES AND BACK ALSO MADE OF 3/4'' THICK CHIP BOARD AND LIPPING WITH SHESHAM WOOD, 1'' THICK GLAZED OPEN ABLE SHUTTERS MADE OF 5MM THICK GLASS PLAIN LOCALLY MADE FIXED IN SHESHAM WOOD FARMING ALL SHESHAM WOOD POLISHED, ALL FITTING LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 8 | **FC-2** | PROVIDING AND MAKING FILLING CABINET OF SIZE 7'-0" X 3'-0" X 20" DEEP, HAVING TWO PORTION, BOTTOM PORTION HAVING 4 NOS PARTITIONS, BACK AND OPEN ABLE SHUTTERS MADE OF 3/4'' THICK AND 1'' THICK LAMINATION CHIP BOARD 700 DENSITY ON TOP WITH SHESHAM WOOD LIPPING ON ALL EDGES, UPPER PORTION, HAVING 4 NOS PARTITIONS AND 3 NOS SHELVES AND BACK ALSO MADE OF 3/4'' THICK CHIP BOARD AND LIPPING WITH SHESHAM WOOD, 3/4" THICK LAMINATION CHIPBOARD OF 700 DENSITY OPEN ABLE SHUTTERS, ALL SHESHAM WOOD POLISHED, ALL FITTING LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 9 | **NB-1** | PROVIDING AND SUPPLYING SOFT BOARD NOTICE BOARD AS PER APPROVED DRAWING AND DESIGN. | NOS | 10 |  |  |  |
| **D** | **FURNITURE FOR TEACHERS COMMON ROOM** | |  |  |  | - | - |
| 1 | **RT-2** | PROVIDING AND MAKING MEETING / READING TABLE OF SIZE 8'-0" X 4'-0"AND 30" HIGH, MADE OF 3/4'' AND 1'' THICK CHIP BOARD OF 700 DENSITY WHEREVER REQUIRED WITH AND INCLUDING SHESHAM WOOD LIPPING AND FARMING OF REQUIRED SIZE, INCLUDING ALL EXPOSED SURFACES SPIRIT POLISH ETC; COMPLETE ALL FITTINGS (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 2 | **CH-8** | PROVIDING AND MAKING VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 22 |  |  |  |
| 3 | **S-3** | PROVIDING AND MAKING SOFA THREE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 3 |  |  |  |
| 4 | **S-1** | PROVIDING AND MAKING SOFA SINGLE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 5 | **CST-2** | PROVIDING AND MAKING CENTER AND SIDE TABLE SET OF SIZE 4'-0" X 2'-0" X 18" HIGH, AND 18" X 18" X 18" HIGH, MADE OF SHESHAM WOOD FRAME AND LEGS INCLUDING 8MM THICK TINTED GLASS FIXED IN 1 1/2'' X 3'' SHESHAM WOOD TOP FINISHED WITH SPRIT POLISH AND ALL SHESHAM COMPLETELY SEASONED AND TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SET | 3 |  |  |  |
| 3 | **NB-1** | PROVIDING AND SUPPLYING SOFT BOARD NOTICE BOARD AS PER APPROVED DRAWING AND DESIGN. | NOS | 2 |  |  |  |
| **E** | **FURNITURE FOR COMPUTER LAB** | |  |  |  | - | - |
| 1 | **T-5** | PROVIDING AND MAKING COMPUTER TABLE, SIZE 4-0" X 2'-6" X 30" H, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 36 |  |  |  |
| 2 | **CH-5** | PROVIDING AND MAKING COMPUTER REVOLVING CHAIR, WITHOUT ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 36 |  |  |  |
| 3 | **T-4** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 5'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 4 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 5 | **NB-1** | PROVIDING AND SUPPLYING SOFT BOARD NOTICE BOARD AS PER APPROVED DRAWING AND DESIGN. | NOS | 2 |  |  |  |
| **F** | **FURNITURE FOR LIBRARY** | |  |  |  | - | - |
| 1 | **BR-1** | PROVIDING AND MAKING BOOK RACKS (DOUBLE FACE), SIZE 3-0" X 2'-6" X 7'-0" H, SIDES AND SHELFES MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 18 |  |  |  |
| 2 | **T-4** | PROVIDING AND MAKING L SHAPE TABLE OF SIZE 5'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 3 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 4 | **RT-1** | PROVIDING AND MAKING MEETING / READING TABLE OF SIZE 16'-0" X 4'-0"AND 30" HIGH, MADE OF 3/4'' AND 1'' THICK CHIP BOARD OF 700 DENSITY WHEREVER REQUIRED WITH AND INCLUDING SHESHAM WOOD LIPPING AND FARMING OF REQUIRED SIZE, INCLUDING ALL EXPOSED SURFACES SPIRIT POLISH ETC; COMPLETE ALL FITTINGS (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 5 | **CH-8** | PROVIDING AND MAKING VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 18 |  |  |  |
| **G** | **FURNITURE FOR COMMITTIE / CONFERENCE ROOM** | |  |  |  | - | - |
| 1 | **CT-1** | PROVIDING AND MAKING CONFERENCE TABLE OF SIZE 18'-0" X 4'-0"AND 30" HIGH, MADE OF 3/4'' AND 1'' THICK CHIP BOARD OF 700 DENSITY WHEREVER REQUIRED WITH AND INCLUDING SHESHAM WOOD LIPPING AND FARMING OF REQUIRED SIZE, INCLUDING ALL EXPOSED SURFACES SPIRIT POLISH ETC; COMPLETE ALL FITTINGS (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 2 | **CH-8** | PROVIDING AND MAKING VISITOR CHAIR WITH ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 19 |  |  |  |
| **H** | **FURNITURE FOR CAFTERIA** | |  |  |  | - | - |
| 1 | **DT-3** | PROVIDING AND MAKING DINNING TABLE OF SIZE 3'-6" DIA AND SHAPE MADE OF 3/4'' AND 1'' THICK CHIP BOARD OF 700 DENSITY WHEREVER REQUIRED WITH AND INCLUDING SHESHAM WOOD LIPPING AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, ALL EXPOSED SURFACES POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 2 | **CH-11** | PROVIDING AND MAKING DINNING CHAIR WITH OUT ARMS AND 1' - 6'' HIGH BACK MADE OF SHESHAM WOOD COMPLETELY SEASONED WITH MASTER MOLTY FOAM SEAT & BACK COVERED WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR INCLUDING ALL WOOD WORK OF SHESHAM WOOD FINISHED WITH SPRIT POLISH AND TERMITE CONTROL TREATMENT ETC, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 12 |  |  |  |
| **I** | **FURNITURE FOR SEMINAR ROOM** | |  |  |  | - | - |
| 1 | **FD-2** | PROVIDING AND MAKING FRONT DESK, CURVED SHAPE TABLE OF SIZE 10'-0" X 16" X 30" HIGH, FRAME STRUCTURE MADE FROM MS PIPE 18 SWG OF APPROVED SIZE AND SHAPE, TOP AND FRONT PANNEL MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, FIXED ON GROUND ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 18 |  |  |  |
| 2 | **CH-14** | PROVIDING AND MAKING STUDENT REVOLVING CHAIR MEDIUM BACK, WITHOUT ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE FIXED ON GROUND, MADE OF CASTED ALUMINUM, COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 90 |  |  |  |
| 3 | **T-6** | PROVIDING AND MAKING TEACHER TABLE OF SIZE 4'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 4 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 5 | **R-3** | PROVIDING AND MAKING ROSTRUM OF SIZE 2'-0" X 1'-6" X 48" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 6 | **WB-2** | PROVIDING AND SUPPLYING WHITE BOARD OF SIZE 16'-0" X 4'-0", COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| **J** | **FURNITURE FOR CLASS ROOMS - 04 NOS** | |  |  |  | - | - |
| 1 | **FD-2** | PROVIDING AND MAKING 02 STUDENT DESK BENCH OF DESK SIZE 4'-0" X 16" X 30" HIGH, BENCH SIZE 4'-0" X 16" X 18" HIGH, FRAME STRUCTURE MADE FROM MS PIPE 18 SWG OF APPROVED SIZE AND SHAPE, TOP AND FRONT PANNEL MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , BENCH TOP COVERED WITH MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, FIXED ON GROUND ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 168 |  |  |  |
| 2 | **T-6** | PROVIDING AND MAKING TEACHER TABLE OF SIZE 4'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 3 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 4 | **R-3** | PROVIDING AND MAKING ROSTRUM OF SIZE 2'-0" X 1'-6" X 48" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 5 | **WB-2** | PROVIDING AND SUPPLYING WHITE BOARD OF SIZE 16'-0" X 4'-0", COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| **K** | **FURNITURE FOR LABS 03 NOS** | |  |  |  | - | - |
| 1 |  | PROVIDING AND FIXING IRON STEEL FRAME MADE OF 1 1/4" X 1 1/4" SQUARE PIPE OF 16 SWG, FRAME COMPLETELY WALDED 3 COAT OF ENAMEL PAINT OVER A COAT OFANTI CROSSIVE (RED OXIDE) ETC. HEIGHT OF FRAME TO BE 2'-9" AND 2'-0" DEEP, SUPPORTING WITH LEGS IN MIDDLE AND IN THE DEPTH 1" EACH, WHICH DIVIDES THE LENGTHS EQUALLY ON THE BACK SIDE. LEGS ARE INTER JOINTED BUT FRONT VIEW OPEN TO FIX THE WOODEN CABINET, ALL WORK COMPLETE AS PER DRAWING DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGEETC. COMPLETE IN ALL RESPECT. | RFT | 210 |  |  |  |
| 2 |  | PROVIDING AND MAKING LABORATORY TOP COUNTER 2'-6" WIDE MADE OF HIGH QUALITY LAMINATION BOARD 3/4" THICK OF 750 DENSITY OF APPROVED COLOR AND USING GERMAN GLUE , WITH AND INCULDING THE COST OF 8MM THICK IMPORTED GLASS PLAIN ON THE TOP INNCLUDING TERMITE CONTROL TREATEMENT TO ALL WOOD WORKETC COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | RFT | 210 |  |  |  |
| 3 |  | PROVIDING AND MAKING LABORATORY MOVEABLE CABINETS WITH DOORS, SHELVESMADE OF HIGH QUALITY LAMINATION BOARD 3/4" THICK OF 750 DENSITY, AND DRAWERS MADE OF PARTAL WOOD 1/2" THICK SIDES, 3/4" THICK SIDES, 3/4" THICK FRONT AND 5MM THICK COMMERICAL PLY AT BOTTOM DRAWERS. 1/2" THICK LASSANI WOOD BACK AND TOP OF CABINET INCLUDING BEST QUALITY OF FORMICA FIXED WITH GERMAN GLUE AND INNER SURFACE OF DRAWERS PAINTED WITH ENAMEL PAINT OF REQUIRED SHADE AND QUALITY, ALL FITTINGS LIKE HANDELS, LOCKS, HINGES AND WHEEL ( ALL IMPORTED ) OF BEST QUALITY OF APPROVED MAKE INCLUDING TERMITE CONTROL TREATEMENT TO ALL WOOD WORKETC COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. |  |  |  | - | - |
| A |  | CABINET SIZE 3'- 0" X 1'-10" DEEP 2'-10" HIGH IN TWO PORTIONS, 1ST PORTION HAVING 4 DRAWERS 3 NOS OF 6" HIGH & ONE OF 10 1/2" HIGH, OTHER PORTION HAVING TWO DOORS AND AND ONE REMOVABLE. | NOS | 15 |  |  |  |
| B |  | CABINET SIZE 3'-6" X 1'-10" DEEP 2'-10" HIGH, UPPER PORTION HAVING TWO DRAWERS, 6" HIGH AND BOTTOM PORTION HAVING 4 DOORS AND ONE REMOVABLE SHELF. | NOS | 15 |  |  |  |
| 4 |  | PROVIDING AND MAKING CHEMICAL RACK 2'-6" HIGH, 6" DEEP, HAVING TWO SHELVES AND PARTITIONS AT 101/2" C/C, MADE OF HIGH QUALITY LAMINATION BOARD 3/4" THICK OF 750 DENSITY FINISHED WITH BEST QUALITY FORMICA FIXED WITH GERMAN GLUE TO ALL EXPOSED SURFACES AND INNER SURFACE PAINTED WITH ENAMEL PAINT OF REQUIRED SHADE AND QUALITY, INCLUDING ALL REQUIRED FITTINGS AND TREATEMENT TO ALL WOOD WORK ETC COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | RFT | 210 |  |  |  |
| 5 |  | PROVIDING AND MAKING SINK CABINET SIZE 3'-0" X 2'-6"" X 2'-10" WITH DOOR AND MOUNTED PARTITION, TOP MADE OF 1" THICK MARBLE AND 1" THICK MARBLE OF 6" HIGHT ON BOTH AND BACK SIDE OVER THE TOP AND FRONT PORTION OF SINK UNIT LABORATORY MOVEABLE CABINETS WITH DOORS, AND INCLUDING COST OF 24" X 18" SIZE GLAZED EARTH WARE CHINA CHEMICAL PROOF SINK OF APPROVED MAKE AND FIXED IN MS PIPE 3/4" X 3/4" 16 SWG, FRAME, WITH SWAN NECK TAP STANDARD SIZE, ALL FITTINGS LIKE HANDELS, LOCKS, HINGES AND WHEEL ( ALL IMPORTED ) OF BEST QUALITY OF APPROVED MAKE INCLUDING TERMITE CONTROL TREATEMENT TO ALL WOOD WORKETC COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 6 |  | PROVIDING AND MAKING HANGING CABINET SIZE 6'-0" X 2' - 6'' HIGH AND 15'' DEEP WITH GLAZED SHUTTER SLIDING OR OPEN ABLE MADE OF 5MM THICK GLASS FIXED IN SHESHAM WOOD FRAMING AND 3/4'' CHIP BOARD 700 DENSITY FOR PARTITION, SHELVES AND BACK AND TOP OF 1'' THICK CHIP BOARD LIPPING WITH SHESHAM WOOD AND FINISHED WITH BEST QUALITY FORMICA OF APPROVED COLOR FIXED WITH GERMAN GLUE AND ALL SHESHAM WOOD POLISHED AND INNER SURFACES PAINTED WITH ENAMEL PAINT OF REQUIRED SHADE AND QUALITY, ALL FITTING LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE | NOS | 9 |  |  |  |
| 7 |  | PROVIDING AND MAKING CUPBOARD SIZE 6'-0" X 3'-O" X 2' - 0'' DEEP HAVING 2 OR 3 PORTIONS WITH 4 NOS SHELVES WITH OPEN ABLE SHUTTERS MADE OF HIGH QUALITY LAMINATION BOARD 3/4'' AND THICK OF 750 DENSITY INCLUDING ALL EXPOSED SURFACES FINISHED WITH BEST QUALITY FORMICA OF APPROVED COLOR FIXED WITH GERMAN GLUE AND INNER SURFACES PAINTED WITH ENAMEL PAINT OF REQUIRED SHADE AND QUALITY ALL FITTINGS LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECTS AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 8 |  | PROVIDING PATIENT BED 6'-6" X 3'-0" SIZE AND 3'-0"BACK AND 2'-6" HIGH FRONT MADE OF MS PIPE FRAME WITH 1" SQUARE MS PIPE FRAME FOR HOLDING BED WITH 4MM THICK MDF SHEET AND 4" THICK MASTER MOLTY FOAM INCLUDING ALL WELDING POWDER COATED ETC; COMPLETE IN ALL RESPECT AS PER DRAWING AND AS DIRECTED BY THE ENGINEER INCHARGE. (AS PER SAMPLE) | NOS | 9 |  |  |  |
| 9 |  | PROVIDING 6' - 6'' X 4' - 0'' WITH ADJUSTABLE HEIGHT (STANDARD) PATIENT BED (COUTCH) MADE OF M.S SECTIONS DOWEL ADJUSTABLE FROM HEAD AND FOOTING WITH METROS OF REQUIRED THICKNESS AND MOVEABLE ACCESSORIES LIKE FRAME WHEELS AND LOCKING SYSTEM INCLUDING FRONT BACK AND FRONT AND REST AS PER STANDARD DESIGN COMPLETE IN ALL RESPECTS AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 10 |  | PROVIDING 1' - 6'' X 1' - 6'' X 2' - 8'' HIGH PATIENT CABINET MADE OF STAINLESS STEEL (18 GAUGE) GRADE 304 TOP, HAVING 1' - 9'' HIGH BOX WITH SHUTTER (OPEN ABLE) OF MS SHEET, WITH LOCK, POWDER COATED, AS SHOWN ON DRAWING ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 15 |  |  |  |
| 11 | **T-6** | PROVIDING AND MAKING TEACHER TABLE OF SIZE 4'-0" X 2'-6" X 30" HIGH, MADE OF 3/4'' AND 1'' THICK LAMINATION BOARD 700 DENSITYOF APPROVED COLOR AND SHADE WHEREVER REQUIRED WITH AND INCLUDING OAK WOOD LIPPING , AND FARMING OF REQUIRED SIZE, FIXED WITH GERMAN GLUE, POLISHED WITH NC LACQUER, ETC; COMPLETE ALL FITTINGS LOCKS, HANDLES (APPROVED) AND TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 12 | **CH-3** | PROVIDING AND MAKING REVOLVING CHAIR MEDIUM BACK, WITH ARMS, CUSHIONED SEAT & BACK MADE OF MASTER MOLTY FOAM WITH GOOD QUALITY CLOTH OF APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME FIVE WHEELS (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| 13 | **FC-5** | PROVIDING AND MAKING FILLING CABINET OF REQUIRED SIZE AND 2' - 0'' DEEP HAVING 2 OR 3 PORTIONS WITH 4 NOS SHELVES WITH OPEN ABLE SHUTTERS MADE OF HIGH QUALITY LAMINATION BOARD 3/4'' AND THICK OF 750 DENSITY INCLUDING ALL EXPOSED SURFACES FINISHED WITH BEST QUALITY FORMICA OF APPROVED COLOR FIXED WITH GERMAN GLUE, ALL FITTINGS LIKE HANDLES, LOCKS AND HINGES OF BEST QUALITY (APPROVED) INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORK ETC. COMPLETE IN ALL RESPECTS AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SFT | 200 |  |  |  |
| 14 | **WB-2** | PROVIDING AND SUPPLYING WHITE BOARD OF SIZE 16'-0" X 4'-0", COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 3 |  |  |  |
| 15 | **ALUM** | PROVIDING AND FIXING GOOD QUALITY ALUMINIUM CHANNEL FRAMING SOLID STRI PARTITION WALL CUM GLASS PARTITON IN ALUMINIUM FRAME WITH HINGES/SLIDING TYPE ALUMINIUM DOOR AND WINDOWS REQUIRED IN 1.6 MM THICK SECTION OF BROWN / SILVER / CHAMPION COLOR AS PER APPROVED DRAWINGS AND DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SFT | 1355 |  |  |  |
| **L** | **FURNITURE FOR RECEPTION AREA** | |  |  |  | - | - |
| 1 |  | PROVIDING AND MAKING RECEPTION COUNTER 16' - 0'' X 3' - 0'' HIGH COVERED AT BOTH END AS SHOWN ON DRAWINGS, MADE OF CHIPBOARD HIGH QUALITY 3/4'' THICK FINISHED WITH BEST QUALITY FORMICA FIXED WITH GERMAN GLUE AND CHIPBOARD LIPPING WITH BEST QUALITY SEASONED SHESHAM WOOD FINISHED WITH SPRIT POLISH, ALL EXPOSED SURFACES AND INNER SURFACE PAINTED WITH ENAMEL PAINT OF REQUIRED SHADE AND QUALITY, INCLUDING TERMITE CONTROL TREATMENT TO ALL WOOD WORKS ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 1 |  |  |  |
| 2 | **S-3** | PROVIDING AND MAKING SOFA THREE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 2 |  |  |  |
| 3 | **S-1** | PROVIDING AND MAKING SOFA SINGLE SEATER MADE OF SEASONED SHESHAM WOOD WITH ARMS, LEGS, BACK SEAT AND FRAME WITH MASTER MOLTY FOAM IN REQUIRED THICKNESS COVERED WITH GOOD QUALITY CLOTH OF APPROVED COLOR AND WOOD WORK FINISHED WITH SPRIT POLISH INCLUDING TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 4 |  |  |  |
| 4 | **CST-2** | PROVIDING AND MAKING CENTER AND SIDE TABLE SET OF SIZE 4'-0" X 2'-0" X 18" HIGH, AND 18" X 18" X 18" HIGH, MADE OF SHESHAM WOOD FRAME AND LEGS INCLUDING 8MM THICK TINTED GLASS FIXED IN 1 1/2'' X 3'' SHESHAM WOOD TOP FINISHED WITH SPRIT POLISH AND ALL SHESHAM COMPLETELY SEASONED AND TERMITE CONTROL TREATMENT ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SET | 2 |  |  |  |
| 5 | **VB-1** | PROVIDING AND MAKING IMPORTED METAL THREE SEATER VISITER BENCH, WITH ARMS, APPROVED SHADE AND COLOR, BASE MADE OF CASTED ALUMINUM FRAME (IMPORTED) COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | NOS | 6 |  |  |  |
| **L** | **GENERAL ITEM** | |  |  |  |  |  |
| 5 |  | PROVIDING AND FIXING ROLLER BLIND IMPORTED OF APPROVED COLOR AND SHADE WITH INCLUDING ALL FITTINGS AND FIXTURES ETC; COMPLETE IN ALL RESPECT AS PER DRAWING, DESIGN AND AS DIRECTED BY THE ENGINEER INCHARGE. | SFT | 2900 |  |  |  |
|  |  |  | **TOTAL AMOUNT** | | | |  |

**BID DECLARATION FORM**

1. Name of Interested Firm:

2. CNIC#: (Please attach Copy of CNIC)

3. NTN #: (Please attach Copy of NTN Certificate)

4. GST#: (Please attach Copy of GST Certificate)

5. Value of Earnest Money Rs: DD/PO#:

(In words):

Bank Name:

6. Contact Person:

7. Postal Address:

8. Email Address:

9. Telephone: PTCL: Cell Phone:

(Compulsory)

**Declaration:** I certify that, to the best of my knowledge and belief, all of the information on and attached is true, correct, complete and made in good faith. I understand that false or fraudulent information on or attached to this form may be grounds for not entertaining my bid, or for cancellation after bid acceptance, and may be punishable by fine or imprisonment according to law of Pakistan. I understand that any information I voluntarily provide on or attached to this bid may be investigated. Moreover, I hereby declare the all the terms and conditions of the biding document are accepted.

**Contractor**

Sign with stamp