Name of work: M/R TO SECRETARY BUNGALOW 1-8 TOWN HOUSES GOR III KARACHI DAY TO DAY COMPLAINTS HARD WARE & SANITARY ITEMS)

Schedule B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S. No. | Description | Qty | Rate | Unit | Amount |
| 1 | P/F approved quality mortice door lock (s.i.21/60). | 16-Nos | 1786/13 | Each | 28578 |
| 2 | P/F Slidding Bolt to doors (ii)Iron slidding bolt to 12’long | 12-Nos | 222/23 | ‘ | 2667 |
| 3 | Nyloon Wire Guaze 144 mesh per square inch fixed to chowkats with ¾”deodar strips and sc | 298.00 | 193/53 | SFT | 57672 |
| 4 | P/F GI expended metal 1/2”to ¾” mesh 16 guage fixed to chowkats without deodar patti (S.I.65B/66) | 298.00  Sft | 60/43 | Sft | 18008 |
| 5 | P/F with sunk iron screwes wooden archtrative approved design shape having with not less then 3.7lbs 2-1/2 inches as directed by Engineer Incharge (S.I.6 | 200.00 | 49/97 | Sft | 9994 |
|  | Total |  |  |  | 116919 |
|  | Total A |  |  |  |  |
|  | Part B W/S & S/F |  |  |  |  |
| 1 | S/F in position CPlong bib cock ¾”thick CP bib cock light pattern(S.I 16 | 24-Nos | 1109/46 | Each | 26627 |
| 2 | S/F Sink Mixture cock superior quality with CP head etc complete. | 6-Nos | 2745/60 |  | 16474 |
| 3 | S/F Swan type Piller cock of superior quality single cp head ½”dia (S.I.16-a/1 | 12-Nos | 795/30 | EACH | 9544 |
| 4 | S/F Jet Shower with rod of superior quality single cp head ½”dia (S.I.15/19) | 4-Nos | 1142/24 | Each | 4569 |
| 5 | S/F CP Muslim shower with crystal head etc complete. | 16-Nos | 3432/- | Each | 54912 |
| 6 | P/F 22x16 lavatory basin in white glazed earthen ware complete with and i/c the cost of WI or CI ventilator brackets 6built into walls pointed white in two coats after a primary coat of red head of paint a pair of 1-1/2 dia rubber plug and chrome plated brass chain 1-1/4 dia maloable iron or brass unions and making requisite number of holes in walls plinth and floor for pipe connection and making good in cement mortor 1.2.4 Foreig or equilent)(S.I.13/4) | 8-Nos | 6237/- | Each | 49896 |
| 7 | P/F squatting type white glazed earthen ware wc pan with front flush into & complete with including the cost of cistern with internal fitting and flush type bends and making requisite number of holes in walls plinth & floor for pipe connection & making good in cement concrete 1.2.4 (foreign equilent)(b) WC 19”clear earthen ware low level flush tank 3-gallons (ii) with 4”dia earthen ware & plastic themble | 6-Nos | 5486/80 | Each | 32921 |
| 8 | Add extra for labour for providing and laying of earthen ware pedestal white or coloured glazed foreign or equilent.(S.I 11/ | 8-Nos | 2533/47 | Each | 20268 |
| 9 | P/F 15x12 bevelled edge mirror of Belgium glass complete with 1/8 thick hard board & screwes fixed to wooden cleats.( | 8-Nos | 2047/76 | Each | 16382 |
| 10 | P/F Steel sinks stainless local make complete with cost of wrought iron brackets & 6inches built into wall 1-1/2’ GP rubber brass vaste with 1-1/2 PVC waste pipe & making requisite number of hole in walls and plinth & floor for pipe connection & making good in CC 1.2.4 steel sink stainless sized 33x18 local make standard pattern. | 4-Nos | 5712/30 |  | 22849 |
| 11 | S/F Bath Room Accessories set (7-Pieces ) i/c towel rod brush holder soap tray shelf of approved design i/c cost of screwes nuts etc complete (Master Brand). | **6-Nos** | **10322/40** | **“** | **61934** |
| 12 | S/F of Fiber Glass Tank of approved quality & design and wall thickness as per specified i/c cost of nuts bolts & fixing in plate form cement concrete 1.3.6 & making connection inlet & outlet for pipe etc complete.(500 gallons) | **2-Nos** | **37505/42** | **Each** | **75011** |
|  | Total |  |  |  | 391388 |
|  | Add % above |  |  |  |  |
|  | B |  |  |  |  |
|  | Part C N.S.Items |  |  |  |  |
| 1 | P/F Draws Locxk ¾ best quality etc complete. | 24-Nos |  |  |  |
| 2 | P/F Draws Locks KGI (Imported make)as per approved make etc complete. | 24-Nos |  | “ |  |
| 3 | P/F Almirah lock upto 2-1/2”long best quality etc complete. | 12-Nos |  | “ |  |
| 4 | S/F double bib cock heavy pattern as per approved quality as directed by the Engineer Incharge etc complete. | 24-Nos |  | ` |  |
| 5 | P/F Tee Stop Cock master make in CP coated as directed by Engineer Incharge etc complete. | 16-Nos |  | “ |  |
| 6 | S/F Basin Mixture (Master make) or equelent quality etc complete. | 8-Nos |  | “ |  |
| 7 | S/F Thermostate imported make as per approved quality etc complete. | 6-Nos |  | “ |  |
| 8 | S/F UPVC Pipe ½”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 200-Rft |  | Rft |  |
| 9 | S/F UPVC Pipe 1”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 100-Rft |  | Rft |  |
| 10 | S/F UPVC Elbow ½ dia heavy pattern as per directed by Engineer Incharge | 18-No |  | Each |  |
| 11 | S/F UPVC Elbow 1”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 12-Nos |  | Each |  |
| 12 | S/F Gate Valve 1-1/2 ”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 12-Nos |  | Each |  |
| 13 | S/F Handle Valve ¾ ”dia heavy pattern as per directed by the Engineer Incharge etc complete. | 12-Nos |  | “ |  |
| 14 | P/F Hydrollic door closer as per approved quality by the Engineer Incharge etc | 16-Nos |  | “ |  |
| 15 | P/F Alpha door Golden door lock as per approved quality etc complete. | 16-Nos |  | “ |  |
| 16 | S/F Cement Bag as per approved quality etc com | 6-Nos |  | “ |  |
| 17 | S/F Waist Pipe 1-1/4”dia brass type as per approved quality by the Engineer Incharge etc co | 12-Nos |  | “ |  |
| 18 | P/F Lassani sheet ¼” (4’x8”) as per approved quality by the Engineer Incharge etc complete. | 4-Sheet |  | “ |  |
| 19 | S/O Nails mixed approved quality | 8-Pkt |  | “ |  |
| 20 | S/O Steel Nails 2”long as per approved quality etc complete. | 8-Pkt |  | Each |  |
| 21 | S/F CI man hole cover size 24”x24” as approved quality by the Engineer Incharge etc complete. | 4-Nos |  | Each |  |
| 22 | P/F double burner stainless steel i/c necessary fittings etc complete as directed by the Engineer Incharge. | 4-Nos |  | Each |  |
| 23 | P/F Water Heater Geyser 30 Gallons Deco make or equelent quality i/c necessary fitting the cost of i/c carriage from Show Room to Site of work as directed by the consultant. | **3-Nos** |  | **Each** |  |
|  | Total C |  |  |  |  |
|  | G Total |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Buildings sub Division-IX,

Karachi