NAME OF WORK**:- : CONST: Of RETAINING WALL ALONG ROAD FORM GHOGI MANGNEJA JEHA ROAD.**

**( SAHEDULE B)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Quantity | Item of work | Rate | Unit | Amount |

1/- Excavation in foundation of building Brigde nd other structure i/e degbeling

dressing refilling around structure with excavated earth watering & remaining

lead upto 100% & left upto 5” (in ordinary soil)

1300 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 1300 Cft | @ Rs.3176/25 | P%0 Cft | Rs.3970/-130Rs. 4129/- |

2/- Cement Brick or stone ballast 11/2” -2” gauge. Ratio 1:4:8 (Hill sand to be used)

325 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 325 Cft | @ Rs.9416/28 | P% Cft | Rs.30602/- |

3/- Pacca Brick work in other than i/c stricking of joints upto 20” height in Cement Sand morta

Ratio 1:4.

1123 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 1123 Cft: | @ Rs.12501/41 | P% Cft | Rs.140390/- |
|  |  |  |  |

4/- Cement Concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of stone aggregate without shuttering, Ratio 1:2:

56 Sft

|  |  |  |  |
| --- | --- | --- | --- |
| 56 Cft | @ Rs.14429/25 | P% Sft | Rs.8080/- |

5/- Cement Plaster (1:3) upto 20 Height ½ thick

500 Sft

|  |  |  |  |
| --- | --- | --- | --- |
| 500 sft | @ Rs.2344/59 | P.Cft | Rs.11722/- |

**Total Rs.194925/-**