**NAME OF WORK:-CONSTRUCTION OF 03’ SPAN CULVERT ROAD FROM KHUHRA ROAD TO RIR MUHAMMAD NAREJO TO BY PASS ROAD**

**( SCHEDULE B )**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Quantity | Item of work | Rate | Unit | Amount |

1/- Excavation in foundation of building Brigde nd other structure i/e degbeling

dressing refilling around structure with excavated earth watering & remaining

lead upto 100% & left upto 0. 5” (in ordinary soil)

= 1217 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 1250 Cft | @ Rs.3176/25 | P%0 Rs.3970/- | Rs.3970/- |

2/- Cement Brick or stone ballast 11/2” -2” gauge. Ratio 1:4:8 (Hill sand to be used)

= 245 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 245 Cft | @ Rs.9416/28 | P% Cft | Rs.23070/- |

3/- Pacca Brick work in other than i/c stricking of joints upto 20” height in Cement Sand morta

Ratio 1:4.

= 357 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 357 Cft | @ Rs.12501/41 | P% Cft | Rs.44630/- |

4/- Cement Concrete plain i/c placing compacting finishing & curing complete i/c screening & washing of stone aggregate without shuttering, Ratio 1:2:

= 21 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 21 Cft | @ Rs.14429/25 | P% Cft | Rs.3030/- |

5/- Fabrication of mild steel reinforcement for cement i/c cutting bending layinging position making joints & fastening i/c cost of mild steel & binding wire (also removal of rust from bars).

|  |  |  |  |
| --- | --- | --- | --- |
| 6.83 Cwt | @ Rs.4820/20 | P.Cwt | Rs.32922/- |

6/- Reinforced Cement Concrete work i/c all labor and materials except the cost

of steel reinforcement and its labor for bending and binding which will be paid

separately. This rate also i/c all kinds of forms moulds lifting shuttering curing

rending and finishing surface (i/c screening & washing of shingle) R.C.C. work in

roof slabs beams columns rafts lintels & other structural members laid in situ of

pre-cuts in position complete in all respect. Ratio (1:2:4) 90 lbs Cement 2 Cft:

Sand 4 Cft: single 4/8”- ¼” gauge.

= 157 Cft

|  |  |  |  |
| --- | --- | --- | --- |
| 157 Cft | @ Rs.337/- | P.Cft | Rs.52909/- |

7/- Cement Plaster (1:3) upto 20” height ½” thick

198 Sft Rs.4642/-

|  |  |  |  |
| --- | --- | --- | --- |
| 198 Sft | @ Rs.2344/59 | P%Sft | Rs.4642 |

Total **Rs.165173/-**