|  |  |
| --- | --- |
| NAME OF SCHEME*:* | **REHABILITION OF ROAD FROM AHMEDPUR ROAD TO GHOGI MANGNEJA TALUKA KINGRMILE0/0- 0/5 (1.0 KM)** |

**(SCHEDULE B)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Qty* | ITEM OF WORK | QTY: | | RATE | UNIT | AMOUNT |
|  |  | | | | |  |
|  | 1/-Earth work for road embankment from bulldozers i/cs: plugging mixing clod breaking dressing & compacting with optimum moisture content lead upto 100’ & lift upto 5.0’in ordinary soil except in rock.  (EARTH WORK ON BERM) | | | | |  |
|  |  | | | | |  |
| 205100 | Cft @ Rs.6278/37 P%0 Cft | | | | | Rs.1287679 |
|  | 1/-Laying Brick on end edging i/cs: supply of 9”x4 ½”2”x3”Ist: Class Burnt bricks excavation for having edging with small size parallel to the road (Rate i/cs: lead upto side of work) | | | | |  |
|  | = 6798 | | | | Rft |  |
| 6800 | Rft |  | | @Rs.2771/63 | P.%Rft | Rs.188470/- |
|  | 2/-Preparing Base course by supplying & spreading stone metal of approved quality properly graded to maximum size of 1 ½”gauge in required thickness to proper camber & grade i/cs: supplying & spreading l5 cft: screening & Non plastic quarry fines filling depression with stone metal after initial rolling i/cs: watering & compacting the same so as to achieve 100% density as per modified AASHO Specification. | | | | |  |
|  | = 1020Cft:  = 20394  21414 | | | | Cft  Cft:: |  |
| 21400 | Cft: |  | | @Rs.7605/65 | P.% Cft: | Rs:1627609//- |
|  | 1/-Providing Surface Dressing Ist: Coat on new or existing surface with 30lbs: bitumen of 80/100 Penetration & 4.0 Cft: Crush bajri with i/cs: cleaning the road surface rolling etc: complete. (Rate i/cs: all costs of materials T&P & carriage upto site of work) | | | | |  |
|  | =40788 Sft | | | |  |  |
| 40800 | Sft: |  | | @Rs.1609/77 | P.%Sft | Rs.656786/- |
|  | 2/-Providing 1”thick (consolidate) Premixed Carpet in proper camber & grade i/cs: supplying of 10 cft: Crush bajri with 67lbs: bitumen of 80/100 Penetration & 4.00 Cft: Hill sand rolling etc: complete. | | | | |  |
|  | =40788 Sft | | | |  |  |
| 40800 Sft: | @Rs.4503/07 | | | | P.% Sft: | Rs.1837252/- |
|  | 7- decreased Cost of Bitumen. | |  |  |  | |
| 17.66 | P.Tons | | | Rs:17595 | P.Ton(-) | Rs: 310727 |

**Total Rs:5287069/-**

|  |  |
| --- | --- |
|  |  |