**NAME OF WORK:- REHABLITATION/ CONSTRUCTION OF (REVENUE) COMPLEX AT TALUKA NARA DISTRICT KHAIRPUR.**

(**SCHEDULE -B)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

1/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 4680 Cft @RS:3176.25 % Cft RS:14865/-

Thirty one hundred seventy six rups:twenty five ps:

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 1377 Cft @RS: 8694.95 % Cft RS: 119729/-

(Eight six hundreds ninty four rupees,ninty five ps:)

03/- Pacca Brick work in foundation / Plint in cement

cement & sand mortar ratio (1:6)(S.I No:05 (c)P.No:20)

Qty: 2458 Cft @RS: 11948.36 % Cft RS:293691/-

(Eleven thousands nine hundered fourty eight rs: thirty six ps.)

04/- Coursed Rubble Masnory 1:6 including hammer dressing (S.I No: 2 d P.26).

Qty: 2915 Cft @RS: 25321/- % Cft RS: 738107/-

(twenty five thousands three hundreds te=wenty one rups:)

05/- Filling watering & ramming earth from foundation lead up to one chain lift up to 5 feet (S.I NO: P.NO: ).

Qty: 4680 cft @RS: 1512.60 %0cft RS: 4719/-

(Fifteen hundred tweleve rupess, sixty ps:)

06/- Supplying Sand under floor plugging into wall (S.I NO: 29 P.NO: 26)

Qty: 25290 cft @RS: 1141.25 % Cft RS: 288622/-

(Eleven hundred fourty one rupees, twenty five ps.)

07/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:6:12). (S.I.No.4 (b) P.No.14)

Qty: 2782 cft @RS: 8122.95 % Cft RS: 225980/-

( eight thousands one hundreds twenty two rupees ninty five ps:)

08/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 3470cft @RS: 337/- P.Cft RS: 1169390/-

(Three hudred thirt seven ps.)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

09/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 30.80cwt @RS:5001.70 P.cwt RS:770262/-

(Five thousands & one ripes, seventy ps:)

10/- Pacca Brick work in Ground Floor in cement sand mortarRatio (1:6) (S.I No:5 P-25).

Qty: 3989 Cft @RS: 12674.65 % Cft RS: 505580/-

(Tweleve thousands six hundred seventy four rupees, sixty five ps.)

11/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for door using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 225 Rft @RS: 228/90 P.Rft RS: 51503/-

(Two hundred twenty eight rupees, ninty ps.)

12/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for window using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 337 Rft @RS: 240.50 P.Rft RS: 81049/-

(Two hundred fourty rupees, fifty ps.)

13/- First class deodar wood wrought joinery in doors & windows etc fixed in position including hold fasts hinges iron tower bolts chock, cleats handles and cords with hooks etc complete.

(S.I No: 54 P.NO: 65).

Qty: 436 Sft @RS:902.92 P.Sft RS: 393677/-

(Nine hundred two rupees, ninty two ps.)

14/- S/F impostion aluminum channel framing for hinging doors or alcop made with 5 mm thick tinted (Belgium) and alpha (Japan) etc complete (S.I NO: 83 P-114).

Qty: 49 @RS: 1507.66 P.Sft RS: 73875/-

(fifteen hundreds seven rupees sixty six ps:)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

15/- S/F impostion aluminum channel framing fo sliding windows and ventilators etcr alcop made with 5 mm thick tinted (Belgium) and alpha (Japan) etc complete (S.I NO: 83 P-114).

Qty: 32 @RS: 1647.69 P.Sft RS: 52726/-

(sixteen hundreds fourty seven rupees sixty nine ps:)

16/- Providing & Fixing Wire gauze fixed to chowakats etc complete.

Qty: 49 Sft @RS: 454.19 P.Sft RS: 22255/-

(four hundred fifty fourrupees ninteen ps:)

17/- Cement Plaster 1:6 up to 20’-0 height ½” thick. (S.I NO: 13(b) P: NO:52 )

Qty: 11282 Sft @RS: 2206.60 % Sft RS: 248949/-

(Twenty two hundreds six rupees, sixty ps.)

18/- Cement Plaster 1:4 up to 20”-0 heights 3/8” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 11282 Sft @RS: 2197.52 % Sft RS: 247929/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

19/- Cement Concrete plain including placing Compacting

Finishing & curing, complete i/c screening & washing

Of stone aggregate Ratio (1:2:4) (S.I No:5 P-18).

[

Qty: 1391 cft @RS: 14429.25 % Cft RS:200711/-

( fourteen thousands four hundreds twenty nine rupes twenty five ps:)

20/- Providing & Laying tiles 6”x6”x1/4” on floor on wall facing in required color and pattern of side specification jointed in white cement and pigment over a base 1:2 grey cement mortar ¾” i/c washing and filling of joints slurry of white cement and pigment in desired shape with finishing cleaning and coats polishing etc complete (S.I No: P.NO: )

Qty: 3865 sft @RS: 27678.86 % Sft RS: 1069788/-

( twenty seven thousands six hundred seventy eight rups: eighty six ps.)

21/- Laying white marble fine dressed in the surface without winding set in lime mortar 1:2 i/c rubbing and polishing pf the joints (a) ¾” thick flooring. (S.I.NO.28 (a) Page No. 43)

Qty: 240 Sft @RS: 567.48 P.Sft RS: 136195/-

(five hundreds sixty seven rupees fourty eight ps:)

22/- Providing & Fixing Wire gauze fixed to chowakats etc complete.

Qty: 176 Sft @RS: 345.53 P.Sft RS: 60813/-

(three hundred fourty five rups: fifty threeps:)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

23/- Supplying and fixing in position iron/steel grill of ¾” x ¼” size flat iron of approved design including painting 3 coats etc complete (Weight or not less than 3.7 Lbs/sq feet of finished grill

(S.I No: P.NO: ).

Qty: 176 Sft @RS: 180.50 P.Sft RS: 31768/-

(One hundred eighty rupees, fifty ps.)

24/- Plain wood work swan wrought aand fixed in position including cost of nails and screws etc complete (S.I NO: 1 P-64).

Qty: 6.21 cft @RS: 3742.42 P.Cft RS: 23240/-

(thirty seven hundreds fourty two rupees fourty two ps:)

25/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 11282 Sft @RS: 442.75 P.Sft RS: 49951/-

(Four hundred fourty two rupees, seventy five ps.)

26/- Matt Polishing finishing etc complete

Qty: 11282 sft @RS: 1989.62 % Sft RS: 224469/-

(ninteen eighty nine rupees sixty ttwo ps:)

27/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 3122 Sft @RS: 1043.90 % Sft RS; 32591/-

(ten hundreds fourty three rupees , Ninty ps.)

28/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty:976 Sft @RS: 2116.41 % Sft RS: 20656/-

(twenty one hundred sixteen rupees, fourty one ps.)

29/- Painting guard bars gets iron bars grating , railing including standard braces (etc) and similar open work. (S.I NO:4(d)P.NO:69).

Qty: 176 Sft @RS: 977.40 % Sft RS: 1720/-

(Nine hundreds seventy seven rupees fourty ps:)

30/- Providing and lying 1” thick C/C topping cement concrete (1:2:4) i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.42).(2” thick).

Qty: 3578 sft @RS: 3275.50 % Sft RS: 117197/-

(fourty four hundreds eleven rupees eighty two ps:)

31/- Two coats of Bitumen hot using 34 Lbs (S.I NO: P.NO: ).

Qty: 3578 Sft @RS: 1887.04 % Sft RS: 67531/-

(eighteen hundreds eighty seven rupees four ps:)

32/- Providing & Fixing Plaster of Pairis ceiling Border of 8”x10” with of specified design etc complete(S.I NO: P.NO ).

Qty: 68 rft @RS: 104.22 P.Rft RS: 7087/-

(One hundred four rupees twenty two ps:)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

33/- Providing & Laying HALA or pattern tiles glazed 6”x6”x1/4” on floor or wall facing in required color & pattern od STILE specification jointed in white cement & pigment over a base of 1:2 grey cement mortar ¾” thick including washing & filling or joints with slurry of white cement and pigment in desired shape with finishing cleaning and cost of wax polish etc. complete including cutting tiles to proper profile (S.I No:61 P.NO:480)

(A) Qty: 912 Sft @RS: 47651.56 % Sft RS: 434577/-

(fourty seven thousands six hundreds fifty one rupes fifty six ps:)

=========================================

Total RS: 7346625/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

**PART- W/S & S/F Mukhtiar kar office wash room**

01/- P/F squatting type white glazed of flushing cistern with internal fitting and flush pipe with band and making requisite Nos. of holes in wall plinth & floor for pipe connections and making good in cement concrete 1:2:4. (A) W.C pan of not less than 23” clear opening between flashing rims and 3 gallons flushing tank. With 4” dia C.I. tape. (S.I.NO.1(A) P.No.1)

Qty: 04 No’s @RS: 5044.60 each RS: 20178/-

(fifty thousands fourty four rups: sixty ps☺

2/- P/F 22”x16” lavatory basin in white glazed earthen ware complete with & i/c the cost of W.I or C.I cantilever brackets 6” built into wall painted white in two coats after a primary coat of red lead paint a pair of ½” dia chrome plate pillar traps 1-1/2” dia rubber plug & chrome plated brass chain 1-1/4” dia malleable iron or c.p brass traps malleable iron or brass union & making requisite number of holes in walls plinth & floor for pipe connection and making good in cement concrete 1:2:4 (standard pattern). Add extra for labour for providing & fixing of earthenware pedestal white or coloured glazed (Standard pattern) (S.I.NO. 8 P. No.3)

Qty: 04 No @RS: 4253.70/- each RS: 17015/-

(Sixty two hundreds thirty seven rupes)

03/- Add: Extra labour for providing and fixing of earthen were pedestal (S.I NO: 9 P-3)

Qty: 04 Nos @RS: 938.47 each RS: 3754/-

04/- P/F Steel stainless local make complete with cast on or wrought bracket 6 inches etc (S.I NO”: 19 P-5).

Qty: 01 NO @RS: 5052.30 each RS: 5050/-

05/- P/F Bath room accessories set 7 pices i/c towel rod brush holder etc complete (S.I NO: P.NO: )

Qty: 04 Nos @RS: 10322.40 each RS: 41289/-

06/- S/F Nyloon connection complete with ½” dia brass stop cock with pair (S.I NO: 23 P-6).

Qty: 08 Nos @RS: 447.15 each RS: 3577/-

07/- S/F Long bib cock of superior quality with crystal C.P Head ½” dia (S.I NO: 3 (b)P-15).

Qty: 09 Nos @RS: 1109.46 each RS: 9985/-

08/- S/F C.P Cancelead stop cock of superior quality (S.I NO: 3 (b0P-15).

Qty: 08 Nos @RS: 337.92 each RS: 2703/-

09/- P/F 6x2 or 6x3 C.I Floor trap of the approves self cleaning desing with a vent etc (S.I NO: 20 P-5).

Qty: 08 Nos @RS: 210.10 each RS: 1681/-

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

10/- S/F Swan type pillar cock of superior qual;ity (S.I NO: P.NO: ).

Qty: 04 Nos @RS: 795/- each RS: 3180/-

11/- Providing & Fixing 4” dia C.I Soil and vent pipes i/c cutting fitting etc complete.

Qty: 100 Rft @RS: 289.25 P.Rft RS: 28925/-

12/- P/F M.S Clamps of the approved design to 4 dial Clipies sockets i/c the cost of cutting fitting etc (S.I NO: 2P-30.)

Qty: 12 Nos @RS: 72.16 each RS: 866/-

13/- P/F 4” Dia C.I Plain bend or the required design etc

Qty: 04 Nos @RS: 566.70 each RS: 2267/-

14/- P/F 4x4x4 dia C.I branch of the required degree with doors rubber washer 1/8” thick (S.I NO: 5 P-8).

Qty: 04 Nos @RS: 271.60 each RS: 1082/-

15/- P/F 4” dia C.I holes rest bend i/c extra painting to match the color of the building (S.I NO: 3 P-8).

Qty: 04 Nos @RS: 212.40 each RS: 850/-

16/- P/F 4” dia C.I Plain band of the required degree with doors rubber washer 1/8” thick (S.I NO: 5 P-8).

Qty: 04 Nos @RS: 176.60 each RS: 706/-

17/- Providing G.I pipes & special etc including fixing cutting and fitting complete with and i/c the cost of cutting trench upto 2-½” feet deep refitting water ramming & disposal of surplus earth with in one chain and painting two coats of bitumen paint to pipe & special after cleaning and cked in maxphalt composition wrapped tightly round pipes & testing to pressure head of etc complete

1-½” Dia Qty: 100 Rft @Rs: 188.97 P.Rft RS: 18897/-

¾” Dia Qty: 200 Rft @RS: 95.20 P.RFt RS:19040/-

1” Dia Qty: 100 Rft @RS: 128.55 P.Rft RS: 12855/-

18/- Add: Extra labour for cancelead G.I pipe and fitting i/c making access in the wall (S.I NO: P.NO ) .

Qty: 200 rft @RS: 3.85 P.Rft RS: 770/-

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

19/- Painting of G-I pipe 02 coats of zink painti.

¾” Dia Qty: 200 Rft @RS: 1.80 P.RFt RS360/-

1-½” Dia Qty: 250 Rft @Rs: 3/- P.Rft RS: 750/-

1”1/4” Dia Qty: 100 Rft @RS: 2.70 P.Rft RS: 750/-

20/- Proviign & Fixing Hnadle valces china 1 ½” dia

1 ½” dia Qty: 02 Nos @RS: 970.92 each RS: 1942/-

¾” Dia Qty: 04 Nos @RS: 227.92 each RS: 912/-

21/- Supplying & fixing Fiber Glass Tank of approved quality and design and wall thickness as specified i/c cost of nuts bolts and fixing in plate form of cement concrete 1:3:6 and making connection for in-let outlet & over flow in-let outlet flow pipes etc. complete. (S.I.No.3 (a) P.No.18) (a) 500 Gallons.

Qty:01 No @Rs:37505/- each RS:37505/-

===================================

Total RS: 233617/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART- C EXTERNAL DEVELOPMENT**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Providing & Fixing R.C.C Pipe Collar glass Band digging the trenches to required depth and fixing in position including cutting , bending & fitting etc complete

9” Dia Qty: 200 rft RS: 163.0 P.Rft RS:32600/-

6” Dia Qty: 100 rft RS: 163/- P.Rft RS:16300/-

4” Dia Qty: 60 rft RS: 130/- P.Rft RS:7800/-

02/- Boring for tube well in all water bearing soils from bound level up to 100 ft: 3/8” meter depth etc

Qty: 60 Rft @RS: 160/- P.Rft RS: 9600/-

03/- Construction of manhole or inspection chamber for the required dia

of circular sewer and 3’-6’ (1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over beching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46).

Qty: 08 Nos @RS: 4905.67 each RS: 39245/-

===================================

Total RS: 105545/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART-D ELECTRIC MOTOR**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

**E-I ITEm**

01/- Supplying & Fixing Motor water pumping set ½” H.P complete

Qty: 02 No RS: 5494.59 each RS: 10989/-

=========================================

Total RS: 10989/-7

**PART- II COMPOUND WALL**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 1219 Cft @RS:3176.25 % Cft RS:3872/-

Thirty one hundred seventy six rups:twenty five ps:

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 609 Cft @RS: 8694.95 % Cft RS:52952/-

(Eight six hundreds ninty four rupees,ninty five ps:)

03/- Un- Coursed rubble masonry dressing dry masonry (S.I No:1 P-27).

Qty: 450 Cft @RS: 17723/- % Cft RS: 79754/-

(Seventeen thousands seven hundreds twenty three rup:)

04/- Coursed Rubble Masnory 1:6 including hammer dressing (S.I No: 2 d P.26).

Qty: 678 Cft @RS: 25321/- % Cft RS: 171676/-

(twenty five thousands three hundreds te=wenty one rups:)

05/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 1303cft @RS: 337/- P.Cft RS: 102111/-

(Three hudred thirt seven ps.)

06/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 13.526cwt @RS:5001.70 P.cwt RS:67653/-

(Five thousands & one ripes, seventy ps:)

07/- Pacca Brick work in Other than building 1:6 (S.I No:7 eP-21).

Qty: 1312 cft @RS: 12346.65 % Cft RS: 161988/-

(Tweleve thousands three hundred fourty six rups: sixty fiveps.)

08/- Cement Plaster 1:6 up to 20’-0 height ½” thick. (S.I NO: 13(b) P: NO:52 )

Qty:2198 Sft @RS: 2206.60 % Sft RS: 48501/-

(Twenty two hundreds six rupees, sixty ps.)

09/- Cement Plaster 1:4 up to 20”-0 heights 3/8” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2198 Sft @RS: 2197.52 % Sft RS: 48301/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

10/- Cement Pointing on Stone work etc (S.I NO: P.NO: )

Qty: 1400 Sft @RS: 1213.58 % Sft RS: 16990/-

(tweleve hundreds thirteen rups: fifty eight ps:)

11/- Making & Fixing Steel grated door with 1/16” thick sheeting including angle iron frame 2”x2”x3/” and square bars 4” center to center with locking arrangement .(S.I NO:24)P.NO:92

Qty: 70 sft @RS: 726.72 P.Sft RS: 50870/-

(seven hundred twenty six rupes, seventy two ps.)

12/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty: 140 Sft @RS: 2116.41 % Sft RS: 2963/-

(twenty one hundred sixteen rupees, fourty one ps.)

13/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 2198 Sft @RS: 442.75 P.Sft RS: 9732/-

(Four hundred fourty two rupees, seventy five ps.)

14/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 2198 Sft @RS: 1043.90 % Sft RS; 22945/-

(ten hundreds fourty three rupees , Ninty ps.)

==================================

**Total RS: 840308/-**

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART- RESIDENTIAL BUILDING SCHEDULE-B-**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 3935 Cft @RS:3176.25 % Cft RS:12499/-

Thirty one hundred seventy six rups:twenty five ps:

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 941 Cft @RS: 8694.95 % Cft RS:88607/-

(Eight six hundreds ninty four rupees,ninty five ps:)

03/- Pacca Brick work in foundation / Plint in cement

cement & sand mortar ratio (1:6)(S.I No:05 (c)P.No:20)

Qty: 1598 Cft @RS: 11948.36 % Cft RS:190935/-

(Eleven thousands nine hundered fourty eight rs: thirty six ps.)

04/- Cement Concrete plain including placing Compacting

Finishing & curing, complete i/c screening & washing

Of stone aggregate Ratio (1:3:6) (S.I No:5 P-18).

[

Qty: 1035 cft @RS: 12695.0 % Cft RS: 131393/-

( fourteen thousands four hundreds twenty nine rupes twenty five ps:)

05/- Errection & Removal & Centering (S.I NOO: 18(b)P-21).

Qty: 1380 sft @RS: 3588.48 % Sft RS: 49521/-

(thirty five hundreds eighty eight rupes: fourty eight ps:)

06/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 2582cft @RS: 337/- P.Cft RS: 870134/-

(Three hudred thirt seven ps.)

07/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 115.267 cwt @RS:5001.70 P.cwt RS:576531/-

(Five thousands & one ripes, seventy ps:)

08/- Pacca Brick work in Ground Floor in cement sand mortarRatio (1:6) (S.I No:5 P-25).

Qty: 3923 Cft @RS: 12674.65 % Cft RS: 497215/-

(Tweleve thousands six hundred seventy four rupees, sixty five ps.)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

09/- Cement Plaster 1:6 up to 20’-0 height ½” thick. (S.I NO: 13(b) P: NO:52 )

Qty: 8638 Sft @RS: 2206.60 % Sft RS: 190606/-

(Twenty two hundreds six rupees, sixty ps.)

10/- Cement Plaster 1:4 up to 20”-0 heights 3/8” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 8638 Sft @RS: 2197.52 % Sft RS: 189822/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

11/- Filling watering & ramming earth from foundation lead up to one chain lift up to 5 feet (S.I NO: P.NO: ).

Qty: 2070 cft @RS: 1512.60 %0cft RS: 3131/-

(Fifteen hundred tweleve rupess, sixty ps:)

12/- Supplying Sand under floor plugging into wall (S.I NO: 29 P.NO: 26)

Qty: 3377 cft @RS: 1141.25 % Cft RS: 38540/-

(Eleven hundred fourty one rupees, twenty five ps.)

13/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 513 Cft @RS: 8694.95 % Cft RS:44605/-

(Eight six hundreds ninty four rupees,ninty five ps:)

14/- Cement Concrete plain including placing Compacting

Finishing & curing, complete i/c screening & washing

Of stone aggregate Ratio (1:2:4) (S.I No:5 P-18).

[

Qty: 265 cft @RS: 14429.25 % Cft RS:38238/-

( fourteen thousands four hundreds twenty nine rupes twenty five ps:)

15/- Laying white marble fine dressed in the surface without winding set in lime mortar 1:2 i/c rubbing and polishing pf the joints (a) ¾” thick flooring. (S.I.NO.28 (a) Page No. 43)

Qty: 1416 Sft @RS: 567.48 P.Sft RS: 674746/-

(five hundreds sixty seven rupees fourty eight ps:)

16/- Providing and fixing 3/8" thick marble tiles of approved quality and colour and shade size 8" x 4" /6" x 4" in dado skirting anf facing removal /tucking of existing plaster surface ete. Over 1/2" thick base of cement mortar 1:3 setting of tiles in slurry of white cement over mortar base including filling the joints and washing the tiles with white cement slurry , currint finishing, cleaning and ploishing etc. complete.(S.I NO: 68 P.NO: 49)

Qty: 579 Sft @RS: 186.04 P.Sft RS: 107717/-

(One hundred eighty six rupees four ps:)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

17/- Providing & Laying tiles glazed 6”x6”x1/4” on floor or wall facing in required color & pattern od STILE specification jointed in white cement & pigment over a base of 1:2 grey cement mortar ¾” thick including washing & filling or joints with slurry of white cement and pigment in desired shape with finishing cleaning and cost of wax polish etc. complete including cutting tiles to proper profile (S.I No:61 P.NO:480)

Qty: 744 sft @RS: 28253.61 % Sft RS:210207/-

(twenty eight thousands two hundreds fifty thre rps: sixty one ps)

18/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for window using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 116 Rft @RS: 240.50 P.Rft RS: 27848/-

(Two hundred fourty rupees, fifty ps.)

19/- roviding & Fixing Wire gauze fixed to chowakats etc complete.

Qty: 168 Sft @RS: 190.72 P.Sft RS: 32041/-

(One hundred ninty rupees seventy two ps:)

20/- Providing & Fixing R.C.C Spouts fixing in position.

Qty: 08 No’s @RS: 261.25 each RS: 2090/-

(Two hundreds sixity one rupees twenty five ps:)

21/- Supplying & Fixing Khapriel (S.I NO: 39P-40).

Qty: 84 sft @RS: 8977.90 % Sft RS: 7541/-

(eight thousands nine hundreds seventy seven rups: ninty ps☺

22/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 6942 Sft @RS: 442.75 P.Sft RS: 30736/-

(Four hundred fourty two rupees, seventy five ps.)

23/- Preparing the surface painting with matt finish i/c rubbing the surface with bath (Slicon carbide rubbing etc (S.I NO: 36P-61).

Qty: 6942 sft @RS: 1989.62 % Sft RS: 138119/-

24/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 1556 Sft @RS: 1043.90 % Sft RS; 16243/-

(ten hundreds fourty three rupees , Ninty ps.)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

25/- Providing and lying 1” thick C/C topping cement concrete (1:2:4) i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.42).(2” thick).

Qty: 2226 sft @RS: 3275.50 % Sft RS: 72913/-

(fourty four hundreds eleven rupees eighty two ps:)

26/- Two coats of Bitumen hot using 34 Lbs (S.I NO: P.NO: ).

Qty: 2226 Sft @RS: 1887.04 % Sft RS: 42014/-

(eighteen hundreds eighty seven rupees four ps:)

27/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty: 640 Sft @RS: 2116.41 % Sft RS: 13545/-

(Twenty one hundred sixteen rupees, fourty one ps.)

28/- Providing & Fixing Plaster of Pairis ceiling Border of 8”x10” with of specified design etc complete(S.I NO: P.NO ).

Qty: 579 rft @RS: 104.22 P.Rft RS: 60343/-

(One hundred four rupees twenty two ps:)

29/- S/F Grop[hy/Natural work Texture coating to period juarable coursed to wall thickness between 2 mm to 32 mm 1/8” wash aerlic-co polynem emulsion etc

Qty: 720 sft @RS: 80/- P.Sft RS: 57600/-

==================================

**Total RS: 4415472/-**

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

**PART- W/S & S/F Mukhtiar kar office wash room**

01/- P/F squatting type white glazed of flushing cistern with internal fitting and flush pipe with band and making requisite Nos. of holes in wall plinth & floor for pipe connections and making good in cement concrete 1:2:4. (A) W.C pan of not less than 23” clear opening between flashing rims and 3 gallons flushing tank. With 4” dia C.I. tape. (S.I.NO.1(A) P.No.1)

Qty: 04 No’s @RS: 5044.60 each RS: 20178/-

(fifty thousands fourty four rups: sixty ps☺

2/- P/F 22”x16” lavatory basin in white glazed earthen ware complete with & i/c the cost of W.I or C.I cantilever brackets 6” built into wall painted white in two coats after a primary coat of red lead paint a pair of ½” dia chrome plate pillar traps 1-1/2” dia rubber plug & chrome plated brass chain 1-1/4” dia malleable iron or c.p brass traps malleable iron or brass union & making requisite number of holes in walls plinth & floor for pipe connection and making good in cement concrete 1:2:4 (standard pattern). Add extra for labour for providing & fixing of earthenware pedestal white or coloured glazed (Standard pattern) (S.I.NO. 8 P. No.3)

Qty: 04 No @RS: 4253.70/- each RS: 17015/-

(Sixty two hundreds thirty seven rupes)

03/- P/F Steel stainless local make complete with cast on or wrought bracket 6 inches etc (S.I NO”: 19 P-5).

Qty: 01 NO @RS: 5052.30 each RS: 5050/-

04/- Add: Extra labour for providing and fixing of earthen were pedestal (S.I NO: 9 P-3)

Qty: 04 Nos @RS: 938.47 each RS: 3754/-

05/- S/Fixing C.P Mulsim Shower etc complete

Qty: 03 Nos @RS: 715/- each RS: 2145/-

06/- S/Fixing Surgical Pillar cock etc

Qty: 04 NOs @RS: 1859/- each RS: 7436/-

07/- S/F Nyloon connection complete with ½” dia brass stop cock with pair (S.I NO: 23 P-6).

Qty: 08 Nos @RS: 447.15 each RS: 3577/-

08/- S/F Long bib cock of superior quality with crystal C.P Head ½” dia (S.I NO: 3 (b)P-15).

Qty: 08 Nos @RS: 1109.46 each RS: 8876/-

09/- Providing & Fixing Chrome plated brass towel rail complete

Qty: 03 Nos @RS: 232.10 each RS: 696/-

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

10/- Providing G.I pipes & special etc including fixing cutting and fitting complete with and i/c the cost of cutting trench upto 2-½” feet deep refitting water ramming & disposal of surplus earth with in one chain and painting two coats of bitumen paint to pipe & special after cleaning and cked in maxphalt composition wrapped tightly round pipes & testing to pressure head of etc complete

¾” Dia Qty:70 Rft @RS: 95.20 P.RFt RS:3856/-

1” Dia Qty: 30 Rft @RS: 128.55 P.Rft RS: 6664/-

11/- Add: Extra labour for cancelead G.I pipe and fitting i/c making access in the wall (S.I NO: P.NO ) .

¾” Dia Qty: 70 rft @RS: 3.85 P.Rft RS: 115/-

1” Dia Qty: 30 Rft @RS: 8.85 P.Rft RS: 620/-

12/- P/F 6x2 or 6x3 C.I Floor trap of the approves self cleaning desing with a vent etc (S.I NO: 20 P-5).

Qty: 08 Nos @RS: 244.35 each RS: 1955/-

13/- Proviign & Fixing Hnadle valces china 1 ½” dia

1 ½” dia Qty: 02 Nos @RS: 970.92 each RS: 1942/-

14/- P/F 4x4x4 dia C.I branch of the required degree with doors rubber washer 1/8” thick (S.I NO: 5 P-8).

Qty: 06 Nos @RS: 271.60 each RS: 1624/-

15/- Providing & Fixing Piston Pump set 1 H.P Single Phase 220 volts etc

Qty:01 No @RS: 5494.59 each RS: 5495/-

16/- Supplying & fixing Fiber Glass Tank of approved quality and design and wall thickness as specified i/c cost of nuts bolts and fixing in plate form of cement concrete 1:3:6 and making connection for in-let outlet & over flow in-let outlet flow pipes etc. complete. (S.I.No.3 (a) P.No.18) (a) 500 Gallons.

Qty:02 No @Rs:37505/- each RS:75010/-

17/- Providing Set 3 H.P (S.I NO: 4 P-29).

Qty: 02 Nos @RS: 22691.35 each RS: 45383/-

===================================

Total RS: 221042/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

PART- P.H.Engineering Schedule.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Providing Asbestive pipe with Collar deed or equivalent i/c digging the trenches to required depth and fixing to position and jointing with rubber etc complete

Qty: 30 Rft` @RS: 663/- P.Rft RS: 19890/-

02/- Construction of manhole or inspection chamber for the required dia

of circular sewer and 3’-6’(1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over beching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46).

Qty: 10 Nos @RS: 1680595 each RS: 168059/-

03/- Providing RCC Pipe with Collar Class “B” and digging the trenches to required depth and fixing in position i/c cutting fitting & jointing etc complete

9” Dia Qty: 150 Rft @RS: 113.97 P.Rft RS: 17095/-

6” Dia Qty: 50 Rft @RS: 72.40 P.Rft RS: 3620/-

===================================

Total RS: 208664/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART- II COMPOUND WALL**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 1219 Cft @RS:3176.25 % Cft RS:3872/-

Thirty one hundred seventy six rups:twenty five ps:

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 609 Cft @RS: 8694.95 % Cft RS:52952/-

(Eight six hundreds ninty four rupees,ninty five ps:)

03/- Un- Coursed rubble masonry dressing dry masonry (S.I No:1 P-27).

Qty: 450 Cft @RS: 17723/- % Cft RS: 79754/-

(Seventeen thousands seven hundreds twenty three rup:)

04/- Coursed Rubble Masnory 1:6 including hammer dressing (S.I No: 2 d P.26).

Qty: 678 Cft @RS: 25321/- % Cft RS: 171676/-

(twenty five thousands three hundreds te=wenty one rups:)

05/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 1303cft @RS: 337/- P.Cft RS: 102111/-

(Three hudred thirt seven ps.)

06/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 13.526cwt @RS:5001.70 P.cwt RS:67653/-

(Five thousands & one ripes, seventy ps:)

07/- Pacca Brick work in Other than building 1:6 (S.I No:7 eP-21).

Qty: 1312 cft @RS: 12346.65 % Cft RS: 161988/-

(Tweleve thousands three hundred fourty six rups: sixty fiveps.)

08/- Cement Plaster 1:6 up to 20’-0 height ½” thick. (S.I NO: 13(b) P: NO:52 )

Qty:2198 Sft @RS: 2206.60 % Sft RS: 48501/-

(Twenty two hundreds six rupees, sixty ps.)

09/- Cement Plaster 1:4 up to 20”-0 heights 3/8” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2198 Sft @RS: 2197.52 % Sft RS: 48301/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

10/- Cement Pointing on Stone work etc (S.I NO: P.NO: )

Qty: 1400 Sft @RS: 1213.58 % Sft RS: 16990/-

(tweleve hundreds thirteen rups: fifty eight ps:)

11/- Making & Fixing Steel grated door with 1/16” thick sheeting including angle iron frame 2”x2”x3/” and square bars 4” center to center with locking arrangement .(S.I NO:24)P.NO:92

Qty: 70 sft @RS: 726.72 P.Sft RS: 50870/-

(seven hundred twenty six rupes, seventy two ps.)

12/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty: 140 Sft @RS: 2116.41 % Sft RS: 2963/-

(twenty one hundred sixteen rupees, fourty one ps.)

13/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 2198 Sft @RS: 442.75 P.Sft RS: 9732/-

(Four hundred fourty two rupees, seventy five ps.)

14/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 2198 Sft @RS: 1043.90 % Sft RS; 22945/-

(ten hundreds fourty three rupees , Ninty ps.)

==================================

**Total RS: 840308/-**

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

**PART- C EXTERNAL DEVELOPMENT**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

01/- Pacca Brick work in foundation / Plint in cement

cement & sand mortar ratio (1:6)(S.I No:05 (c)P.No:20)

Qty: 8235 Cft @RS: 11948.36 % Cft RS:93982/-

(Eleven thousands nine hundered fourty eight rs: thirty six ps.)

02/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:6:12). (S.I.No.4 (b) P.No.14)

Qty: 1087 cft @RS: 8122.95 % Cft RS: 88296/-

( eight thousands one hundreds twenty two rupees ninty five ps:)

03/- Cement Concrete plain including placing Compacting

Finishing & curing, complete i/c screening & washing

Of stone aggregate Ratio (1:3:6) (S.I No:5 P-18).

[

Qty: 1087 cft @RS: 12695.0 % Cft RS: 137995/-

( fourteen thousands four hundreds twenty nine rupes twenty five ps:)

03/- P/F cement paving blocks flooring having size of 197x97x80(mm)of cuty/ quddra / cobble shape with natural colours, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc. complete. (S.I. No.74 P. No.50).

Qty: 3294 Sft @RS: 223.97 P.Sft RS:737757/- (two hundreds twenty three rupees ninty seven ps:)

===================================

Total RS: 1058030/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR