**SCHEDULE-B**

**PROVIDING OF PAVER BLOCK FOR SINDHI KARBALLA NEAR OLD NHW TALUKA & DISTRICT KHAIRPUR.**

**PART-A COMPOUND WALL**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SR NO.** | **ITEM OF WORKS** | | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| **01.** | Excavation in foundation of buildings bridges and other structures including dag belling dressing refilling around structure with excavated earth watering and ramming lead upto 5ft. (b) in ordinary soil. (S.I.No.18 P.No.5). | | **2529.00** | **3176/25** | **%0Cft** | **Rs.8033/-** |
|  |  |  |  |  |  |  |
| **02.** | Cement concrete brick or stone ballast 1-1/2 to 2”gauge. Ratio 1:5:10. (S.I.No.4 P.No.17). | | **843.00** | **8694/95** | **%Cft** | **Rs.73298/-** |
|  |  |  |  |  |  |  |
| **03.** | Pacca Brick work in foundation & plinth in cement & sand mortar Ratio 1:6 (S.I.No.4 (c) P.No.25). | | **3175.00** | **11948/36** | **%Cft** | **Rs.379379/-** |
|  |  |  |  |  |  |  |
| **04.** | Supplying and filling sand under floor and plugging in walls.(S.I.No.29 P.No.31). | | **35685.00** | **1141/25** | **%Cft** | **Rs.407255/-** |
|  |  |  |  |  |  |  |
| **05.** | Add extra lead for 3”miles. | | **35685.00** | **579/41** | **%Sft** | **Rs.206762/-** |
|  |  |  |  |  |  |  |
| **06.** | Dressing & leveling of earth work to designed section etc complete in ordinary soil (S.I.No.24 P.No.46). | | **35685.00** | **187/55** | **%0Cft** | **Rs.6693/-** |
|  |  |  |  |  |  |  |
| **07.** | Cement concrete brick or stone ballast 1 ½” to 20 gauge ratio 1:6:12. (S.I.No.21 P.NO.56). | | **4715.00** | **8122/95** | **%Cft** | **Rs.382997/-** |
|  |  |  |  |  |  |  |
| **08.** | Cement concrete plain including placing compacting finishing and curing, complete (including screening and washing of stone aggregate without shuttering Ratio 1:2:4. (S.I.No.05 P.No.18). | | **1603.00** | **14429/25** | **%Cft** | **Rs.231300/-** |
|  |  |  |  |  |  |  |
| **09.** | P/F cement paving block flooring having size of 197x97x80(mm) of city/quid/cobble shape with painted having strength b/w 5000psi 8500 phi i/c filling the joints with hill sand and laying in specified manner/patter and design etc complete. (S.I.No.74 P.No.56). | | **5630.00** | **223/97** | **P-Sft** | **Rs.1260951/-** |
|  |  |  |  |  |  |  |
| **10.** | Coursed fine builds grated as sand (S.I.No.51 P.No.04). | | **2358.00** | **2500/-** | **%Cft** | **Rs.58950/-** |
|  |  |  |  |  |  |  |
| **11.** | Cement plaster 1:6 upto 20 height ½ thick. (S.I.No.13 P.No.58). | | **5620.00** | **2206/60** | **%Sft** | **Rs.124011/-** |
|  |  |  |  |  |  |  |
| **12.** | Cement plaster 1:4 upto 20 height 3/8 thick. (S.I.No.11 P.No.58). | | **5620.00** | **2197/52** | **%Sft** | **Rs.123500/-** |
|  |  |  |  |  |  |  |
|  |  |  | **TOTAL** | | | **Rs.3263129/-** |

% Above/Below (Amount to be added/deducted).Rs.

**Grand Total** Rs.

Total Amount in word:

**Note:-** Quantities and rates may be changed as per/according to the Technical Sanction by the competent authority.

|  |  |
| --- | --- |
| **CONTRACTOR** | **EXECUTIVE ENGINEER**  (BUILDINGS) WORKS & SERVICES  DEPARTMENT KHAIRPUR |