**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER AT RAJA COLONY DAHARKI.**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 43950.00 | 2117.50 | %ocft | 93064/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 43950.00 | 502/32 | %ocft | 220770/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 43950.00 | 354.00 | %ocft | 15558/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 7325.00  732.50 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 826901/00  105694/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 1465.00 | 3127/41 | P%sft. | 45817/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 4981.00 | 2500/00 | P%cft | 124525/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 29300.00 | 199.77 | P.sft | 5853261/00 |
|  |  |  | **Total.** |  | **7285590/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Excavation in foundation of building bridges and other structures i/c belling dressing filling around the structure with excavated earth watering ramming lead upto one chain and lift upto 5ft.CSI No> 18 P.No.4). | 2407.50 | 3176/25 | %ocft | 7647/00 |
| 2. | CC Plain i./c placing compacting finishing and curing complete i/c screenings and washing of stone aggregate without shuttering CSI No> 5 P.17). | 677.50  71.54 | 11288/75  14429.25 | 1:$:8  %cft  1;2:4  %cft | 76481/00  10323/00 |
| 3. | Construction of standard open drain cunnet block of CC 1:2:4 I/AC SITU TO THE DESIGN PROFILE EII./C COST OF MATERIAL I/CS PER DRAWING I/C SUPPLYING FILLING COST OF CEMENT 1/22” THICK | 500.00  500.00 | 94/00  174/00 | P.rft.  P.rft. | 47000/00  87000/00 |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 1875.00 | 11948/36 | P%cft. | 224032/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 2750.00 | 2283/93 | P.%cft/ | 62808/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 105.50 | 337/00 | P.cft. | 35554/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 3.76 | 4820/20 | P.cwt. | 18806/00 |
|  |  | **Total.** |  |  | **550845/00** |

**ABSTRACT.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| 1 | Part-I CC Paver | 7285590/00 |  | 7285590/00 |
| 2 | Part-II Drains. | **550845/00** |  | **550845/00** |
|  | Total. | 7836435/00 |  | 7836435/00 |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER AT VILLAGE MOHAMMAD**

**YOUSUF RID.**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 9150.00 | 2117.50 | %ocft | 19375/- |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 9150.00 | 502/52 | %ocft | 45980/- |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 9150.00 | 354.00 | %ocft | 3239/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 1525.00  152.50 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 172153/00  22005/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 305.00 | 3127/41 | P%sft. | 9539/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 1037.00 | 2500/00 | P%cft | 25925/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 6100.00 | 199.77 | P.sft | 1218597/00 |
|  |  |  | **Total.** |  | **1516813/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Excavation in foundation of building bridges and other structures i/c belling dressing filling around the structure with excavated earth watering ramming lead upto one chain and lift upto 5ft.CSI No> 18 P.No.4). | 181.50 | 3176/25 | %ocft | 576/00 |
| 2. | CC Plain i./c placing compacting finishing and curing complete i/c screenings and washing of stone aggregate without shuttering CSI No> 5 P.17). | 60.50  6.38 | 11288/75  14429.25 | 1:$:8  %cft  1;2:4  %cft | 6830/00  921.00 |
| 3. | Construction of standard open drain cunnet block of CC 1:2:4 I/AC SITU TO THE DESIGN PROFILE EII./C COST OF MATERIAL I/CS PER DRAWING I/C SUPPLYING FILLING COST OF CEMENT 1/22” THICK | 100.00 | 94/00 | P.rft. | 9400/00 |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 150.00 | 11948/36 | P%cft. | 17923/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 250.00 | 2283/93 | P.%cft/ | 5710/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 24.20 | 337/00 | P.cft. | 8155/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 0.92 | 5001/70 | P.cwt. | 4852/00 |
|  |  | **Total.** |  |  | **54867/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **1516813/00** |  | **1516813/00** |
| **2** | **Part-II Drains.** | **54867/00** |  | **54867/00** |
|  | **Total.** | **1571680/00** |  | **1571680/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER FROM G.T. ROAD DEGFREE**

**COLLEGE TO DARGAH SAYED BACHAL SHAH BUKHARI**

**MIRPUR MATHELO.**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 14400.00 | 2117.50 | %ocft | 30492/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 14400.00 | 502/52 | %ocft | 72362/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 14400.00 | 354.00 | %ocft | 5098/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 2400.00  200.00 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 270930/00  28859/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 400.00 | 3127/41 | P%sft. | 12510/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 1632.00 | 2500/00 | P%cft | 40800/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 9200.00 | 199.77 | P.sft | 1837884/00 |
|  |  |  | **Total.** |  | **2298935/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 487.50 | 11948/36 | P%cft. | 58248/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 950.00 | 2283/93 | P.%cft/ | 21697/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 55.04 | 337/00 | P.cft. | 18548/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 2.21 | 5001/70 | P.cwt. | 11054/00 |
|  |  | **Total.** |  |  | **109547/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **2298935/00** |  | **2298935/00** |
| **2** | **Part-II Drains.** | **109547/00** |  | **109547/00** |
|  | **Total.** | **2408482/00** |  | **2408482/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER CHOHAN MOHALLAH VARIOUS STREETS**

**MIRPUR MATHELO**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 23542.50 | 2117.50 | %ocft | 49851/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 23542.50 | 502/52 | %ocft | 118305/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 23542.50 | 354.00 | %ocft | 8334/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 3923.75  341.25 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 442942/00  49240/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 682.50 | 3127/41 | P%sft. | 21345/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 2668.15 | 2500/00 | P%cft | 66704/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 15517.50 | 199.77 | P.sft | 3099931/00 |
|  |  |  | **Total.** |  | **3856652/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1. | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 513.75 | 11948/36 | P%cft. | 61385/00 |
| 2 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 887.50 | 2283/93 | P.%cft/ | 20270.00 |
| 3 | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 59.04 | 337/00 | P.cft. | 19896/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 2.37 | 5001/70 | P.cwt. | 11854/00 |
|  |  | **Total.** |  |  | **113405/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **3856652/00** |  | **3856652/00** |
| **2** | **Part-II Drains.** | **3856652/00** |  | **3856652/00** |
|  | **Total.** | **3970057/00** |  | **3970057/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER AT VILLAGE ABDULLAH**

**RAJRI VARIOUS STREET.**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 40200.00 | 2117.50 | %ocft | 85124/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 40200.00 | 502/32 | %ocft | 201933/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 40200.00 | 354.00 | %ocft | 14231/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 6700.00  670.00 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 756346/00  96676/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 1340.00 | 3127/41 | P%sft. | 41907/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 4556.00 | 2500/00 | P%cft | 113900/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 26800/00 | 199.77 | P.sft | 5353836/00 |
|  |  |  | **Total.** |  | **6663953/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Excavation in foundation of building bridges and other structures i/c belling dressing filling around the structure with excavated earth watering ramming lead upto one chain and lift upto 5ft.CSI No> 18 P.No.4). | 1444.50 | 3176/25 | %ocft | 4588/00 |
| 2. | CC Plain i./c placing compacting finishing and curing complete i/c screenings and washing of stone aggregate without shuttering CSI No> 5 P.17). | 406.50  71.54 | 11288/75  14429.25 | 1:$:8  %cft  1;2:4  %cft | 45889/00  10323/00 |
| 3. | Construction of standard open drain cunnet block of CC 1:2:4 I/AC SITU TO THE DESIGN PROFILE EII./C COST OF MATERIAL I/CS PER DRAWING I/C SUPPLYING FILLING COST OF CEMENT 1/22” THICK | 300.00  300.00 | 94/00  174/00 | P.rft.  p.RFT. | 28200/00  52200/00 |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 1125.00 | 11948/36 | P%cft. | 134419/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 1650.00 | 2283/93 | P.%cft/ | 37685/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 105.50 | 337/00 | P.cft. | 35554/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 3.76 | 5001/70 | P.cwt. | 18806/00 |
|  |  | **Total.** |  |  | **367664/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **6663953/00** |  | **6663953/00** |
| **2** | **Part-II Drains.** | **367664/00** |  | **367664/00** |
|  | **Total.** | **7031617/00** |  | **7031617/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’**

**Name of Work:- CONSTRUCTION OF C.C. PAVER AT VILLAGE SAMANDAR KHAN BHAYO**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 4005.00 | 2117.50 | %ocft | 8981/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 4005.00 | 502/52 | %ocft | 20126/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 4005.00 | 354.00 | %ocft | 1418/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 667.50  66.75 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 75352/00  9632/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 133.50 | 3127/41 | P%sft. | 4175/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 453.90 | 2500/00 | P%cft | 11348/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 2670.00 | 199.77 | P.sft | 533386/00 |
|  |  |  | **Total.** |  | **663918/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Excavation in foundation of building bridges and other structures i/c belling dressing filling around the structure with excavated earth watering ramming lead upto one chain and lift upto 5ft.CSI No> 18 P.No.4). | 453.75 | 3176/25 | %ocft | 1441/00 |
| 2. | CC Plain i./c placing compacting finishing and curing complete i/c screenings and washing of stone aggregate without shuttering CSI No> 5 P.17). | 151.25  6.38 | 11288/75  14429.25 | 1:$:8  %cft  1;2:4  %cft | 17074/00  921/00 |
| 3. | Construction of standard open drain cunnet block of CC 1:2:4 I/AC SITU TO THE DESIGN PROFILE EII./C COST OF MATERIAL I/CS PER DRAWING I/C SUPPLYING FILLING COST OF CEMENT 1/22” THICK | 250.00 | 94/00 | P.rft. | 23500.00 |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 375.00 | 11948/36 | P%cft. | 44806/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 625.00 | 2283/93 | P.%cft/ | 14275/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 24.20 | 337/00 | P.cft. | 8155/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 0.97 | 5001/70 | P.cwt. | 4852/00 |
|  |  | **Total.** |  |  | **115024/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **663918/00** |  | **663918/00** |
| **2** | **Part-II Drains.** | **115024/00** |  | **115024/00** |
|  | **Total.** | **778942/00** |  | **778942/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

**SCHEDULE ‘B’.**

**Name of Work:- CONSTRUCTION OF C.C. PAVER AT JAM ZAFAR MOHALLAH DAHARKI.**

**Head of Account. Community Development Programme 2016-17.**

**Part-I.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Barrow pit excavation undressed lead upto 100 ft ( in ordinary soil CSI NO. 1 P.No> 1). | 43950.00 | 2117.50 | %ocft | 93064/00 |
| 2 | Carriage of earth (CSI NO> 8 P.No> 02 | 43950.00 | 502/32 | %ocft | 220770/00 |
| 3 | Laying earth in 6 Layers leveling dressing and watering for compaction etc complete (CSI No. P.No> ). | 43950.00 | 354.00 | %ocft | 15558/00 |
| 4 | Cement concrete PLAIN I/C PLACING COMPACTING FINISHING & curring complete including screening and washing of stone aggregate without shuttering CSI No> 5 P.No>< 16 | 7325.00  732.50 | 11288.75  1429/25 | 1:4:8  %cft  1:2:4 P.%sft. | 826901/00  105694/00 |
| 5 | Errection and removal of centering for RCC plain cc work of partial wood CSI No> 18 P.No> 21). | 1465.00 | 3127/41 | P%sft. | 45817/00 |
| 6 | Crushed fire bricks graded as sand (SMINO<> 51 P,No, 78), | 4981.00 | 2500/00 | P%cft | 124525/00 |
| 6 | Providing and fixing cement paving blocks flooring having size of 197 x97x80 mm of city /qudda / cobble shape with natural color having strength between 5000 spsi to 8500 psi i/c filling the joints with hil sand and laying in specified manner pattern and design etc complete (CSI NO. 71 P.No. 49)., | 29300.00 | 199.77 | P.sft | 5853261/00 |
|  |  |  | **Total.** |  | **7285590/00** |

**Part-II Surface Drains.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Item of work** | **Qty** | **Rate** | **Unit** | **Amount.** |
| 1 | Excavation in foundation of building bridges and other structures i/c belling dressing filling around the structure with excavated earth watering ramming lead upto one chain and lift upto 5ft.CSI No> 18 P.No.4). | 2407.50 | 3176/25 | %ocft | 7647/00 |
| 2. | CC Plain i./c placing compacting finishing and curing complete i/c screenings and washing of stone aggregate without shuttering CSI No> 5 P.17). | 677.50  71.54 | 11288/75  14429.25 | 1:$:8  %cft  1;2:4  %cft | 76481/00  10323/00 |
| 3. | Construction of standard open drain cunnet block of CC 1:2:4 I/AC SITU TO THE DESIGN PROFILE EII./C COST OF MATERIAL I/CS PER DRAWING I/C SUPPLYING FILLING COST OF CEMENT 1/22” THICK | 500.00  500.00 | 94/00  174.00 | P.rft.  p.RFT. | 47000/00  87000/00 |
| 4 | Pacca briuck work in foundation and plinth in cement sand mortor 1:6 (CSI NO> 4 P.No> 24). | 1875.00 | 11948/36 | P%cft. | 224032/00 |
| 5 | Cement plaster 1:4 upto 20’height i/c “ thick CSI NO> 11 P.No> 57). | 2750.00 | 2283/93 | P.%cft/ | 62808/00 |
| 6. | RCC work in roof slabs beams columns rafts lintels and other structure members laid in situ or precast laid in position etc complete in all respect ratio 1:2:4 (CSI NO. 6 P.No. 18). | 105.50 | 337/00 | P.cft. | 35554/00 |
| 7 | Fabrication of mild steel reinforcement for cement concretes i/.c cutting bending laying in position making points and fastening i/c cost of b including wire also i/cs removal of rust from bars CSI No. 7 P.No. 19). | 3.76 | 5001/70 | P.cwt. | 18806/00 |
|  |  | **Total.** |  |  | **550845/00** |

ABSTRACT.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Item of work | Schedule ‘B’ | Non Schedule Items | Amount. |
| **1** | **Part-I CC Paver** | **7285590/00** |  | **7285590/00** |
| **2** | **Part-II Drains.** | **550845/00** |  | **550845/00** |
|  | **Total.** | **7836435/00** |  | **7836435/00** |

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.

CONDITIONS.

1. The work shall have to bexecuted according to PWD/PHE specifications.
2. No premium on non schedule items shall be allowed to the contractors.
3. Any error or omission in the description of item of work and the rate shall be governed with the relevant schedule of rates and estimates.
4. The contractor shall have to bring the material to be used from the quarries mentioned in the estimate.

Contractor. Executive Engineer

Public Health Engg. Division Ghotki

@ Mirpur Mathelo.