Name of work: M/R to Chief Minister House Karachi (PWD Office ) (Electric Work)

Schedule B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.No. | Description | Qty | Rate | Unit | Amount |
| 1 | Wiring for light or fan point with 3/029 PVC insulated wire in 20mm (3/4)channel patti on surface as required.(S.I.129/18) | 30-Nos | 910/- | P.pts | 27300 |
| 2 | Wiring for Plug point with 3/029 PVC insulated wire in 20mm (3/4)channel patti on surface as required.(S.I.134/15) | 15-Nos | 742/- | P.Pts | 11130 |
| 3 | P/F Circuit Brackers ,15,20, 30,40,50 60,&75&100 amps TP (XS-100NS) on a prepared board as required.(S.I.207/31) | 1-Nos | 9261/- | P.No. | 9261 |
| 4 | P/F Circuit Brackers 6,10,15,20, 30,40,50 & 63 amps SP (TB SS) on a prepared board as required.(S.I.203/31) | **18-Nos** | **916/-** | P.No. | **16488** |
| 5 | P/L main or Sub main PVC insulated with size 2-7/029 (6mm2) copper conductor in 1” dia PVC conduit on surface.(S.I.5/1) | 100-Meter | 222/- | P.Meter | 22200 |
| 6 | P/L main or Sub main PVC insulated with size 2-7/044 (6mm2) copper conductor in 1” dia PVC conduit on surface.(S.I.5/1) | 80.00 | 305/- | P.Meter | 24400 |
|  | Total |  |  |  | 110779 |
|  | Part B NSI |  |  |  |  |
| 1 | P/F Distribution board double shutter size (1-1/2”x1-1/4”) to accommodate heavy duty for Circuit Brackers i/c painting enameled paint for other similar job on prepared board on surface. | **3.13** |  | **Sft** |  |
| 2 | **P/F Energy Saver 24 watts Philiphs or equilenet quality as directed by the E.I** | **24-nos** |  | **“** |  |
| 3 | S/F Fancy Switch socket with board as approved quality by the Engineer Incharge etc complete. | 45-Nos |  | Each |  |
| 4 | P/F Universal light Plug 10-amp imported quality i/c necessary electric connection etc complete. | 10-Nos |  | “ |  |
| 5 | P/F Power Plug 15-amps imported quality i/c necessary electric connection etc complete. | 8-Nos |  | “ |  |
| 6 | P/F Fancy Tube Light 2-40 watt fancy shade i/c chock & starter i/c necessary electric connection etc complete. | 8-Nos |  | “ |  |
| 7 | P/F Ceiling Fan 56”sweep make GFC imported or equalent quality i/c necessary electric connection as req. | **6-Nos** |  | **“** |  |
| 8 | S/F Fancy Fan Dimmer as approved quality etc complete. | 6-Nos |  | “ |  |
| 9 | P/F Wall Bracket Fan 18”sweep make GFC imported or equalent quality i/c necessary electric connection as req. | **8-Nos** |  | **“** |  |
| 10 | P/F LED Pannel Light (Energy Saving Effect)(24”x24”)(Model 6500 k) for using false ceiling imported quality i/c making connection as per requirement of site etc complete. | 6-Nos |  |  |  |
|  | Total |  |  |  |  |
|  | G Total |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Electrical sub Division-XII,

Karachi