|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**M/R TO CIVIL JUDGE @ GHOTKI ( OLD JUDGE BUNGALOW).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A(I) BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Removing cement or lime plaster. (S.I.No: 53 P- 13 ). | | | | |  |  |
|  |  |  | **3780** | **SFT** | **121/00** | **%SFT** | **3780/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Removing door & Windows with chowkats. | | | |  |  |  |
|  | Doors. |  | 03 | Nos. | 142/18 | EACH | 427/- |
|  |  |  |  |  |  |  |  |
|  | Window. |  | 01 | No. | 102/85 | EACH | 103/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Scraping ordinary distemper or oil bound on walls. (S.I.No:54(b) P-13). | | | | |  |  |
|  |  |  | **1486** | **SFT** | **226/88** | **%SFT** | **3371/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Scraping white wash or colour wash. (S.I.No:54(a) P-13). | | | | |  |  |
|  |  |  | **1120** | **SFT** | **75/63** | **%SFT** | **847/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Providing and fixing G.I. frames/chowkats 7”x2” or 4-1/2” x3” for door using 20 guage G.I. Sheet i/c welded hinges and fixing. (S.I.No:29 P-94). | | | | |  |  |
|  | A)Door. |  |  |  |  |  |  |
|  |  |  | **52** | **RFT** | **228/90** | **P.RFT** | **11903/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B)Windows. |  | **84** | **RFT** | **240/50** | **P.RFT** | **20202/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Applying floating coat of cement 1/32”thick. (S.I.No:14 P-53). | | | | |  |  |
|  |  |  | 3780 | SFT | **660/00** | **%SFT** | **4574/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Cement plaster (1:6) upto 20’ height ½” thick. (S.I.No:13(b) P-52). | | | | |  |  |
|  |  |  | **3780** | **SFT** | **2206/60** | **%SFT** | **83409/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Cement plaster (1:4) upto 20’ height 3/4” thick. (S.I.No:11(c) P-52). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **3780** | **SFT** | **3015/76** | **%SFT** | **113996/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Cement pointing struck joints on walls. (S.I.No:19 P-53). | | | | |  |  |
|  |  |  | **318** | **SFT** | **1287/44** | **%SFT** | **3193/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | First class deodar wood wrought joinery in doors and windows fixe to position including chowkats, hold fasts, hinges, iron tower bolts cleats deodar paneled or paneled and glazed or fully glazed (Only shutters)( 1-1/3” thick (S.I.No:7(b)P-58). B)1-3/4” thick. | | | | |  |  |
|  |  |  | **141** | **SFT** | **902/93** | **P.SFT** | **127313/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | First class deodar wood wrought joinery work wire gauze doors and windows with 22 S.W.G . Galavanized wire gauze 144 mesh per square inch iron fitting etc complete.(b) 1-1/4” thick deodar wood framing i/c wire gauze with ordinary hinges. (S.I.No:14(b)P-59). | | | | |  |  |
|  | A)Doors. |  |  |  |  |  |  |
|  |  |  | **105** | **SFT** | **562/98** | **P.SFT** | **59113/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B)Galvanized wire gauze fixed to chowkats with ¾” deodar strips and screws. (S.I.No:14(d) P-60). | | | | |  |  |
|  | Windows. |  |  |  |  |  |  |
|  |  |  | **334** | **CFT** | **190/72** | **P.SFT** | **63700/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Primary coat of chalk under distemper. (S.I.No:23 P-54). | | | |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **3780** | **SFT** | **442/75** | **%SFT** | **16736/-** |

**Page No:2.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 13/- | Distempering two coats old surface. (S.I.No:24(b) P-54). | | | | |  |  |
|  |  |  | **6751** | **SFT** | **442/75** | **%SFT** | **70474/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 14/- | Colour washing two coats old surface (S.I.No:25(b) P-54). | | | |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | 1120 | SFT | **859/90** | **%SFT** | **9631/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 15/- | Painting doors and windows any type two coats Old surface (S.I.No:4© P-68). | | | | | |  |
|  |  | **TOTAL:-** | **1356** | **SFT** | **1160/06** | **%sft** | **15730/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 16/- | Painting guard bars gates irons bars grating, railing including braces etc two coats. (S.I.No:5(b) P-69). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **439** | **SFT** | **896/39** | **%SFT** | **7870/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 17/- | Painting surface and painting guard bars, gates or iron bars gratings, railings i/c standards braces etc © and similar open work. (S.I.No:5(d) P-70). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **147** | **SFT** | **896/39** | **%SFT** | **1318/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 18/- | Two coat of bitumen laid hot using 34 lbs for % Sft over roof and binding with sand at one Cft per % Sft. (S.I.No:13 P-41). | | | |  |  |  |
|  |  |  | **1637** | **SFT** | **1887/40** | **%SFT** | **30896/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A(i)” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **6,50,281/-** |

**PART “B” W/S & S/F SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Providing & fixing24”x18” lavatory basin in white glazed earthenware complete.(S.I.No:8 P-3). | | | |  |  |  |
|  |  |  | 03 | Nos. | 4253/70 | EACH | 12761/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Add extra for labour for providing and fixing earthe ware etc complete. (S.I.No:9 P-3). | | | |  |  |  |
|  |  |  | 03 | Nos. | 938/47 | EACH | 2815/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Providing and fixing steel sinks stainless local make complete with cost or iron or wraught irone brackets 6” inches built in wall, 1-1/2” C.P. rubber plug chrome plated brass chain 1-1/2” C.P. brass waste, with 1-1/2” P.V.C. waste pipe and making requisite number of holes in wall and plinth and floor for pipe connection and making good in cement concrete (b) Steel sink stainless sized 36”x18” local make (Standard pattern). (S.I.No:19(b) P-6). | | | |  |  |  |
|  |  |  | 01 | No. | 5162/30 | EACH | 5162/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Providing andc fixing 6”x2” or 6”x3” C.I. floor trap of the approved self cleaning design with a C.I scrwed down gritting with or without a vent arm complete with and i/c making requisite number of holes in wall plinth and floor for pipe connection and making good in C.C. (1;2:4).(S.I.No:20 P-6). | | | | |  |  |
|  |  |  | 09 | Nos. | 2042/43 | EACH | 18382/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | P/F in position nylon connection complete with ½” dia brass stop cock with pair of brass nuts and lining jointing to nylon connection.. (S.I.No:23 P-6). | | | |  |  |  |
|  |  |  | 03 | Nos. | 447/15 | EACH | 1341/- |

**Page No:3.**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | | QUANTITY. | | | RATE. | | UNIT. | | AMOUNT. | |
| 6/- | Providing and Fixing chrome plated brass towel rail complete with brackets fixing on wooden cleats with 1” long C.P. brass screws. (1) Towel rail 30” long (b) ¾” dia round or square (Superior quality) (S.I.No:1(ii)b P-7). | | | | | |  | |  | |  |
|  |  |  | | 03 | Nos. | | 1269/95 | | EACH | | 3810/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Providing and fixing 15”x12” beveled edge mirror of Belgium glass complete with 1/8” thick hard board and C.P. screws fixed to wooden pleat, Standard pattern. (S.I.No:4(a) P-7). | | | |  |  |  |
|  |  |  | 03 | Nos. | 1161/60 | EACH | 3482/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Supplying and fixing Soap tray earthen ware with C.P. screws etc complete. (S.I.No:5 P-8). | | | |  |  |  |
|  |  |  | 03 | Nos. | 497/20 | EACH | 1492/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Providing and fixing 4” dia C.I. soil and vent pipe i/c cutting and fitting and extra painting to match the colour of the building. (S.I.No:1 P-9). | | | |  |  |  |
|  | 4” dia. |  | 45 | RFT | 333/29 | P.RFT | 14998/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | Providing and fixing 4” dia C.I. plain bend of the required degree including extra painting to match the colour of the building. (S.I.No:10 P-10). | | | |  |  |  |
|  |  |  | 06 | Nos. | 566/70 | EACH | 3400/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | Providing and fixing 4” dia C.I. terminal guard including extra painting to match the colour of the building. (S.I.No:11 P-10). | | | |  |  |  |
|  |  |  | 03 | Nos. | 389/70 | EACH | 1169/- |
|  |  |  |  | | | | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Providing G.I. pipes and special etc clamps etc i/c fixing cutting and fitting complete with and i/c the cost of breaking through walls and roof making good etc painting two coats after cleaning the pipe etc with white zink paint with pigment to match the colour of the building and testing with water to a pressure head of 200 feet and handling. (S.I.No: 1 P-11). | | | |  |  |  |
|  | a)1/2” dia. |  | 30 | RFT | 73/21 | P.RFT | 2196/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | b)3/4” dia. |  | 30 | RFT | 95/79 | P.RFT | 2874/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | c)1” dia. |  | 30 | RFT | 128/55 | P.RFT | 3857/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 13/- | Supplying and fixing in position brass bib cocks.  (S.I.No:1(i)(a) P-16). | | | |  |  |  |
|  |  |  | 03 | Nos. | 299/42 | EACH | 898/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 14/- | Providing and fixing Handle valve (China). (S.I.No:5 P-7). | | | |  |  |  |
|  | a) 3/4” dia. |  | 03 | Nos. | 271/92 | EACH | 816/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 15/- | Supplying and fixing long bib cocks of superior quality with C.P. head ½” dia (S.I.No:1b-b P-19). | | | |  |  |  |
|  |  |  | 03 | Nos. | 1109/46 | EACH | 3328/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 16/- | Supplying and fixing wash basin mixture of superior quality with C.P. head ½” dia. (S.I.No:14(a) P-19). | | | |  |  |  |
|  |  |  | 03 | Nos. | 2882/00 | EACH | 8646/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 17/- | Supplying and fixing sink mixture cock of quperior quality with C.P. head et completed. (S.I.No:17 P- 19 ). | | | |  |  |  |
|  |  |  | 03 | Nos. | 2745/60 | EACH | 8237/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 18/- | Supplying and fixing C.P. Muslim Shower with double Bib cock & ring pipe etc complete. (S.I.No:19 P-19). | | | |  |  |  |
|  |  |  | 03 | Nos. | 3432/00 | EACH | 10296/- |

**Page No:4.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 19/- | Providing R.C.C. pipe with collar class “B” digging the trenches to required depth & fixing in position including cutting, fitting & jointing with maxphalt composition & cement mortar (1:1) and testing with water pressure to a head of 4’ feet above the top of the highest pipe & refilling with excavated staff. (S.I.No:2 P-24). | | | |  |  |  |
|  | a) 6” dia |  | 18 | RFT | 199/25 | P.RFT | 3587/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 20/- | Fixing aquatting tuype W.C. pan set consisting of flushing cutting flush pipe & a trap i/c cutting and making good the requisite number of holes in walls, plinth and floor and making in (1:2;4) C.C. (S.I.No:1 P-26). | | | |  |  |  |
|  |  |  | 03 | Nos. | 810/70 | EACH | 2432/- |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 21/- | | Manufacturing and supplying of 21” R.C.C. Manhole cover cost in (1:2:4)( Consreteratio 3” deep at centre reinforced with ½” dia tor steel barsat 4” i/c welded 3/16” thick wide M.S. plate two hook of 3/8”dia tor bar i/c compacting i/c curing and tranches portation within 10 miles.  (S.I.No:1-b P-31). | | | | |  |  | |  | |
|  | | a)24” inch dia. | |  | 10 | Nos. | 1051/25 | EACH | | 10513/- | |
|  |  | | **PART “B” W/S & S/F SCHEDULE ITEMS TOTAL RS:-** | | | | | | **1,26,492/-** | |

**PART “C” NON SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Supplying and fixing 1 H.P. Electric Motor. | | | |  |  |  |
|  |  |  | 01 | No. |  | EACH |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | | Supplying and fixing Sui Gas Gizar K.S.C. Company (35 Gallons). | | | | |  |  | |  |
|  | |  | |  | 01 | No. |  | EACH | |  |
|  |  | | **PART “C”NON SCHEDULE ITEMS TOTAL RS:-** | | | | | |  | | |

**GENERAL ABSTRACT.**

|  |  |  |
| --- | --- | --- |
| 1/- | **PART “A” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **6,50,281/-** |
| 2/- | **PART “B” W/S & S/F SCHEDULE ITEMS TOTAL RS:-** | **1,26,492/-** |
| 4/- | **PART “C” NON SCHEDULE ITEMS TOTAL RS:-** |  |
|  | **TOTAL RS:-** |  |
|  | **SAY RS:-** |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PART "A" | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | | | **Total Rs:-** |  |
| PART "B" |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below W/S & S/F Schedule Items | | | **Total Rs:-** |  |
| PART "C" |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Non Schedule Items | | | **Total Rs:-** |  |
|  |  |  |  |  | **G. Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |