|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**CONSTRUCTION OF OFFICE BUILDINGS FOR ON FORM WATER MANAGERMENT STAFF**

**@ SHIKARPUR (CONSTRUCTION OF COMPOUND WALL I/C MAIN GATE PILLARS).**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. |  | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A” BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |
| --- | --- | --- | --- |
| 1/- | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth watering and ramming lead upto 5’ ft: ( In ordinary soil).  (S.I.NO:18(b) P-4). |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | 3808 | CFT | 3176/25 | %OCFT | 12095/- |
| 2/- | Cement concrete brick or stone ballast 1-1/2” to 2” gauge Ratio(1:4:8).  (S.I.No:4(b) P-14). | | | | |  |  |
|  |  |  | 1298 | CFT | 9416/28 | %CFT | 122223/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Reinforcement cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding, which will be paid separately. This rate also includes all kinds of forms moulds: lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle)a) R.C. work in roof slab, beams columns rafts, lintels and other structural members laid in situ or pre cast laid in position complete in all respect. i) Ratio (1:2:4) 90 Lbs cement 2 Cft shingle 1/8” to ¼” gauge.(S.I.No:6(a)(i) P-16).  Plinth Beam. | | | | |  |  |
|  |  |  | **2474** | **CFT** | **337/00** | **P.CFT** | **833738/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Fabrication of mild steel reinforcement for cement concrete i/c cutting bending, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars).  Plinth Beam. | | | | |  |  |
|  |  |  | **112.09** | **CWT** | **5001/70** | **P.CWT** | **560641/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Random rubble masonry (Un-Coursed) in cement sand mortar (1:6). (S.I.No:1(iv) P-26). | | | |  |  |  |
|  |  |  | **780** | **CFT** | **17723/-** | **%CFT** | **138239/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Coursed rubble masonry i/c hammer dressing in cement sand mortar (1:6) (S.I.No:2(iv) P-26). | | | |  |  |  |
|  |  |  | **2188** | **CFT** | **25321/-** | **%CFT** | **553897/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Bitumen coating to plastered or cement concrete surface. (S.I.No:9 P-71). | | | |  |  |  |
|  |  |  | **1000** | **SFT** | **778/09** | **%SFT** | **7781/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Pacca brick work other than building i/c striking of joints in cement sand mortar 1.6. (S.I.no:7(i)(e) P-21). | | | |  |  |  |
|  |  |  | **3240** | **CFT** | **12346/65** | **%CFT** | **400031/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Cement plaster 1:6 upto 20’height ½” thick. (S.I.No:11(a) P-52). | | | | |  |  |
|  |  |  | **4800** | **SFT** | **2206/60** | **%SFT** | **105917/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | Cement plaster 1:4 upto 20’height3/8” thick. (S.I.No:11(b) P-51). | | | | |  |  |
|  |  |  | **4800** | **SFT** | **2197/52** | **%SFT** | **105481/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | Cement pointing struck joints on wall Ratio (1:2).  (S.I.No:19 P-52). | | | |  |  |  |
|  |  |  | **4360** | **SFT** | **1287/44** | **%SFT** | **56132/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Cement pointing stone work raised. (S.I.No:13-c P-53). | | | | |  |  |
|  |  |  | **5600** | **SFT** | **1726/37** | **%SFT** | **96677/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 13/- | Providing and laying Hala or pattern tiles glazed 6’x6” x 1/4” on floor wall facing in required COLOUR AND PATTERN OF rtile. (S.I.No:61 P-48). | | | | |  |  |
|  |  |  | **153** | **SFT** | **47651/56** | **%SFT** | **72907/-** |

Page No:2.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. |  | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 14/- | Making & fixing steel grated doors 1/16” thick sheeting angle iron frame 2”x2”x3/8” and square bars with locking arrangement 4” centre to centre (S.I.No:28 P-91). | | | | |  |  |
|  |  |  | **96** | **SFT** | **594/57** | **P.SFT** | **57079/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 15/- | Distempering two coats. (S.I.No:24 (b) P-53). | | | | |  |  |
|  |  |  | **9600** | **SFT** | **1043/90** | **%SFT** | **100214/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 16/- | Preparing surface and painting guard bars two coats.  (S.I.No:5(d)(i)(ii) P-70). | | | | |  |  |
|  |  |  | **192** | **SFT** | **896/39** | **%SFT** | **1721/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL RS:-** | **32,24,773/-** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PART "A” | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Non Schedule Items | | | **Total Rs:-** |  |
|  |  |  |  | | **G. Total Rs:-** |  |
|  |  |  |  | |  |  |
|  |  |  |  | EXECUTIVE ENGINEER | | |
| CONTRACTOR | |  |  | PROVINCIAL BUILDINGS DIVISION | | |
|  |  |  |  | SUKKUR | | |