|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**13- M/R TO CIVIL COURT COMPLEX BUILDING @ UBAURO**

**(I/C RAISING OF COMPOUND WALL).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A” BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Cement concrete plain i/c placing compacting finishing and curring complete i/c screening and washing at stone aggregate without shuttering ratio (1:2:4).  (S.I.No:5(f) P-16). | | | | |  |  |
|  |  |  | **20** | **CFT** | **14429/25** | **%CFT** | **2886/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Pacca brick work in other than building cement sand mortar Ratio (1:6). (S.I.No:7(e) P-22). | | | | |  |  |
|  |  |  | **110** | **CFT** | **12346/65** | **%CFT** | **3440/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Erecting and removal of centering for R.C.C. or plain cement concrete works of deodar wood (2” class) b) for partal wood (ii) vertical. (S.I.No:19(b+ii) P-18). | | | | |  |  |
|  |  |  | **60** | **SFT** | **3127/41** | **%SFT** | **7408/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Cement plaster (1:6) upto 20’ height ½” thick. (S.I.No:13(b) P-52). | | | | |  |  |
|  |  |  | **413** | **SFT** | **2206/60** | **%SFT** | **9113/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Cement plaster (1:4) upto 20’ height 3/8” thick. (S.I.No:11(a) P-52). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **413** | **SFT** | **2197/52** | **%SFT** | **9076/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | White washing 3 coats (S.I.No:26(c) P-53). | | | | |  |  |
|  |  |  | **413** | **SFT** | **829/95** | **%SFT** | **3428/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Providing and fixing angle iron vertical posts for barbed wire fencing of size 2”x2”x1/4” embedded in R.C.C./ Masonary pillars i/c making cuts/ holes @ 12” i/c fixing in pillars by chiseling and filling the with cement sand mortar spraining and finishing the surface. (S.I.No:8 P-95). | | | | |  |  |
|  |  |  | **40** | **RFT** | **169/18** | **P.RFT** | **6767/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Making and fixing barbed wire fancing i/c R.C.C. posts upto 4.0 horizontel and cross wires. (S.I.No:7 P-95). | | | | |  |  |
|  |  |  | **400** | **LFT** | **25283/36** | **%LFT** | **101133/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Painting new surface:- Painting guard bars gates iron bars, grating, railing etc. (S.I.No: P- ). | | | | |  |  |
|  |  |  | **183** | **SFT** | **1270/83** | **%SFT** | **2326/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **TOTAL RS:-** | **143251/-** |
|  |  | **FOR 100 RFT RS:145577 / 100 X 485 RFT = RS:-** | **694767/-** |

|  |  |  |  |
| --- | --- | --- | --- |
| PART "A" | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR. |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR. |