|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**17- M/R TO CIVIL JUDGE @ GHOTKI ( OLD JUDGE BUNGALOW).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A(I) BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Removing cement or lime plaster. (S.I.No: 53 P- 13 ). | | | | |  |  |
|  |  |  | **3780** | **SFT** | **121/00** | **%SFT** | **4574/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Removing door & Windows with chowkats. | | | |  |  |  |
|  | Doors. |  | 03 | Nos. | 142/18 | EACH | 427/- |
|  |  |  |  |  |  |  |  |
|  | Window. |  | 01 | No. | 102/85 | EACH | 103/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Scraping ordinary distemper or oil bound on walls. (S.I.No:54(b) P-13). | | | | |  |  |
|  |  |  | **1486** | **SFT** | **226/88** | **%SFT** | **3371/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Scraping white wash or colour wash. (S.I.No:54(a) P-13). | | | | |  |  |
|  |  |  | **1120** | **SFT** | **75/63** | **%SFT** | **847/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Providing and fixing G.I. frames/chowkats 7”x2” or 4-1/2” x3” for door using 20 guage G.I. Sheet i/c welded hinges and fixing. (S.I.No:29 P-94). | | | | |  |  |
|  | A)Door. |  |  |  |  |  |  |
|  |  |  | **52** | **RFT** | **228/90** | **P.RFT** | **11903/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B)Windows. |  | **84** | **RFT** | **240/50** | **P.RFT** | **20202/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Applying floating coat of cement 1/32”thick. (S.I.No:14 P-53). | | | | |  |  |
|  |  |  | 3780 | SFT | **660/00** | **%SFT** | **4574/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Cement plaster (1:6) upto 20’ height ½” thick. (S.I.No:13(b) P-52). | | | | |  |  |
|  |  |  | **3780** | **SFT** | **2206/60** | **%SFT** | **83409/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Cement plaster (1:4) upto 20’ height 3/4” thick. (S.I.No:11(c) P-52). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **3780** | **SFT** | **3015/76** | **%SFT** | **113996/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Cement pointing struck joints on walls. (S.I.No:19 P-53). | | | | |  |  |
|  |  |  | **318** | **SFT** | **1287/44** | **%SFT** | **4094/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | First class deodar wood wrought joinery work wire gauze doors and windows with 22 S.W.G . Galavanized wire gauze 144 mesh per square inch iron fitting etc complete.(b) 1-1/4” thick deodar wood framing i/c wire gauze with ordinary hinges. (S.I.No:14(b)P-59). | | | | |  |  |
|  | A)Doors. |  |  |  |  |  |  |
|  |  |  | **105** | **SFT** | **562/98** | **P.SFT** | **59113/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B)Galvanized wire gauze fixed to chowkats with ¾” deodar strips and screws. (S.I.No:14(d) P-60). | | | | |  |  |
|  | Windows. |  |  |  |  |  |  |
|  |  |  | **334** | **CFT** | **190/72** | **P.SFT** | **63700/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | Primary coat of chalk under distemper. (S.I.No:23 P-54). | | | |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **3780** | **SFT** | **442/75** | **%SFT** | **16736/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Distempering two coats old surface. (S.I.No:24(b) P-54). | | | | |  |  |
|  |  |  | **6751** | **SFT** | **442/75** | **%SFT** | **70474/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 13/- | Colour washing two coats old surface (S.I.No:25(b) P-54). | | | |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | 1120 | SFT | **859/90** | **%SFT** | **9631/-** |

**Page No:2.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 14/- | Painting doors and windows any type two coats Old surface (S.I.No:4© P-68). | | | | | |  |
|  |  | **TOTAL:-** | **434** | **SFT** | **1160/06** | **%sft** | **5035/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A(i)” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **4,72,189/-** |

|  |  |  |  |
| --- | --- | --- | --- |
| PART "A" | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |