|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**M/R TO DISTRICT COURT COMPLEX BUILDING @ GHOTKI**

**(I/C RAISING OF COMPOUND WALL).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A(i)” C/Wall BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Cement concrete plain i/c placing compacting finishing and curring complete i/c screening and washing at stone aggregate without shuttering ratio (1:2:4).  (S.I.No:5(f) P-16). | | | | |  |  |
|  |  |  | **20** | **CFT** | **14429/25** | **%CFT** | **2886/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Erecting and removal of centering for R.C.C. or plain cement concrete works of deodar wood (2” class) b) for partal wood (ii) vertical.  (S.I.No:19(b+ii) P-18). | | | | |  |  |
|  |  |  | **110** | **SFT** | **3127/41** | **%SFT** | **3440/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Pacca brick work in other than building cement sand mortar Ratio (1:6). (S.I.No:7(e) P-22). | | | | |  |  |
|  |  |  | **60** | **CFT** | **12346/65** | **%CFT** | **7408/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Cement plaster (1:6) upto 20’ height ½” thick. (S.I.No:13(b) P-52). | | | | |  |  |
|  |  |  | **413** | **SFT** | **2206/60** | **%SFT** | **9113/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Cement plaster (1:4) upto 20’ height 3/8” thick. (S.I.No:11(a) P-52). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **413** | **SFT** | **2197/52** | **%SFT** | **9076/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | White washing 3 coats (S.I.No:26(c) P-53). | | | | |  |  |
|  |  |  | **413** | **SFT** | **829/95** | **%SFT** | **3428/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Providing and fixing angle iron vertical posts for barbed wire fencing of size 2”x2”x1/4” embedded in R.C.C./ Masonary pillars i/c making cuts/ holes @ 12” i/c fixing in pillars by chiseling and filling the with cement sand mortar spraining and finishing the surface. (S.I.No:8 P-95). | | | | |  |  |
|  |  |  | **40** | **RFT** | **169/18** | **P.RFT** | **6767/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Making and fixing barbed wire fancing i/c R.C.C. posts upto 4.0 horizontel and cross wires. (S.I.No:7 P-95). | | | | |  |  |
|  |  |  | **400** | **LFT** | **25283/36** | **%LFT** | **101133/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **C/WALL TOTAL RS:-** | **143251/-** |
|  |  | **PART “A(i)” FOR 100 RFT RS:143251 / 100 x 465 RFT =** | **6,66,117/-** |

**PART “A(ii) BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Providing and fixing iron collapsible gate with channel framing of section ¾”x5/16” at 4” i/c revitted with ¾”x1/8” flat iron patti piaced diagonally and provided top and bottom T-Section 1”x1” 1/8” long with rollers also i/c locking arrangement and fixing in floor/ ceiling or wall etc complete. (S.I.No:32 P-94). | | | | |  |  |
|  |  |  | 55 | SFT | 387/04 | P.SFT | 21287/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Providing and fixing G.I. frames/chowkats 7”x2” or 4-1/2” x3” for door using 20 guage G.I. Sheet i/c welded hinges and fixing.(S.I.No:29 P-94). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **102** | **RFT** | **228/90** | **P.RFT** | **23348/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Scraping Ordinary distemper oil bound distemper paint on walls.  (S.I.No:54 (b) P- 13). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **224** | **SFT** | **226/88** | **%SFT** | **508/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Distempering three coats. (S.I.No:24© P-54). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **560** | **RFT** | **1079/65** | **%SFT** | **6046/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Painting doors and windows any type two coats. (S.I.No:4(c)i+ii P-68). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **352** | **RFT** | **1160/06** | **%SFT** | **4083/-** |

Page No:2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Preparing surface and painting guard bars, gates of iron bars, grating railings including standards braces, etc and similar open work two coats new surface. (S.I.No:5(d)+i+ii) P-70). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **111** | **RFT** | **896/39** | **%SFT** | **995/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A(ii) BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **56267/-** |

**PART “A(iii)” BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Removing cement or lime plaster. (S.I.No: 53 P- 13 ). | | | | |  |  |
|  |  |  | **312** | **SFT** | **121/00** | **%SFT** | **378/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Applying floating coat of cement 1/32” thick. (S.I.No:14 P-52). | | | | | |  |  |
|  |  |  | **327** | **SFT** | **660/-** | **%SFT** | | **2158/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | Pacca brick work in Ground floor in cement sand mortar 1.6.  (S.I.no:5(c) P-21). | | | | |  |  |
|  |  |  | **37** | **CFT** | **12674/36** | **%CFT** | **4690/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Cement plaster 1:6 upto 20’height ½” thick. (S.I.No:11(a) P-52). | | | | |  |  |
|  |  |  | **423** | **SFT** | **2206/60** | **%SFT** | **9334/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Cement plaster 1:4 upto 20’height3/8” thick. (S.I.No:11(b) P-51). | | | | |  |  |
|  |  |  | **423** | **SFT** | **2197/52** | **%SFT** | **9296/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Removisng door with chowkat.(S.I.No:33(a+b) P-12). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **01** | **Nos.** | **142/18** | **EACH** | **142/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Supplying and fixing false ceiling of plaster of paris, in panels including making frame, work of deodar wood including painting with soligia pant. (S.I.No:52 P-64). | | | | |  |  |
|  |  |  | **369** | **SFT** | **30509/77** | **%SFT** | **112581/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Supplying and fixing in position aluminuim channels hangeds doors or alcop made with 5 mm thick tinted glass glazing (Belguim) and alpha Japan locks i/c handles stoppers etc deluxe model (White) (S.I.No:83(a) P-108). | | | | |  |  |
|  |  |  | **74** | **SFT** | **1592/69** | **P.SFT** | **117859/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Preparing the surface and painting with matt finishing i/c rubbing the surface with bathy (silicon carbide rubbing brick) filling the voids with zink/chalk / plaster of Paris mixture, applying first coat premix, making the surface smooth and then painting 3 coats with matt finish of approved make et complete. (New surface) (S.I.No:3 A P-54). | | | | |  | |  |
|  |  |  | **326** | **SFT** | **3444/38** | **%SFT** | **11229/-** | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | Providing and Fixing False Ceiling. | | | | |  |  |
|  |  |  | **168** | **SFT** | **25293/42** | **P.SFT** | **42493/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | Applying chemical polishing on existing mosaic / marble flooring/ dado including cleaning grinding with carborandum stone/ sand papers and applying chemical polishing as per requirement. (S.I.No:70 P-49) | | | | |  |  |
|  |  |  | **168** | **SFT** | **36/00** | **P.SFT** | **5000/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A(iii)” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **3,15,160/-** |

Page No:3.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “B” NON SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Providing and Fixing Granite Slabs for Counter. | | | | |  |  |
|  |  |  | **26** | **Feets.** |  | **P.Feet.** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | S/F innarguration Plate Stainless steel. | | | | |  |  |
|  |  |  | **1** | **No.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | S/F un-arguration Curtain. | | | | |  |  |
|  |  |  | **1** | **No.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Supply computer tables. | | | | |  |  |
|  |  |  | **3** | **Nos.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Supply Master (Aura) Chairs. | | | | |  |  |
|  |  |  | **3** | **Nos.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Supply & Fixing Ambosc Mirrors. | | | | |  |  |
|  |  |  | **2** | **Nos.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Supplying and fixing Sticker. | | | | |  |  |
|  |  |  | **1** | **No.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Supply 2” dia Holes in Granite top. | | | | |  |  |
|  |  |  | **3** | **Nos.** |  | **EACH** |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | | Supplying and fixing Roller Blinds. | | | | | |  | |  |
|  | |  | |  | **25** | **Nos.** |  | **P.SFT** | |  |
|  |  | | **PART “B” NON SCHEDULE ITEMS TOTAL RS:-** | | | | | |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| PART "A(i+i+ii)" | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |
| PART "B" |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Non Schedule Items | **Total Rs:-** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  | **G. Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR. |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR. |