|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

16- **M/R TO SENIOR CIVIL JUDGE @ GHOTKI**

**( OLD DISTRICT JUDGE 01 NO BUNGALOW).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A” BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Cement concrete plain (1:2:4). | | | | |  |  |
|  |  |  | **42** | **CFT** | **14429/25** | **%CFT** | **6060/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Providing and laying tiles glazed 6”x6” on floor or wall facing in required colour and pattern of STILE specification. (S.I.No:60 P-47). | | | | |  |  |
|  |  |  | **510** | **SFT** | **30509/77** | **%SFT** | **155600/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 3/- | First class deodar wood wrought joinery in doors and windows fixe to position including chowkats, hold fasts, hinges, iron tower bolts cleats deodar paneled or paneled and glazed or fully glazed (Only shutters)( 1-1/3” thick (S.I.No:7(b)P-58). | | | | |  |  |
|  | B)1-3/4” thick.D |  |  |  |  |  |  |
|  |  |  | **39** | **SFT** | **902/93** | **P.SFT** | **35214/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | First class deodar wood wrought joinery work wire gauze doors and windows with 22 S.W.G . Galavanized wire gauze 144 mesh per square inch iron fitting etc complete.(b) 1-1/4” thick deodar wood framing i/c wire gauze with ordinary hinges. (S.I.No:14(b)P-59). | | | | |  |  |
|  | Doors. |  | **169** | **SFT** | **562/98** | **P.SFT** | **95144/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Galvanized wire gauze fixed to chowkats with ¾” deodar strips and screws. (S.I.No:14(d) P-60). | | | | |  |  |
|  | Windows. |  | **524** | **CFT** | **190/72** | **P.SFT** | **99937/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6/- | Two coat of bitumen laid hot using 34 lbs for % Sft over roof and binding with sand at one Cft per % Sft. (S.I.No:13 P-41). | | | |  |  |  |
|  |  |  | **2628** | **SFT** | **1887/40** | **%SFT** | **49601/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Providing and fixing deodar Almirah 9”x12” depth i/c boxing with back shelves, shutters brass fittings complete. (S.I.No:23 P-61). | | | |  |  |  |
|  |  |  | 33 | SFT | **1778/50** | **P.SFT** | **58690/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **5,00,046/-** |

|  |  |  |  |
| --- | --- | --- | --- |
| PART "A" | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PART "A" | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | | | **Total Rs:-** |  |
| PART "B" |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below W/S & S/F Schedule Items | | | **Total Rs:-** |  |
|  |  |  | | |  |  |
|  |  |  |  |  | **G. Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |