|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

M&R TO DISTRICT JAIL PRISON @ GHOTKI ( REPAIR OF INSIDE PRISONS BARRACKS 13 NOS, HOSPITAL BLOCK, SECURITY CELLS 26 NOS AND OFFICE BLOCK).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “A” BUILDINGS SCHEDULE ITEMS.**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Excavation in foundation of Building Bridges and other structures including dag belling dressing, refilling around structure with excavated earth watering and ramming lead upto 5’ ft: ( In ordinary soil).  (S.I.NO:18(b) P-4). | | | | | | |  | |  |
|  |  |  |  | |  | |  |  | |  |
|  |  |  | **4110** | **CFT** | | **3176/25** | | | **%OCFT** | **13054/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2/- | Cement concrete brick or stone ballast 1-1/2” to 2” gauge Ratio(1:4:8).  (S.I.No:4(b) P-14). | | | | |  |  |
|  |  |  | **1293** | **CFT** | **9416/28** | **%CFT** | **121753/-** |

|  |  |  |  |
| --- | --- | --- | --- |
| 3/- | Pacca brick work in foundation and plinth in cement sand mortar (1:6). (S.I.No:4(e) P-21). |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **2792** | **CFT** | **11948/36** | **%CFT** | **333598/-** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 4/- | Reinforcement cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding, which will be paid separately. This rate also includes all kinds of forms moulds: lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle)a) R.C. work in roof slab, beams columns rafts, lintels and other structural members laid in situ or pre cast laid in position complete in all respect. i) Ratio (1:2:4) 90 Lbs cement 2 Cft shingle 1/8” to ¼” gauge.(S.I.No:6(a)(i) P-16). | | | | |  | |  |
|  |  |  |  |  |  |  | |  |
|  |  |  | **1955** | **CFT** | **337/00** | **P.CFT** | **658835/-** | |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 5/- | Bitumen coating to plastered or cement concrete surface. (S.I.No:9 P-71). | | | | |  |  | |  |
|  |  |  | | **612** | **SFT** | **778/09** | **%SFT** | | **4762/-** |
| 6/- | Fabrication of mild steel reinforcement for cement concrete i/c cutting bending, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars). | | | | | |  |  | |
|  |  | |  | **87.27** | **CWT** | **5001/70** | **P.CWT** | **436498/-** | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 7/- | Pacca brick work in other than building cement sand mortar Ratio (1:6). (S.I.No:7(e) P-22). | | | | |  | |  |
|  |  |  | **8002** | **CFT** | **12346/65** | **%CFT** | **987979/-** | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Cement plaster (1:6) upto 20’ height ½” thick. (S.I.No:13(b) P-52). | | | | |  |  |
|  |  |  | **14432** | **SFT** | **2206/60** | **%SFT** | **318457/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 9/- | Cement plaster (1:4) upto 20’ height 3/4” thick. (S.I.No:11(c) P-52). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **14432** | **SFT** | **2197/52** | **%SFT** | **317146/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 10/- | Making & fixing steel grated doors 1/16” thick sheeting angle iron frame 2”x2”x3/8” and square bars with locking arrangement 4” centre to centre (S.I.No:28 P-91). | | | | |  |  |
|  |  |  | **480** | **SFT** | **594/57** | **P.SFT** | **285394/-** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 11/- | Painting new surface:- Painting guard bars gates iron bars, grating, railing etc. (S.I.No:5(d)i+ii+iii) P- 70 ). | | | | |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  | **960** | **SFT** | **1270/83** | **%SFT** | **12200/-** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **PART “A” BUIDLINGS SCHEDULE ITEMS TOTAL RS:-** | **34,89,676/-** |

Page No:2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

**PART “B” W/S & S/F SCHEDULE ITEMS**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | | Manufacturing and supplying of 21” R.C.C. Manhole cover cost in (1:2:4)( Consreteratio 3” deep at centre reinforced with ½” dia tor steel barsat 4” i/c welded 3/16” thick wide M.S. plate two hook of 3/8”dia tor bar i/c compacting i/c curing and tranches portation within 10 miles.  (S.I.No:1-b P-31). | | | | |  |  | |  | |
|  | | a)Main Hole 24” inch dia. | |  | 08 | Nos. | 1051/25 | EACH | | 8410/- | |
|  |  | | **PART “B” W/S & S/F SCHEDULE ITEMS TOTAL RS:-** | | | | | | **8,410/-** | |

**GENERAL ABSTRACT.**

|  |  |  |
| --- | --- | --- |
| 1/- | **PART “A” BUILDINGS SCHEDULE ITEMS TOTAL RS:-** | **34,89,676/-** |
| 2/- | **PART “B” W/S & S/F SCHEDULE ITEMS TOTAL RS:-** | **8,410/-** |
|  | **TOTAL RS:-** | **34,98,034/-** |
|  | **SAY RS:-** | **34,98,000/-** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PART "A" | | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | | | **Total Rs:-** |  |
| PART "B" |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below W/S & S/F Schedule Items | | | **Total Rs:-** |  |
|  |  |  |  |  | **G. Total Rs:-** |  |
|  |  |  |  |  |  |  |
| CONTRACTOR | | |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR | | |