**SCHEDULE-“B” / BOQ-4**

**(B)**

**NAME OF WORK:– RECONDITIONING INTERNAL ROAD OF SCARP COLONY NAUSHAHRO FEROZE ROAD MILE 0/0 – 1/4**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.NO** | **ITEM** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
| 1 | Preparing Base Course including supplying and spreading stone metal of approved quality properly gauge to maximum size 1-1/2” in required thickness to proper camber and gauge i/c supplying and spreading 15Cft screening and on plastic quarry fines, filling depressions with stone metal after initial rolling including watering and compaction the same so as to achiever 100% density as per modified AASHO specification. Rate includes providing and using templates, camber plates, screen forms as directed. Rate all cost of materials T&P and carriage up to site of work etc | 47520 Cft | 9388.63 | % Cft | 4461477.00 |
| 2 | Laying bricks on end edging including supplying 9” x 4 – 1/2” x 3” 1st Class bricks, excavation for having edging with small size parallel to the road. Rate include lead up to 3 chains. | 15840 Rft. | 2729.93 | %Rft. | 432421.00 |
| 3 | Providing Surface Dressing 1st coat on new or existing surface with 30 lbs bitumen and 4 Cft crush bajri of required size including cleaning the road surface rolling etc complete. Rate includes all costs of materials T&P and carriage up to 3 chains. | 95040 Sft. | 1657.27 | %Sft. | 1575069.00 |
| 4 | Providing 1” thick (consolidated) premixed carpet in camber and grade including supplying 10 Cft crushed bajri 4 Cft hill sand of approved quality and grade bitumen of 80/100 penetration including mixing in mechanical mixer in required proportion including heating materials and cleaning the road surface (hill sand 2 cft for mixing and 2 cft dusting). Rate includes all cost of materials T & P and carriage up to 3 chains. | 95040 Sft. | 4638.24 | %Sft. | 4408183.00 |
| 5 | Earth work for embankment form borrows pits including lying 6” layers. Clod breaking ramming, dressing complete, lead up to 100ft in ordinary soils 85% density without extra lead | 67320 Cft. | 7723.95 | %o Cft. | 519976.00 |
| **Total RS:** | | | | | **11397126.00** |
| **Add \_\_\_\_\_\_% above / below on Schedule Items Rs:** | | | | |  |
| **G-Total RS:** | | | | |  |

**CONTRACTOR EXECUTIVE ENGINEER**

**KHAIRPUR DRAINAGE DIVISION**

**KHAIRPUR**