**SCHEDULE “B”**

**NAME OF WORK: REHABILITATION, IMPROVEMENT, RENOVATION & PROVISION FOR**

**MISSING FACILITIES IN EXISTING PRIMARY SCHOOL GOVT: BOYS**

**PRIMARY SCHOOL AT WARYAM KOSH TALUKA UBAURO**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sr;No:** | **Name of Item** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1. | Excavation in foundation of building bridges and other structures including dag belling dressing, refilling around structure with excavated earth watering and ramming lead upto 5 ft (S. I No: 18 P. No: 4) | | | | |
|  |  | 4245.0 | 1306/80 | %CFT | Rs:13483/- |
| 2. | Cement concrete brick or stone ballast 1 ½ “ to 2” gauge 1:5:10 (S. I No: 4 (c) P. No: 15). | | | | |
|  |  | 1059.0 | 5445/- | %CFT | Rs:91861/- |
| 3. | Pacca brick work in foundation and plinth in cement sand mortar 1:6 (S. I No: 4 (e) P. No: 21). | | | | |
|  |  | 3297.0 | 121/- | %CFT | Rs:393937/- |
| 4. | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle) 1:2:4 (S. I No: 6 a i P. No: 17) | | | | |
|  |  | 564.0 | 337/- | P:cft | 190068/- |
| 5. | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of mild steel (S. I No: 8 (b) P. No: 17) | | | | |
|  | Tor bar | 27.696 | 5001/70 | P;CWT | Rs:138527/- |
|  |  |  |  |  |  |
|  | M.Steel | 5.035 | 4820/20 | P:CWT | Rs:24270/- |
| 6. | Pacca brick work in other then building in cement sand 1:6(SI:NO: P. ) | | | | |
|  |  | 3370.0 | 12346/65 | %sft | Rs:465469/- |
| 7. | Erection and removal of centering for R.C.C or plain cement concrete works of Deodar wood (2nd-Class)(SI: No:19(b)(ii)P.17) | | | | |
|  |  | 437.0 | 3127/41 | %CFT | Rs:13667/- |
| 8. | Cement concrete plain i/c placing compacting finishing and curing complete (i/c screening and washing at stone aggregate without ratio 1:2:4(SI.No.5(f)P.15) | | | | |
|  |  | 164.0 | 14429/25 | %SFT | Rs:23664/- |
| 9. | Cement plaster 1:6 upto 20’ height ½ “ thick (S. I No: 13 (b) P. No: 52). | | | | |
|  |  | 9278.0 | 2206/60 | %SFT | Rs:204728/- |
|  |  |  |  |  |  |
| 10. | Cement plaster 1:4 upto 20’ height 3/8” thick (S. I No: P. No: 52). | | | | |
|  |  | 9278.0 | 2197/52 | %SFT | Rs:203886/- |
| 11. | Cement Pointing struck joints on walls ration 1:2 (SI:NO:19P.52) | | | | |
|  |  | 4433.0 | 1287/44 | %SFT | Rs;57072/- |
| 12. | M/F steel grated door with 1/16”thick sheeting i/c angle iron frame 2”x2”x3/8” and ¾”square bars 4”centre to centre with locking agrrangement (SI.No.24P.No.91) | | | | |
|  |  | 60.0 | 726/72 | P:SFT | Rs:43603/- |
| 13. | White wash three coat (SI.No.26© P. No.53) ) | | | | |
|  |  | 9278.0 | 829/95 | %SFT | Rs:77003/- |
| **Sr;No:** | **Name of Item** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 14. | Colour wash two coats (SI.No. 25 (b) P.No.53 ) | | | | |
|  |  | 4433.0 | 859/90 | %SFT | Rs:38119/- |
| 15. | Preparing surface and painting guards bars gates iron bars railing (S.I No: 41 (j) P.No: 69). | | | | |
|  |  | 120.0 | 1270/83 | %SFT | Rs:1525/- |
| 16. | Providing and laying HALA or gattewrn tilles glazed 8" x 8" x1/4" on floor or wall facing in required pattern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slurry of white cement and pigment in desired shape with finishing , cleaning and cost of wax ploish etc. complete including cutting tiles to proper profile.(SI:NO:62P.48) | | | | |
|  |  | 112.0 | 34520/31 | %SFT | Rs:38663/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total** | **2022575/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**

**CONTRACTOR**