|  |  |  |
| --- | --- | --- |
| **NAME OF WORK :-** | **M/R TO SINDH SECRETARIAT NO. III OLD K-D-A BUILDING KARACHI**  **( REPAIR WORKS IN OFFICE OF SECRETARY IPC & DEPUTY SECRETARY IPC GROUND & 3RD FLOOR)** |  |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS (A)** |  |  |  |  |
| 1. | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 2232.00Sft. | 226/88 | %Sft | 5064/- |
|  | Rupees. two hundred twenty six. And. Eighty eight. Paisa | | | | |
| 2 | Preparing the surface and painting with matt finish paint of approved make to old matt finish ( b ). 2nd & subsequent coat. ( SI.37(A+B) / P-55 ). | 2975.61 Sft | 1772/38 | %Sft | 52739/- |
|  | Rupees. one thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | |
| 3 | Distempering.( b ) Two coats.( SI.24(b) / P-54 ). | 417.50 Sft | 1043/90 | %Sft | 4358/- |
|  | One thousand & fourty three. And. Ninety. Paisa | | | | |
| 4 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2” thick Teak wood ply shutters of 2nd class deodar wood skeleton ( solid ) styles and rails core of Partal wood and commercial ply wood ( 3-Ply ) on both side in/c hold fasts, hinges, Iron tower blots, handles and cleats with cord etc complete. ( SI.58 / P-65 ) – ( SI.25-b / P-61 ) Rs.1077/06 ( - ) Rs.370/83 = 706/23 | 65.00 P.Sft | 706/23 | P.Sft | 45905/- |
|  | Rupees. seven hundred & six. And. Twenty three. Paisa | | | | |
| 5 | Providing and fixing with sunk iron screws wooden Architrave approved design/ shape having width not less than 2- 1/2 inches as directed by Engineer Incharge. ( SI.60/P-66 ) | 297.00 P.Rft | 49/97 | P.Rft | 14841/- |
|  | Rupees. forty nine. And. Ninety seven. Paisa | | | | |
|  | **Total** | | | | **122908/-** |
|  | Above / Below Rs. | | | |  |
|  | **(A). Total Rs.** | | | |  |
|  | **NON-SCHEDULE ITEMS (B)** |  |  |  |  |
| 1 | P/F door closer heavy type (OPAL OR KGI) make i/c. fixing on door with screws and adjusting speed as required etc . complete and as directed by Engineer Incharge. | 03 Nos |  | Each |  |
| 2 | P/F door lock (Handle Type) of approved quality and make as directed by Engineer Incharge. | 03 Nos |  | Each |  |
| 3 | P/F proper heavy type fancy L-Drop 12’’ long in/c all cost of labour material etc complete. | 03 Nos |  | Each |  |
| 4 | French polish of door / windows etc including preparing surface and polish by using lakh Dana ,sprit, thinner, pigment, ICI lacquer, Regmal (Germany) material ICI sealer tar pine oil, polishing as per satisfaction of competent authority etc complete. | 235.00 P.Sft |  | P.Sft |  |
| 5 | S/F bath room accessories set (Master make) (7 pieces) in/c soap dish, looking mirror shelf tray, tower rails, paper holder etc complete. | 01 Nos |  | Each |  |
| 6 | P/F sanitary fitting chrome plated heavy gauge of approved quality (Irfan or equivalent make) fitted with completed accessories as directed by the Engineer Incharge. Side Pillar Cock . ½” dia. | 01 Nos |  | Each |  |
| 7 | P/F Double Bib Cock / Long Bib Cock 1/2” dia plastic coated A Class as directed by the Engineer Incharge. (Irfan Make) | 02 Nos |  | Each |  |
| 8 | P/F sanitary fitting chrome plated heavy gauge of approved quality (Sonex / Master make) fitted with completed accessories as directed by the Engineer Incharge. Muslim shower. ½” dia. | 2 Nos |  | Each |  |
| 9 | P/F sanitary fitting chrome plated heavy gauge of approved quality (Irfan or equivalent make) fitted with completed accessories as directed by the Engineer Incharge. Stop Cock /Bib Cock / Tee Cock . ½” dia | 05 Nos |  | Each |  |
| 10 | P/F Aluminum partition with fixed glass (frosted) 5mm thick using 4” lucky section in champion color as frame on floor or block masonry fixed with necessary fixtures rubber packings etc. The cost in/c tools & plants used in making and carriage from shop to site as directed by the Engineer Incharge. | 78.00 Sft. |  | P/Sft. |  |
| 11 | P/Fixing fiber glass shade with fiber glass sheet 2-3mm thick including necessary frame work of angle iron or G.I pipe & fixing sheet with screws in proper design & shape as directed by Engineer Incharge. | 90.00 Sft. |  | P/Sft |  |
|  |  | **(B). Total Rs.** | | |  |
|  |  | **(A). Total Rs.** | | |  |
|  |  | **(A+B) Total Rs.** | | |  |
|  |  | **Say** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |