|  |  |
| --- | --- |
| **NAME OF WORK :** | **M/R TO SINDH SECRETARIAT NO.III ( OLD K.D.A ) BUILDING KARACHI.**  **(P/L SEWERAGE LINE IN/C PAVERS @ BACK SIDE & ADDITIONAL WORK OF LIBRARY).** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORK )** |  |  |  |  |
| 1 | Providing and laying 1: 3: 6 cement concrete solid block masonry wall 6” and below in thickness set in 1:6 cement mortar in ground floor Super Structure including raking out joints & curing etc, complete.( SI.24 / P-19 ). | 126.00 Cft | 15771/01 | % Cft | 19871/- |
|  | Rupees. fifteen thousand seven hundred seventy one. And. One. Paisa | | | | |
| 2 | Cement Plaster 1:5 upto 12’ height.( a ) 3/8” thick ( SI.12-a / P-52 ). | 568.66 Sft | 2166/72 | %Sft | 12321/- |
|  | Rupees. two thousand one hundred sixty six. And. Seventy two. Paisa | | | | |
| 3 | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 3347.87  Sft | 226/88 | %Sft | 7596/- |
|  | Rupees. two hundred twenty six. And. Eighty eight. Paisa | | | | |
| 4 | Preparing the surface and painting with weather coat of approved make to old weather coat surface (Three coats). (39/A+B) | 3882.17 Sft | 1948/10 | %Sft | 75629/- |
|  | Rupees. one thousand nine hundred forty eight. And. Ten. Paisa | | | | |
| 5 | Providing & fixing cement paving blocks flooring having size of 197x97x60 (mm) of city / Quadra / cobble shape with natural colors, having strength b/w 5000 psi to 8500 psi i/c filling the joints with hill sand and laying in specified manner / pattern and design etc complete.( SI.71 / P-49 ). | 957.30 Sft | 199/77 | P.Sft | 191240/- |
|  | Rupees. one hundred ninety nine. And. Seventy seven. Paisa | | | | |
| 6 | Providing and fixing G.I frames /Chowkhat of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing.( SI.29/P-93 ). | 17.00 Rft | 228/90 | P.Rft | 3891/- |
|  | Rupees. two hundred twenty eight. And ninety. Paisa | | | | |
| 7 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2” thick Teak wood ply shutters of 2nd class deodar wood skeleton ( solid ) styles and rails core of partal wood and commercial ply wood ( 3-Ply ) on both side in/c hold fasts, hinges, Iron tower blots, handles and cleats with cord etc complete.( SI.58 / P-65 ) – ( SI.25-b / P-61 ) Rs.1077/06 ( - ) Rs.370/83 = 706/23 | 19.94 Sft | 706/23 | P.Sft | 14082/- |
|  | Rupees. seven hundred & six. Twenty three. Paisa | | | | |
|  |  |  | **Total Rs. (A)** | | **324630/-** |
|  |  | Above / Below Rs. | | |  |
|  |  | **Total Rs. (A).** | | |  |
|  | **NON-SCHEDULE ITEMS** |  |  |  |  |
| 1 | P/Making Sindh Secretariat name works (19) letters in sindhi fonts with solid steel in/c fixing with screw nut bolts in/c all cost of labour material + cartage etc complete. | 01 Job |  | P/Job |  |
| 2 | S/F LED spot light China make with 12 Nos lamps each 12 watts fitted on walls, ceiling of approved quality as directed by the Engineer Incharge. | 27 Nos |  | Each |  |
| 3 | P/F New Fibre Glass tank 500 gallons having wall thickness upto 8mm of approved quality & design and wall thickness as specified in/c. cost of nuts & Bolts and fixing on plate form and making connection for inlet outlet & over flow inlet / outlet floor pipes etc. complete (Master Brand). The cost include carriage from shop to site & lifting from ground floor to roof of any floor as directed by the Engineer Incharge. | 01 No |  | Each |  |
| 4 | P/F UPVC water supply pipe of AGM or Pak Arab make schedule 40(E) ASTM standard D-1785 with all necessary fittings like elbow, bend, tee etc. This includes fixing on walls with clamps or Jubilee clips upto height of 50’-0 invertical or horizontal position using Jhoola or long ladder or scaffolding and jointing pipe & fittings with approved solvent / JTG solution. The rate includes all cost of labor, material, and cartage, as directed by Engineer Incharge **3/4” dia.** | 78.00 Sft |  | P.Sft |  |
| 5 | P/F UPVC handle valve ¾” dia of approved quality & make as directed by the Engineer Incharge,. | 04 Nos |  | Each |  |
| 6 | Repair of aluminum windows .removing windows P/F new packing rubber channel wheels and replacing broken handles and hinges refixing the windows at same place in\c all cost of labour material and cartage etc complete | 16 Nos |  | Each |  |
|  |  |  | **(B). Total Rs.** | |  |
|  |  |  | **(A). Total Rs.** | |  |
|  | **G. Total (A+B) = Rs.** | | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |