**Name of work: M/R TO DRIVER RESIDENCY AT CHIEF MINISTER HOUSE KARACHI.**

**SCHEDULE B**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **Description** | **Qty** | **Rate** | **Unit** | **Amount** |
| **1** | Scraping ordinary distemper oil bound distemper or paint on walls. (S.I-54(a)/15) | 4907.28 | 226/28 | %SFT | 11133 |
| **2** | Distempering. (c) Three Coat. (S.I-24(c)/54) | 621.04 | 1079/65 | %SFT | 6705 |
| **3** | Providing & Laying 2” thick topping cement concrete (1:2:4) including Surface finishing and dividing into panels. (S.I-16(c)/42) | 1631.74 | 3275/50 | %SFT | 53448 |
| **4** | Cement Plaster 1:4 upto 12' height. (d) 3/4" thick (only for block masonry). (S.I-11(d)/52) | 1631.74 | 3191/76 | %SFT | 52081 |
| **5** | Cement plaster 1:6 upto 12' height. (c) 3/4" thick (S.I-13(c)/52) | 1631.74 | 2590/50 | %SFT | 42270 |
|  | Total |  |  |  | 165637 |
|  | Part B NSI |  |  |  |  |
| **1** | Repairing old surface & painting with Matt Finish i/c. filling of joints and cracks with fine finishing including all respect labour, as directed by the Engineer Incharge etc. complete. | 4286.29 |  | SFT |  |
| **2** | Providing and laying fancy type Porcelain glazed tiles as per required size specified approved quality / make / design and colour including laying with bond solution sand mortar including jointing in white cement including washing of tiles and filling of joints with Slurry of white cement in desired shape with finishing including cutting of tiles to proper profile i/c. all respect labour and necessary required material as directed by the Engineer Incharge etc. complete. | 2022.38 |  | SFT |  |
| **3** | Providing and fixing fiber glass tank 600 gallons capacity as approved quality etc. complete. | 2-NOS |  | EACH |  |
| **4** | P/F Wash Basin with Pedestal etc. complete in all respect (Imported make) | **4-NOS** |  | **EACH** |  |
| **5** | S/F Wash Basin Mixture of superior quality with CP head 3/4" dia (Imported make) | **4-NOS** |  | **“** |  |
| **6** | P/F Stainless steel floor trap jalli imported make etc. complete. | **8-NOS** |  | **“** |  |
| **7** | P/F Indian WC i/c. flushing cistern and also etc. complete in all respect. | **4-NOS** |  | **“** |  |
| **8** | P/F Double Bib Cock 1/2" dia Plastic / Powder coated Master "A" Class as directed by the Engineer Incharge. | 8-NOS |  | “ |  |
| **9** | S/F CP brass concealed T-stop cock of superior quality with crystal head 1/2" dia (Master make) | 12-NOS |  | “ |  |
| **10** | Supplying & Fixing sink mixture cock of superior quality with c.p head etc. complete. | 4-NOS |  | “ |  |
| **11** | P/F double burner gas stove of stainless steel i/c. S/I with all fitting & all fixture. | 4-NOS |  | “ |  |
|  | **Total B** |  |  |  |  |
|  | **G Total** |  |  |  |  |

TERMS & CONDITION

1. Any typographical errors in the schedule B are subject to the correct condition with Reference to the schedule of rate General 2012 enforced from 12-07-2012 as approved by the SRC Sindh.
2. Arbitraction clause stands deleted from the agreement.
3. No Premium shall be paid on Non Schedule Items
4. 100% well Graded crushed bajri shall be used in items of work without any extra payment.
5. No any items of exveceed then the quantity provided in the schedule B without prior of the Executive Engineer.
6. All sample of items should be got approved by the Executive Engineer

Contractor

Assistant Engineer,

Provincial Buildings sub Division-IX,

Karachi