|  |  |
| --- | --- |
| **NAME OR WORK :-** | **M/R TO SINDH SECRETARIAT NO- I, (NEW BUILDING) KARACHI**  **PROVIDING PARTITION IN DINING HALL CEMENT IN CONFERENCE ROOM IN/C COLORING, PAINTING, & MISC: WORKS @ 7TH FLOOR** |

**“ SCHEDULE ‘B’ “**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.#** | **DESCRIPTION OF ITEMS** | **QTY:** | **RATE** | **UNIT** | **AMOUNT** |
|  | **SCHEDULE ITEMS PART-“A” ( CIVIL WORKS )** | |  |  |  |
| 1 | Scraping ( b) Ordinary distemper oil bound distemper or Pain on Walls. ( SI.54-(b) / P-13 ). | 2066.00-Sft | 226/88 | %Sft | 4687/- |
|  | Rupees. two hundred twenty six. And. Eighty eight. Paisa | | | | |
| 2 | Preparing the surface & painting with matt finish paint of approved make to old matt finish surface (2nd & subsequent coat (37-a+b / P-55) | 2066.00-Sft | 1772/38 | %Sft | 36617/- |
|  | Rupees. one thousand seven hundred seventy two. And. Thirty eight. Paisa | | | | |
| 3 | Supplying & fixing imposition Aluminum channels framing for hinged doors of Alcop made with 5 mm thick tinted glass glazing ( Belgium ) and Alpha ( Japan ) locks in/c handles, stoppers etc.( a ) Deluxe model (White).( SI.83-a / P-108 ). | 49.00 Sft | 1450/76 | P.Sft | 71087/- |
|  | Rupees. one thousand four hundred fifty. And. Seventy six. Paisa | | | | |
|  |  |  | **Total Rs:** | | **112391/-** |
|  | Above / Below Rs. | | | |  |
|  |  | **(i). Total Rs:** | | |  |
|  | **NON-SCHEDULE ITEMS.** |  |  |  |  |
| 1 | S/F SCG sheera board partition wall high impact strength with galvanized C-74 and 476 framing 0.55 thick, fixing both sides jiber cement sheet 10-mm resist to moisture, heat, & then putting poly urethane / rock full form with mixing of glass powder & covering both side expended metal (For sound proofing) as directed by the Engineer Incharge. | 185.00-Sft |  | PSft |  |
| 3 | S/F solid fully teak wood flooring (WOOD MAN) size 15mm x 90mm x 400mm fitted on floor & skirting pasting with glue or binding solution filing joints with pigment, cutting, wastage, carriage etc in/c in this rate as directed by the Engineer Incharge. | 610.00-Sft |  | PSft |  |
| 4 | P/F fine quality roller type blind with approved design false & in/c steel angle fixing with steel screws as per window as required @ site as directed by the Engineer Incharge. | 549.00-Sft |  | PSft |  |
| 5 | P/F Gypsum board pelmet to be hanged from ceiling in specified shape and design as approved by the consultant. This in/c cutting the existing Gypsum board false ceiling in proper shape, hanging the structure by aluminum angle 1’x1” @ 3’-0 apart drilled and screwed in RCC slab, making hanging frame by using Aluminum U-channel section 1-1/2” wide in 18”x18” rafters and fixing Gypsum board sheet with chips and screws. Then filling the joints & screws holes with plastic mesh and plaster of Paris and making surface smooth as directed by the Engineer Incharge. | 1187-Sft |  | PSft |  |
| 6 | French polishing of doors windows ventilators stair floor work etc includes preparing surface and polishing by using Indian lakh Dana, spirit, thinner, pigment, ICI Lacquer, ICI hardener, Regmal (Germany) material ICI sealer tar pine oil, polishing as per satisfaction of competent authority etc complete | 675.00-Sft |  | PSft |  |
|  |  | **(ii). Total Rs.** | | |  |
|  |  | **(i). Total Rs.** | | |  |
|  |  | **Part “A” Total Rs.** | | |  |
|  | **Part (B) Electrification.** |  |  |  |  |
| 1 | Wiring for light or fan point with 3/.029 PVC insulated wire in 20mm ( ¾” ) PVC conduit on surface as required. ( SI.123 / P-15 ) | 32-Nos | 797/- | P.Point | 25504/- |
|  | Rupees. seven hundred ninety seven. Only. | | | | |
| 2 | Providing & laying (MAIN or SUB MAIN ) PVC insulated with size 2-7/.029 copper conductor in ¾” dia PVC conduit on surface.( SI.03 / P-01 ). | 20-Meter | 171/- | P.Meter | 3420/- |
|  | Rupees. one hundred seventy one. Only. | | | | |
| 3 | Providing & laying ( MAIN or SUB MAIN ) PVC insulated with size 2-7 / .044 ( mm2 ) copper conductor in 1” dia PVC conduit on surface.( SI.05 / P-01 ). | 38-Meter | 305/- | P.Meter | 11590/- |
|  | Rupees. three hundred & five. Only. | | | | |
|  |  | **Part (B) G. Total Rs.** | | |  |
|  | **A B S T R A C T** | | | |  |
|  |  | **Part (A) G. Total Rs.** | | |  |
|  |  | **Part (A+B) G. Total Rs.** | | |  |
|  |  | **Say Rs.** | | |  |

**CONDITION.**

1). Typographical errors in the schedule-“B” are the subject to the correction with reference to the schedule of rate ( Gen: Vol: III, Part-II, inforced: 2012, as approved by the standing rates committee.

2). No Cartage will be paid on any items of works.

3). No premium shall be paid on Non-Schedule items.

4). Water shall be arranged by the Contractor.

|  |  |  |
| --- | --- | --- |
| **CONTRACTOR.** | **ASSISTANT ENGINEER**  **PROVINCIAL BUILDINGS SUB-DIVISION-V,**  **KARACHI.** | **EXECUTIVE ENGINEER**  **PROVINCIAL BUILDINGS DIVISION-II,**  **KARACHI.** |