|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

PART-E W/S & S/F (**N.S.I Item)**

01/- P/F I.C.L Porta company aorisa WC i/c flushing cistern complete in all respects (Italina Forte Modle).

= 07 No’s

= 07 No’s

02/- P/F I.C.L on Porta company English commode with seat cover i/c flushing cistern complete in all respect (Italina Forte Modle).

= 01 No’s

= 01 No’s

03/- P/F I.C.L on Porta company wash basin with pedestal complete in all respect. (Italina Forte Modle).

= 23 No’s

= 23 No’s

04/- P/F UPVC terminal guard 4” Dia complete in all respect.

3” Dia = 150 Rft

4” Dia = 150 Rft

6” Dia = 150 Rft

05/- P/F bath room accssories set of (23 pieces) Master/Sonex equivalent etc complete.

= 23 No’s

= 23 No’s

06/- water Tank 500 Gallons.

= 02 No’s

= 02 No’s

07/- Providing & Fixing Cancelead “T” Stop Cock1/2” (Code # 010)

= 06 No’s

= 06 No’s

08/- Providing & Fixing C.P Brass Handle valve etc complete

¾” Dia = 04 No’s

09/- Providing & Fixing C.P Brass wash basin Mixture (Master/Sonex or equivalant).

= 23 No’s

10/- Providing & Fixing C.P Brass Double Bib Cock (Code# 05880 with Muslim Shower(Master/Sonex or equivalant).

= 01 No

11/- P/F UPVC floor trap 6”x2” or 6”x3” Dia i/c steel floor Jali grade -1 (Dadex or equivalant) i/c cutting fitting with Coller clamps & solvent this rate also i/x Making holes in walls plinth floor and roof for fixing pipe & making good in c.c 1:2:4 twsting pressure head 200 feet.

4” Dia = 10 No’s

12/- Geezer.

= 01 No

13/- Pillars and walls Groves Dsign etc complete up to 30 ft: height.

= 30 Rft

14/- Providing & Fixing Minars etc complete

= 04 No’s

15/- Providing & Fixing C.C Ornamental Jalli etc complete.

=

16/- G-I Pipe etc complete

½” = 200 Rft

¾” Dia = 200 Rft

1” Dia = 200 Rft

=====================================

Total RS:

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work |  | QTY | Rate | Unit | Amount |

PART-D P.H.S Item

01/- Construction of manhole or inspection chamber for the required dia

of circular sewer and 3’-6’ (1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over beching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46).

Qty:03 Nos @Rs:14748/- each RS: 44244/-

02/- Supplying & Fixing water pumping set 3” H.P complete

Qty: 03 No @RS: 17000 each RS: 34000/-

===================================

Total RS: 78244/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR