**NAME OF WORK:- REHABLITATION / REPAIR OF BASIC HEALTH AT ZAFAR ABAD TALUKA FAIZ GUNJ DISTRICT KHAIRPUR.**

(**SCHEDULE -B)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

01/- Dismantlling of R.C.C work etc complete.

Qty: 1034 Cft @RS: 5445/- % Cft RS: 56301/-

(fifty four hundreds fourty five ruppes).

02/- Dismantling Pacca Brick work in lime or sand etc complete

Qty: 798 cft @RS: 1285.63 % Cft RS: 10259/-

(tweleve hundreds eight five rupees sixity three ps:)

03/- Dismantling cement concrete plain ratio 1:2:4 etc

Qty: 558 cft @RS: 3327.50 % Cft RS:18567/-

(thirty three hundreds twenty seven rupees fifty ps)

04/- Removing cement or lime plaster (S.I NO: 18 P.NO: 20).

Qty: 1768 sft @RS: 121/- % Sft RS: 2139/-

(One hundred twenty one rupees)

05/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 1200 Cft @RS:3176.25 % Cft RS: 3811/-

Thirty one hundred seventy six rups:twenty five ps:

06/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 369 Cft @RS: 8694.95 % Cft RS: 32084/-

(Eight six hundreds ninty four rupees,ninty five ps:)

07/- Pacca Brick work in foundation / Plint in cement

cement & sand mortar ratio (1:6)(S.I No:05 (c)P.No:20)

Qty: 968 Cft @RS: 11948.36 % Cft RS:115660/-

(Eleven thousands nine hundered fourty eight rs: thirty six ps.)

08/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 1048cft @RS: 337/- P.Cft RS: 353176/-

(Three hudred thirt seven ps.)

09/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 46.785cwt @RS:5001.70 P.cwt RS: 234008/-

(Five thousands & one ripes, seventy ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

10/- Pacca Brick work in Other than building 1:6 (S.I No:7 eP-21).

Qty: 798 cft @RS: 12346.65 % Cft RS: 98526/-

(Tweleve thousands three hundred fourty six rups: sixty fiveps.)

11/- Applying floating coat of cement (S.I NO: 14 P.NO: 52)

Qty: 1768 sft @RS: 660/- % Sft RS: 11669/-

(Six hundreds sixty rupees)

12/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 1768 Sft @RS: 3015.76 % Sft RS: 53319/-

( Three Thousands Fifteen Rupees Seventy Six Ps:.)

13/- Cement Plaster 1:6 up to 20”-0 heights ½”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2268 Sft @RS: 2206.60 % Sft RS: 50046/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

14/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2268 Sft @RS: 2197.52 % Sft RS: 49840/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

15/- Cement Pointing on Stone work etc (S.I NO: P.NO: )

Qty: 980 Sft @RS: 1213.58 % Sft RS: 11893/-

(tweleve hundreds thirteen rups: fifty eight ps:)

16/- Providing and lying 1” thick C/C topping cement concrete (1:2:4) i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.42).(3” thick).

Qty: 1846 sft @RS: 4411.82 % Sft RS: 81442/-

(fourty four hundreds eleven rupees eighty two ps:)

17/- Providing and lying 1” thick C/C topping cement concrete (1:2:4) i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.42).(2” thick).

Qty: 1954 sft @RS: 3275.50 % Sft RS: 64003/-

(fourty four hundreds eleven rupees eighty two ps:)

18/- Two coats of Bitumen hot using 34 Lbs (S.I NO: P.NO: ).

Qty: 1954 Sft @RS: 1887.04 % Sft RS: 36873/-

(eighteen hundreds eighty seven rupees four ps:)

19/- Cement Concrete plain including placing Compacting

Finishing & curing, complete i/c screening & washing

Of stone aggregate Ratio (1:2:4) (S.I No:5 P-18).

[

Qty: 28 cft @RS: 14429.25 % Cft RS: 4040/-

( fourteen thousands four hundreds twenty nine rupes twenty five ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

20/- Laying Floor of approved with glazed tile ¼” thick in white cement 1:2 over ¾” thick cement mortar 1:2 complete (S.I No: 24 P.NO:43)

Qty: 164 sft @Rs:27678.86 % sft RS:45393/-

(twenty seven thousands six hundreds seventy eight rupees eighty six ps:)

21/- White Glazed tiles ¼” thick dado jointed in white cement and laid over 1:2 cement sand mortar ¾” thick including finishing (S.I No:37 P.No;45).

Qty:608 sft @Rs:28253.61 % sft RS:172390/-

22/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for door using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 72 Rft @RS: 228/90 P.Rft RS: 16430/-

(Two hundred twenty eight rupees, ninty ps.)

23/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for window using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 96 Rft @RS: 240.50 P.Rft RS: 23088/-

(Two hundred fourty rupees, fifty ps.)

24/- Supplying and fixing in position iron/steel grill of ¾” x ¼” size flat iron of approved design including painting 3 coats etc complete (Weight or not less than 3.7 Lbs/sq feet of finished grill

(S.I No: P.NO: ).

Qty: 24 Sft @RS: 180.50 P.Sft RS: 4332/-

(One hundred eighty rupees, fifty ps.)

25/- First class deodar wood wrought joinery in doors & windows etc fixed in position including hold fasts hinges iron tower bolts chock, cleats handles and cords with hooks etc complete. (S.I No: 54 P.NO: 65).

Qty:268 Sft @RS:902.92 P.Sft RS: 241985/-

(Nine hundred two rupees, ninty two ps.)

26/- Making & Fixing Steel grated door with 1/16” thick sheeting including angle iron frame 2”x2”x3/” and square bars 4” center to center with locking arrangement .(S.I NO:24)P.NO:92

Qty: 70 sft @RS: 726.72 P.Sft RS: 50870/-

(seven hundred twenty six rupes, seventy two ps.)

27/- White washing 03 three coats (S.I No: P.NO: ).

Qty: 1044 Sft @RS: 829.95 % Sft RS: 8665/-

(eight hundreds twenty nine rupees ninty five ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

28/- Colour washing two 02 coats etc

Qty: 4514 Sft @RS: 859.90 % Sft RS: 38816/-

(Eight hundred fifty nine rupees, ninty ps.)

29/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 4692 Sft @RS: 442.75 P.Sft RS: 20774/-

(Four hundred fourty two rupees, seventy five ps.)

30/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 4692 Sft @RS: 1079.65 % Sft RS; 50657/-

(ten hundreds Seventy Nine rupees , Ninty ps.)

31/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty: 874 Sft @RS: 1160.06 % Sft RS: 10139/-

==================================

**Total RS: 1950909/-**

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

NON-RESIDENTIAL (**SCHEDULE -B)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

01/- Removing cement or lime plaster (S.I NO: 18 P.NO: 20).

Qty: 1222 sft @RS: 121/- % Sft RS: 1479/-

(One hundred twenty one rupees)

02/- Dismantling cement concrete plain reionoferced separating reionofercemetn from concrete cleaning and starightheing the same 1:3:6 (S.I NO;20 P.11).

Qty: 69 cft @RS: 1306.80 % Cft RS: 902/-

(thirteen hundreds six rupees eighty ps:)

03/- Scarping Ordinary Soil Distempering oil bond etc.

Qty: 4448 Sft @RS: 226.88 % SFt RS: 10092/-

(two hundreds twenty six rupees eighty eight ps:)

04/- Excavation in foundation of building bridges and other structures i/c dag balling dressing refilling around structure with excavated earth watering and ramming lead up-to 5ft. (b) in ordinary soil. (S.I.No.18 (b) P.No.5)

Qty: 252 Cft @RS:3176.25 % Cft RS: 800/-

Thirty one hundred seventy six rups:twenty five ps:

05/- Cement concrete stone of brick ballast 1½” to 2” gauge. Ratio (1:5:10). (S.I.No.4 (b) P.No.14)

Qty: 65 Cft @RS: 3894.95 % Cft RS: 2532/-

(thirty eight hundreds ninty four rupees ninty five ps:)

06/- Un- Coursed rubble masonry dressing dry masonry (S.I No:1 P-27).

Qty: 180 Cft @RS: 17723/- % Cft RS: 31901/-

(Seventeen thousands seven hundreds twenty three rup:)

07/- Coursed Rubble Masnory 1:6 including hammer dressing (S.I No: 2 d P.26).

Qty: 67 Cft @RS: 25321/- % Cft RS: 16965/-

(twenty five thousands three hundreds te=wenty one rups:)

08/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 69cft @RS: 337/- P.Cft RS: 23253/-

(Three hudred thirt seven ps.)

09/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 3.08 cwt @RS:5001.70 P.cwt RS:15405/-

(Five thousands & one ripes, seventy ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

10/- Pacca Brick work in Other than building 1:6 (S.I No:7 eP-21).

Qty: 344 cft @RS: 12346.65 % Cft RS: 42472/-

(Tweleve thousands three hundred fourty six rups: sixty fiveps.)

11/- Making & Fixing Steel grated door with 1/16” thick sheeting including angle iron frame 2”x2”x3/” and square bars 4” center to center with locking arrangement .(S.I NO:24)P.NO:92

Qty: 80 sft @RS: 726.72 P.Sft RS: 42472/-

(seven hundred twenty six rupes, seventy two ps.)

12/- Cement Plaster 1:6 up to 20”-0 heights ½”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 630 Sft @RS: 2206.60 % Sft RS: 13902/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

13/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 630 Sft @RS: 2197.52 % Sft RS: 13844/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

14/- Applying floating coat of cement (S.I NO: 14 P.NO: 52)

Qty: 1222 sft @RS: 660/- % Sft RS: 8065/-

(Six hundreds sixty rupees)

15/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 1222 Sft @RS: 3015.76 % Sft RS: 36852/-

(three thousands fifteen rupees seventy six ps:)

07/- Pacca Brick work in foundation / Plint in cement

cement & sand mortar ratio (1:6)(S.I No:05 (c)P.No:20)

Qty: 968 Cft @RS: 11948.36 % Cft RS:115660/-

(Eleven thousands nine hundered fourty eight rs: thirty six ps.)

08/- R.C.C. work in roof slab beams columns rafts lintels and other structural members laid in situ or precast laid in position complete in all respects: (i) Ratio (1:2:4) .(S,I No:06 P-19).

Qty: 1048cft @RS: 337/- P.Cft RS: 353176/-

(Three hudred thirt seven ps.)

09/- Fabrication of mild steel reinforcement for cement Concrete i/c cutting bending laying in position making joints and fastenings i/c cost of binding wire (also includes removal of rust from bars) (a) Using tor bars. (S.I.No.7 (a) P.No.20)

Qty: 46.785cwt @RS:5001.70 P.cwt RS: 234008/-

(Five thousands & one ripes, seventy ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

10/- Pacca Brick work in Other than building 1:6 (S.I No:7 eP-21).

Qty: 798 cft @RS: 12346.65 % Cft RS: 98526/-

(Tweleve thousands three hundred fourty six rups: sixty fiveps.)

11/- Applying floating coat of cement (S.I NO: 14 P.NO: 52)

Qty: 1768 sft @RS: 660/- % Sft RS: 11669/-

(Six hundreds sixty rupees)

12/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 1768 Sft @RS: 3015.76 % Sft RS: 53319/-

( Three Thousands Fifteen Rupees Seventy Six Ps:.)

13/- Cement Plaster 1:6 up to 20”-0 heights ½”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2268 Sft @RS: 2206.60 % Sft RS: 50046/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

14/- Cement Plaster 1:4 up to 20”-0 heights 3/8”” thick. . ( S.I NO: 11(a) P:NO:52 )

Qty: 2268 Sft @RS: 2197.52 % Sft RS: 49840/-

(Twenty one hundred ninty seven rupees, fifty two ps.)

15/- Cement Pointing on Stone work etc (S.I NO: P.NO: )

Qty: 420 Sft @RS: 1213.58 % Sft RS: 5097/-

(tweleve hundreds thirteen rups: fifty eight ps:)

16/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for windows using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 48 Rft @RS: 240.50 P.Rft RS: 11544/-

(Two hundred fourty rupees, fifty ps.)

17/- Providing and fixing G.I frames/chowkhats of size 7”x2” or 4½”x3” for Door using 20 gauge G.I sheet i/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S.I.No. 28 Page No. 93)

Qty: 36 Rft @RS: 228/90 P.Rft RS: 8240/-

(Two hundred twenty eight rupees, ninty ps.)

18/- Providing and lying 1” thick C/C topping cement concrete (1:2:4) i/c surface finishing and dividing into panels. (S.I.No.16 (d) P.No.42).(3” thick).

Qty: 276 sft @RS: 4411.82 % Sft RS: 12177/-

(fourty four hundreds eleven rupees eighty two ps:)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr | Item of work | QTY | Rate | Unit | Amount |

19/- First class deodar wood wrought joinery in doors & windows etc fixed in position including hold fasts hinges iron tower bolts chock, cleats handles and cords with hooks etc complete. (S.I No: 54 P.NO: 65).

Qty:90 Sft @RS:902.92 P.Sft RS: 81264/-

(Nine hundred two rupees, ninty two ps.)

20/- White washing 02 coars.

Qty: 1172 sft @RS: 425.84 % Sft RS: 4991/-

(four hundreds twenty five rupees eighty four ps:)

21/- Priming coat of Chalk under distemper (S.I NO:23 P-53).

Qty: 4448 Sft @RS: 442.75 P.Sft RS: 19694/-

(Four hundred fourty two rupees, seventy five ps.)

22/- Distempering 02 wo coats (S.INO:24(b)P.53).

Qty: 4448 Sft @RS: 1079.65 % Sft RS; 46433/-

(ten hundreds fourty three rupees nonty ps.)

23/- Colour washing two 02 coats etc

Qty: 2866 Sft @RS: 859.90 % Sft RS: 24645/-

(Eight hundred fifty nine rupees, ninty ps.)

24/- Painting doors & Windows any type including edges of three coats (S.I NO:40 ii P 67).

Qty: 1040 Sft @RS: 1160.06 % Sft RS: 12065/-

25/- Painting guard bars gets iron bars grating , railing including standard braces (etc) and similar open work. (S.I NO:4(d)P.NO:69).

Qty:429 sft @RS: 605.60 % Sft RS: 2598/-

(six hundreds five rupees sixty ps☺ ==================================

**Total RS: 447212/-**

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work | No: L:B:D | QTY | Rate | Unit | Amount |

**PART- WATER SUPPLY**

1/- P/F squatting type white glazed of flushing cistern with internal fitting and flush pipe with band and making requisite Nos. of holes in wall plinth & floor for pipe connections and making good in

Cement concrete 1:2:4. (A) W.C pan of not less than 23” clear opening between flashing rims and 3 gallons flushing tank. With 4” dia C.I. tape. (S.I.NO.1(A) P.No.1)

Qty: 03 No @RS: 4802.60 each RS: 4803/-

(fourty eight hundreds two rupes sixity ps:)

2/- P/F 22”x16” lavatory basin in white glazed earthen ware complete with & i/c the cost of W.I or C.I cantilever brackets 6” built into wall painted white in two coats after a primary coat of red lead paint a pair of ½” dia chrome plate pillar traps 1-1/2” dia rubber plug & chrome plated brass chain 1-1/4” dia malleable iron or c.p brass traps malleable iron or brass union & making requisite number of holes in walls plinth & floor for pipe connection and making good in cement concrete 1:2:4 (standard pattern). Add extra for labour for providing & fixing of earthenware pedestal white or coloured glazed (Standard pattern) . (S.I.NO. 8 P. No.3)

Qty: 01 No @RS: 6237/- each RS: 6237/-

(Sixty two hundreds thirty seven rupes)

3/- Supplying & fixing Fiber Glass Tank of approved quality and design and wall thickness as specified i/c cost of nuts bolts and fixing in plate form of cement concrete 1:3:6 and making connection for in-let outlet & over flow in-let outlet flow pipes etc. complete. (S.I.No.3 P.No.18) (Rate per gallon Rs: 33/60 for tanks upto capacity of 250 gallons) 200 Gallons

Qty: 01 NO @RS: 21989.16 each RS: 21989/-

(twenty one thousands nine hundreds eight nine rupees sixteen ps:)

4/- Providing G.I pipes special & clamps etc i/c fixing cutting and fitting complete with and i/c the cost of breaking through walls and roof making good etc painting two coats after cleaning the pipe etc with white zink paint with pigment to match the colour of the building and testing with water to a pressure head of 200 feet and handling. **(Internal)** (i) ½ dia G.I pipe. (S.I.NO.1 (i) P. No.11)

“ “ ¾” dia 20 rft @RS: 95.79 P.Rft RS: 1916/-

(ninty five ruppes seventy nine ps:)

“ “ ½” dia 10 rft @RS:73.21 P.Rft RS:732/-

(Seventy three rupees twenty one ps:)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr | Item of work | No: L:B:D | QTY | Rate | Unit | Amount |

05/- Construction of manhole or inspection chamber for the required dia

of circular sewer and 3’-6’ (1067 mm ) depth with walls of B.B in cement mortar 1:3 cement plaster 1:3 ½” thick in side 1” (25 mm ) thick over beching and channel i/c fixing C.I main hole cover with frame of clear opening 1 ½”x 1 ½”” 457x457 mm) of 1.75 cwt . (88.9 kg) embedded in plain c.c 1:2:4) & fixing (25 mm) dia M.S steps 6” 150 mm) white projecting 4” (102 mm) from the face of walls at 12” (305 mm) c/c duly painted etc complete as per standard specification & drawing.(S.I No- P-46).

Qty:01 Nos @Rs:14748/- each RS: 14748/-

(fourtheen thousands seven hundreds fourty eight)

06/- Providing & Fixing R.C.C Pipe Collar glass Band digging the trenches to required depth and fixing in position including cutting , bending & fitting etc complete

Qty: 50 rft @RS: 250.60 P.Rft RS: 12530/-

(two hundreds fifty rupees sixty ps:)

=========================================

Total RS: 62955/-

\_\_\_\_\_\_% Above / Below (Amount to be added as per/deducted)RS:\_\_\_\_\_\_\_\_\_\_\_

G.Total RS:

Total Amount in word:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Note:- Quantities ans rates may be changed as per/according to the Techinical Sanction vy the competent authority.

EXECUTIVE ENGINEER

(BUILDINGS) WORKS & SERVICES

DEPARTMENT KHAIRPUR