**“SCHEDULE B”**

**NAME OF WORK: - SPECIAL REPAIR / ORDINARY REPAIR 2016-17 PROGRAMME**

**@ GOVT: BOYS DEGREE COLLEGE GHOTKI TALUKA GHOTKI.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | | **Amount** | |
| 1 | Dismantling brick work in lime or cement mortar (S. I No: 13 P. No: 10). | | | | | | |
|  |  | 371 | @ 1285/63 | %0Cft | | 4770/- | |
| 2 | Dismantling cement concrete reinforced separating reinfor cement from concrete cleaning and straightening the same. (S. I No: 20 P. No: 10). | | | | | | |
|  |  | 584 | @ 5445/- | %Cft | | 31798/- | |
| 3 | Removing cement or lime plaster (S. I No: 53 P. No: 13). | | | | | | |
|  |  | 3098 | @ 121/- | %Sft | | 3749/- | |
| 4 | Dismantling cement concrete plain 1: 3: 6. (S. I No: 19 (b) P. No: 10). | | | | | | |
|  |  | 475 | @ 1306/80 | %Cft | | 6207/- | |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds: lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle.) (a) R.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. (I) Ratio (1 : 2: 4 ) 90 Lbs.cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge. (S. I No: 6 (a. i) P. No: 17). | | | | | | |
|  |  | 692 | @337/- | P.Cft | | 233204/- | |
| 6 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.) (S. I No: 8 (b) P. No: 17). | | | | | | |
|  | Tar Steel | 40.160 | @ 5001/70 | P.Cwt | | 200868/- | |
| 7 | Pacca brick work in ground floor in Cement sand mortar 1:6 (S. I No: 5 (e) P. No: 21). | | | | | | |
|  |  | 371 | @ 12674/36 | %Cft | | 47022/- | |
| 8 | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels 2" thick (S. I No: 16 (c) P. No: 42). | | | | | | |
|  |  | 1059 | @ 3275/50 | %Sft | | 34688/- | |
| 9 | Cement concrete plain including placing compacting, finishing and curing, complete (including screening and washing at stone aggregate without shuttering Ratio. 1:2:4 (S.I No: 5 (f) P. No: 16). | | | | | | |
|  |  | 304 | @ 14429/25 | %Cft | | 43865/- | |
| 10 | Applying floating coat of Cement 1/32" thick. (S. I No: 14 P. No: 53). | | | | | | |
|  |  | 3098 | @660/- | %Sft | | 20447/- | |
| 11 | Cement plasters 1:4 upto 12' height. 3/4" thick. (S.I No: 11 (c) P. No: 52). | | | | | | |
|  |  | 3098 | @3015/76 | %Sft | | 93428/- | |
| 12 | Cement plaster 1:6 upto 12' height 1/2" thick (S.I No: 13 (b) P. No: 52). | | | | | | |
|  |  | 990 | @ 2206/60 | | %Sft | | 21845/- | |
| 13 | Cement plaster 1:4 upto 12' height 3/8" thick (S.I No: 11 (a) P. No: 52). | | | | | | |
|  |  | 990 | @ 2197/52 | %Sft | | 21755/- | |
| 14 | Providing and laying tiles glazed 6" x 6" x 1/4" on floor or wall facing in required colour and apttern of STILE specification jointed in white cement and pigment over a base of 1:2 grey cement mortar 3/4" thick including washing and filling of joints with slaurry of white cement and pigment in desired shape with finishing, clearing and cost of wax polish etc. complete including cutting tiles to proper profile. (S.I No: 60 P. No: 47). | | | | | | |
|  |  | 2095 | @ 30509/77 | %Sft | | 639180/- | |
| 15 | Reinforced cement concrete spout including fixing in position 2 1/2" x 6" x 5" 9 (S.I No: 14 P. No: 18). | | | | | | |
|  |  | 10 | 261/25 | Each | | 2613/- | |
| 16 | Supplying & fixing in position iron/steel grill of 3/4" x 1/4" size flat iron of approved design including painting 3 coats etc. complete (weight not to be less than 3.7 Lbs./Sq . Foot of finished grill) (S. I No: 26 P. No: 93). | | | | | | |
|  |  | 146 | @ 180/50 | P.Sft | | 26353/- | |
|  |  |  |  |  | |  | |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | | **Amount** | |
|  |  |  |  |  | |  | |
| 17 | Supplying and filling sand under floor and %Cft plugging in walls (S. I No: 29 P. No: 26) | | | | | | |
|  |  | 500 | @ 1141/25 | %Cft | | 5706/- | |
| 18 | Add Extra lead 03 miles. | | | | | | |
|  |  | 500 | @ 579/41 | %Sft | | 2897/- | |
| 19 | Providing and fixing G.I frames /Chowkats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing. (S. I No: 28 P. No: 93) | | | | | | |
|  |  | 330 | @ 240/50 | P.Rft | | 79365/- | |
| 20 | Providing and fixing G.I frames /Chowkats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants used in making and fixing (S. I No: 29 P. No: 93). | | | | | | |
|  |  | 53 | @ 228/90 | P.Rft | | 12132/- | |
| 21 | First class deodar wood wrought joinery work in wire gauze door and windows with 22 S.W.G . Galvanized wire gauze 144 mesh per square inch iron fittings complete 1 3/4" thick deodar wood framing including wire gauze with ordinary hinges. (S. I No: 14 (a) P. No: 69). | | | | | | |
|  |  | 210 | @ 902/93 | P.Sft | | 189615/- | |
| 22 | White washing Three coats(S.I No: 26 (c) P. No: 54). | | | | | | |
|  |  | 1315 | @ 829/95 | %Sft | | 11412/- | |
| 23 | Priming coat of chalk distemper (S. I No: 23 P. No: 54). | | | | | | |
|  |  | 4088 | @ 442/75 | %Sft | | 18100/- | |
| 24 | Distempering Three coats (S. I No: 24 (c) P. No: 54). | | | | | | |
|  |  | 5258 | @ 1079/65 | %Sft | | 56768/- | |
| 25 | Painting doors / windows (Old Surface) 03 coats. | | | | | | |
|  |  | 1656 | @ 1662/21 | %Sft | | 27526/- | |
|  |  |  |  | **Total:** | | **1835312/-** | |

\_\_\_\_\_\_\_\_\_%Above/Below on the rates of CSR.

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**

**CONTRACTOR**