***SCHEDULE “B”***

**NAME OF WORK: - REHABILITATION OF OFFICE BUILDING OF EDUCATION & LITERACY DEPARTMENT DIVISION SUKKUR DISTRICT GHOTKI OFFICE OF DISTRICT EDUCATION OFFICER GHOTKI @ M.MATHELO AND OFFICE OF TALUKA EDUCATION OFFICER (MALE) M.MATHELO.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1 | Dismantling cement concrete plain 1: 3: 6 (S. I No: 19 (b) P. No: 10). | | | | |
|  |  | 109 | @ 1306/80 | %Cft | 1424/- |
| 2 | Dismantling cement concrete reinforced separating reinfor cement from concrete cleaning and straightening the same (S. I No: 20 P. No: 10). | | | | |
|  |  | 56 | @ 5445/- | %Cft | 3049/- |
| 3 | Removing cement or lime plaster (S. I No: 53 P. No: 13). | | | | |
|  |  | 1716 | @ 121/- | %Cft | 2076/- |
| 4 | Pacca brick work in foundation and plinth in Cement sand mortar 1:6 (S. I No: 4 (e) P. No: 21). | | | | |
|  |  | 43 | @ 11948/36 | %Cft | 5138/- |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds: lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle.) (a) R.C work in roof slab, beams columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respects. (I) Ratio (1 : 2: 4 ) 90 Lbs.cement 2 Cft. Sand 4 Cft. Shingle 1/8" to 1/4" gauge. (S. I No: 6 a i P. No: 17). | | | | |
|  |  | 46 | @ 337/- | P.Cft | 15502/- |
| 6 | Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire (also includes removal of rust from bars.) (S. I No: 8 (b) P. No: 17). | | | | |
|  |  | 2.053 | @ 5001/70 | P.Cwt | 10268/- |
| 7 | Pacca brick work in ground floor in Cement sand mortar 1:6 (S. I No: 5 I (e) 21). | | | | |
|  |  | 379 | @ 12674/36 | %Cft | 48036/- |
| 8 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing (S. I No: 29 P. No: 93). | | | | |
|  |  | 67 | @ 228/90 | P.Rft | 15336/- |
| 9 | Providing and fixing G.I frames /Choukhats of size 7" x 2" or 4 1/2" x 3" for windows using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing (S. I No: 28 P. No: 93). | | | | |
|  |  | 12 | @ 240/50 | P.Rft | 2886/- |
| 10 | Cement plaster 1:6 upto 12' height 1/2" thick (S.I No: 13 (b) P. No: 52). | | | | |
|  |  | 1089 | @ 2206/60 | %Sft | 24030/- |
| 11 | Cement plaster 1:4 upto 12' height 3/8" thick (S.I No: 11 (a) P. No: 52). | | | | |
|  |  | 1089 | @ 2197/52 | %Sft | 23931/- |
| 12 | Applying floating coat of Cement 1/32" thick (S. I No: 14 P. No: 53). | | | | |
|  |  | 1716 | @ 660/- | %Cft | 11326/- |
| 13 | Cement plaster 1:4 upto 12' height 3/4" thick (S. I No: 11 (c) P. No: 52). | | | | |
|  |  | 1716 | @ 3015/76 | %Sft | 519750/- |
| 14 | Mud plaster on floor or roof 1" thick (S. I No: 2 P. No: 51). | | | | |
|  |  | 4841 | @ 555/- | %Sft | 26868/- |
| 15 | Providing and laying single per layer of polythene sheet 0.13 mm thick for water proffing as per specification and instructions of Engineer incharge (S. I No: 38 P. No: 38). | | | | |
|  |  | 4841 | @ 10/70 | P.Sft | 51799/- |
|  |  |  |  |  |  |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 16 | Laying floor of approved with glazed tile 1/4" thick in white cement 1:2 over 3/4" thick cement mortar 1:2 complete (S. I No: 24 P. No: 43). | | | | |
|  |  | 70 | @ 27678/86 | %Sft | 19375/- |
| 17 | White glazed tiles 1/4" thick dado jointed in white cement and laid over 1:2 cement sand mortar 3/4" thick including finishing (S. I No: 37 P. No: 43). | | | | |
|  |  | 232 | @ 28253/61 | %Sft | 65548/- |
| 18 | First class deodar wood wrought joinery in doors and windows etc fixed in chowkats tower bolts cleats cords with hocks etc. | | | | |
|  |  | 72 | @ 902/93 | P.Sft | 65011/- |
| 19 | Cement concrete brick or stone ballast 1 1/2" to 2" gauge Ratio 1 : 5 : 10 (S. I 4 (c) P. No: 15). | | | | |
|  |  | 59 | @ 8694/95 | %Cft | 5130/- |
| 20 | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels 3" thick (S. I No: 16 (d) P. No: 42). | | | | |
|  |  | 780 | @ 8694/95 | %Sft | 67821/- |
| 21 | Making & fixing steel grated door with 1/16" thick sheeting including angle iron frame 2" x 2" 3/8"and 3/4" square bars 4" centre to centre with locking arrangement (S. I No: 24 P. No: 92). | | | | |
|  |  | 24 | @ 726/72 | P.Sft | 17441/- |
| 22 | Supplying and fixing false cailing of plaster of paris, in pannels including making frame , work of Deodar wood including painting with Soligia paint (S. I No: 52 P. No: 64). | | | | |
|  |  | 396 | @ 25293/42 | %Sft | 100162/- |
| 23 | White washing Two coats (S. I No: 26 (b) P. No: 54). | | | | |
|  |  | 4378 | @ 425/84 | %Sft | 18643/- |
| 24 | Distempering Two coats (S. I No: 24 (b) P. No: 54). | | | | |
|  |  | 14027 | @ 1043/90 | %Sft | 146428/- |
| 25 | Painting guards bars, gates irons work similar any type edges three coats (old surface). | | | | |
|  |  | 2043 | @ 977/40 | %Sft | 19968/- |
| 26 | Preparing surface painting doors and windows old surface (S. I No: 4 (c) P. No: 68). | | | | |
|  |  | 1658 | @ 1662/21 | %Sft | 27559/- |
| 27 | Painting doors / windows (New Surface) 03 coats. | | | | |
|  |  | 131 | @ 2116/41 | %Sft | 2772/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total** | **849277/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**

**CONTRACTOR**