***SCHEDULE “B”***

**NAME OF WORK:- SPECIAL REPAIR / ORDINARY REPAIR 2016-17 PROGRAMME @ GOVT. GIRLS PRIMARY SCHOOL AMIR BUX MUHALLA TALUKA DAHARKI.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
|  |  |  |  |  |  |
| 1 | Dismantling cement concrete plain 1: 3: 6 (S. I No: 19 (b) P. No: 10). | | | | |
|  |  | 68 | @ 1306/80 | %Cft | 889/- |
| 2 | Removing cement or lime plaster (S. I No: 53 P. No: 13). | | | | |
|  |  | 1641 | @ 121/- | %Sft | 1986/- |
| 3 | Pacca brick work in ground floor in Cement sand mortar 1:6 (S. I No: 5 I (e) 21). | | | | |
|  |  | 85 | @ 12674/36 | %Cft | 10773/- |
| 4 | Providing and fixing G.I frames /Chowkats of size 7" x 2" or 4 1/2" x 3" for door using 20 gauge G.I sheet I/c welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage , tools and plants used in making and fixing (S. I No: 29 P. No: 93). | | | | |
|  |  | 18 | @ 228/90 | P.Rft | 4120/- |
| 5 | Cement plaster 1:6 upto 12' height 1/2" thick (S.I No: 13 (b) P. No: 52). | | | | |
|  |  | 227 | @ 2206/60 | %Sft | 5009/- |
| 6 | Cement plaster 1:4 upto 12' height 3/8" thick (S.I No: 11 (a) P. No: 52). | | | | |
|  |  | 227 | @ 2197/52 | %Sft | 4989/- |
| 7 | Applying floating coat of Cement 1/32" thick (S. I No: 14 P. No: 53). | | | | |
|  |  | 1641 | @ 660/- | %Sft | 10929/- |
| 8 | Cement plaster 1:4 upto 12' height 3/4" thick (S. I No: 11 (c) P. No: 52). | | | | |
|  |  | 1641 | @ 3015/76 | %Sft | 49489/- |
| 9 | First class deodar wood wrought joinery in doors and windows etc, fixed in position including chowkats hold fasts hinges, iron twer bolts, chocks cleats, handles and cords with hooks, etc deodar paneled or paneled and glazed, or fully glazed 1 ¾” thick (S. I 7 (b) P. No: 58). | | | | |
|  | Only Shutters | 249 | @ 902/93 | P.Sft | 224830/- |
| 10 | Mud plaster on walls 1" thick (S. I No: 1 P. No: 51). | | | | |
|  |  | 1486 | @ 555/- | %Sft | 8247/- |
| 11 | Notice board made with cement (S. I No: 1 P. No: 95). | | | | |
|  |  | 160 | @ 58/11 | P.Sft | 9298/- |
| 12 | Reinforced cement concrete spout including fixing in position 2 1/2" x 6" x 5" (S. I No: 14 P. No: 18). | | | | |
|  |  | 5 | @ 261/25 | Each | 1306/- |
| 13 | White washing three coats (S. I No: 26 (c) P. No: 54). | | | | |
|  |  | 1399 | @ 829/95 | %Sft | 11605/- |
| 14 | Colour washing Two coats (S. I No: 25 (b) P. No: 54). | | | | |
|  |  | 6127 | @ 859/90 | %Sft | 52686/- |
| 15 | Preparing surface painting guards bars, gates irons work similar any type edges three coats (new surface) (S.I 04 P. No: 76). | | | | |
|  |  | 1161 | @ 1270/83 | %Sft | 14754/- |
| 16 | Painting doors and windows (New Surface). | | | | |
|  |  | 590 | @ 1662/21 | %Sft | 9807/- |
|  |  |  |  |  |  |
|  |  |  |  | **Total Rs:** | **420717/-** |

\_\_\_\_\_\_\_\_% above/below on the rates of CSR.

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**

**CONTRACTOR**

W/S & S/F PART “B”

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No:** | **Item of Work** | **Qty:** | **Rate** | **Unit** | **Amount** |
| 1 | Providing and fixing squatting type white glazed earthen ware w.c pan with front flush inlet & complete with including the cost of flushing cistern with internal fitting and flush Pipe with bend and making requisite number of holes in walls plinth & floor for Pipe connection & making good in cement concrete 1: 2: 4: (Foreign Equivalent) With 4" dia C.I Trap (S. I No: 2 (b) P. No: 1). | | | | |
|  |  | 2x1 Nos: | @ 6014/80 | Each | 12030/- |
| 2 | Providing & fixing 4" dia. C.I plain bend of the required degree including extra painting to match the colour of the building (S. I No: 10 P. No: 10). | | | | |
|  |  | 2x1 | @ 566/70 | Each | 1133/- |
| 3 | Providing & fixing 4" x 4" x 4" dia plain C.I branch of the required degree including extra painting to match the colour of the building plain tee (S. I No: 7 P. No: 9). | | | | |
|  |  | 2x1 | @ 704/20 | P.Rft | 1408/- |
| 4 | Providing & fixing 4" dia C.I soil & vent Pipe including cutting and fitting and extra painting to match the colour of building (S. I No: 1 P. No: 9). | | | | |
|  |  | 2x6 | @ 333/29 | P.Rft | 3999/- |
| 5 | Providing G.I Pipes, specials, and clamps etc, including fixing cutting & fitting complete with and I/c the cost of breaking through walls and roof, making good etc. painting two coats after cleaning the Pipe etc. with white zink paint with pigment to match the colour5 of the building and testing with water to a pressure head of 200 feet and handling (S. I No: 1 P. No: 12). | | | | |
|  | 1/2" dia G.I Pipe | 1x25.0 | @ 73/21 | P.Rft | 1830/- |
|  | 3/4" dia G.I Pipe | 1x60.0 | @ 95/79 | P.Rft | 5747/- |
|  | 1" dia G.I Pipe | 1x20.0 | @ 128/55 | P.Rft | 2571/- |
| 6 | S/F in position long bib cocks ½” dia standard pattern (S I No:1 (i) b /P-16) | | | | |
|  |  | 1x3. | 337/92 | Each | 1014/- |
| 7 | Concealed C.P fittings of Superior quality for tiles Bath Rooms S/Fixing concealed stop cock of superior quality with c.p head 1/2" dia (S. I No: 211 (a) P. No: 18). | | | | |
|  |  | 1x2 | @ 478/25 | Each | 957/- |
| 8 | Providing and fixing handle valves (china) (S. I No: 5 P. No: 17). | | | | |
|  |  | 1x4 | @ 271/92 | Each | 1088/- |
| 9 | Supplying & fixing fiber glass tank of approved quality and design and wall thickness as specified I/c cost of nuts, bolts and fixing in plate form of cement concrete 1: 3: 6 and make in connections for in -let ,& ou-let & over flow pipes etc. complete 250 gallons wall thickness 3.5 mm (S. I No: 3 (a) P. No: 21). | | | | |
|  |  | 1x1 | @ 21989/61 | Each | 21990/- |
| 10 | Providing R.C.C pipe with collars class "B" and digging the trenches to required depth & fixing in position including cutting , fitting & jointing with maxphalt composition & cement mortar 1: 1 and testing with water pressure to a head of 4 feet above the top of the highest pipe & refilling with excavated staff (S I No: 2 P-24). | | | | |
|  | 6” dia | 1x50 | @ 199/25 | P.Rft | 9963/- |
|  | 4” dia | 1x12 | @ 146/57 | P.Rft | 1759/- |
| 11 | Providing, Laying uPVC Pressure Pipes of Class 'B' (equivalent make) fixing in trench i/c cutting, fitting and jointing with 'Z' joint with one rubber ring i/c testing with water to a head 61meter or 200 ft. 100 mm (4" dia) (PHE S. I No: 1 (b) P. No: 22). | | | | |
|  |  | 1x15 | @ 137/- | P.Rft | 2055/- |
|  |  |  |  | **Total** | **67544/-** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  | **NON SCHEDULE ITEM** |  |  |  |  |
| 1 | P/F piston pump approved quality (jawed mak) 1 ½ “x 1 suction and delivery with bas plates and complete 1 H.P single phase motor sacraments makos 60 ft. head 2800 i/c the cost of G.I fitting nuts and builts the cost in c.c 1.2.4 plate from (a) local made coir strainer 1 ½” dia with wooden shoe i/c boring fitting and fixing complete (c) Hand pump machine with all accessories 4” dia C.I casing pipe moved make 1 H.P phase motor etc complete. | | | | |
|  | Filter Pipe | 2x10.0 | @ 76/05 | P.Rft | 1521/- |
|  | G.I Pipe | 2x40.0 | @ 38/95 | P.Rft | 3116/- |
|  | Piston Pump | 1x1 No: | @ 4276/- | Each | 4276/- |
|  | Hand Pump | 1x1 No: | @ 1441/65 | Each | 1422/- |
|  |  |  |  | Total | **10335/-** |

Part (B) \_\_\_\_\_\_\_\_% above/below/@ Par on the rates of CSR.

### EXECUTIVE ENGINEER

**EDUCATION WORKS DIVISION**

**GHOTKI**

**CONTRACTOR**