**Financial Proposals**

****

**OFFICE OF THE**

**DIRECTORATE OF MALARIA CONTROL**

**PROGRAMME SINDH HYDERABAD**

**@ DIRECTORATE GENERAL HEALTH SERVICES SINDH HYDERABAD**

**BIDDING DOCUMENTS FOR PROCUREMENT OF**

**ULV MACHINE FOR THE FINANCIAL YEAR 2016-17**

**DATE & TIME RECEIPT OF TENDER : 29.03.2017 11.00 A.M**

**DATE & TIME OF OPENING TENDER : 29.03.2017 12.00 Noon**

**Tender Issued to M/s.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**SPECIFCATION FOR U.L.V MACHINE.**

|  |  |  |  |
| --- | --- | --- | --- |
| **NAME OF ITEM** | **QUANTITY REQUIRED** | **A/U** | **UNIT RATE with GST** |
| **ULV MACHINES (10 Liter)**  **Technical Specification**  Solution Tank : 10 Liters  Fuel Tank : 02-03 Liters  Automatic Ignition: Electronic ignition coil  fed by 4x dry batteries =6v  Starting Devices : Manual start  Max fuel consumption: 1.9 1/h  Flow rate : 10-35 l/h (according to  Nozzle size used)  Standard flow rate : 12 1/h |  |  |  |
|  |  |  |
|  |  |  |
| 15 Nos. |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| **ULV MACHINES (50 Liter)**  **Technical Specification.**  Solution Tank : 50 Liters Stain less Steel  Fuel Tank : 10 Liters  Automatic Ignition: Electronic ignition coil  fed by 4x dry batteries =6v  Starting Devices : Manual start  Max fuel consumption: 3.8 l/h  Flow rate : 10-75 l/h (according to  Nozzle size used)  Standard flow rate : 40 l/h | 10 Nos. |  |  |