***SCHEDULE OF QUANTITIES***

***WORK No: 04***

# 

**DISTRICT MUNICIPAL CORPORATION (WEST)**

**KARACHI, BALDIA ZONE**

***Estimated Cost Rs: 9,99,662/- Earnest Money Rs: 19,993/-***

***Time Limit: 45 Days Penalty Per Day Rs: 1,000/-***

**SUBJECT: P/L 12” Dia R.C.C Pipe Line I/C Aggregate Base Course at Govt. Farhan Boys Secondary**

**School Block “A” Gulshan-e-Ghazi in UC-33 DMC (West) Baldia Zone.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***S.No:*** | ***DESCRIPTION OF WORK*** | ***QUANTITY*** | ***RATE*** | ***PER*** | ***AMOUNT*** |
| *1.* | *Excavation for pipe line in trenches, and pits in all kind of soil of Murum Shape Leveling of beds of trenches to correct lever & grade, surplus earth within a one chain as directed by Eng incharge.* | *3000* | *4650* | *%Cft* | *13950/-* |
| *2.* | *Excavation for pipe line in trenches, and pits in hard rock by hammering and chiseling i/c trimming and dressing sides to true alignment and shape leveling of beds of trenches to correct level and grade cutting joints holes and disposal of surplus earth within a one chain as directed by Engineers Incharge. Providing fence guards. Lights flags and temporary crossings for non-vehicular traffic where ever required lift up to 5ft. (1.52m) and lead upto one chain (30.5m)* | *3750* | *24150* | *P-Cft* | *90562/-* |
| *3.* | *P/L reinforced cement concrete pipes with rubber rings i/c cartage, loading unloading at site of work fixing in trenches cutting fitting, jointing with rubber rings etc complete KWSB Approved Rate, M/S Balochistan R.C.C Pipe Co. M/S Pakistan construction (Pvt.) Ltd. M/S Kamal R.C.C Pipe Co. 12”dia pipe* | *500* | *412.00* | *P/rft* | *206000/-* |
| *4.* | *Construction of 4” dia manhole inside complete with 21”dia c c 1:2:4 pre cast C.I frame 15kg i/c the cost of M.S bars reinforcement and two handles 5” clear depth c c 1:2:4 cast in situ walls with 50% screened graded bajri of 9” thick i/c bending and channel i/c inside walls surface complete i/c cutting asphalt roads excavation in all kind of soil back filling and disposal of surplus stuff (KW&SB) approved rate.* | *20-Nos* | *14529.29* | *Each* | *290586/-* |
| *5.* | *Extra depth beyond 5” ft or less then 5 deducted at the same rate (KWSB) approved rate.* | *(-)10* | *2538.60* | *Pft* | *(-)25386/-* |
| *6.* | *Refilling the excavated stuff & surplus Earth etc. complete.* | *6075* | *2760* | *%Cft* | *16767/-* |
| *7.* | *Carriage of 100-Cft tons of all kind material like Cole brick i/c loading unloading 10 mile.* | *675* | *595.80* | *%Cft* | *4022/-* |
| *8.* | *P/L aggtt base course material over proper grade and camber having CBR 80% as per AASHTO standard specification i/c spreading an compacting by approve mechanical means (Motor harder, Vibratory roller and smooth wheel roller etc) watering to maintain the moisture content the compaction of each layer shall 100 percent to the max dry density (Rate i/c all cost of material T&P and carriage upto 3 Chain). 12’Dia* | *1250* | *5542.24* | *%Cft* | *69278/-* |
| *9.* | *Manufacturing and supplying R.C.C main hole covers cast in situ 1:2:4 C.C. 3” inch deep in center reinforced with 3/8” dia M.S Bars welded on M.S. sheet i/c curing transportation.*  *21” dia.*  *24” dia.* | *25-Nos* | *913.63* | *Each* | *22841/-* |

***PTO***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *10.* | *Manufacturing and supplying of R.C.C Ring Slab of 21” inside 36” dia outside 75 wide and to thick i/c 3/8” dia tor steel bar two concentric rings with 3/8” dia Nos. cross links bars welded and two sunk type hook, lasted in 1:1-1/2:3 concrete with embedded 15kg C.I frame in per feet position i/c terms partition charges for an average lead of 20 km per trip from casting yard to town office (A minimum of 25 slabs per trip will be transported.)* | *25-Nos* | *1906.60* | *Each* | *47665/-* |
| *11.* | *Rate analysis for shifting to the site and fixing 26” dia Ring Slab in perfect position on damage manhole i/c cutting of damage portion of mentioned in past shape and lying of cement concrete mortar of 2” thickness and disport* | *25-Nos* | *563.09* | *Each* | *14077/-* |
| *12.* | *Hiring of Skilled Labour for cleaning of Nallah (Afghani Bajorri) for 8-Hour* | *277-Nos* | *900* | *P-Labour* | *249300/-* |
| ***Total Estimated Cost*** | | | | | ***9,99,662.00*** |

*Nomenclature, Quantities and Rates etc checked*

*and found correct.*

***ASSTT: EX-ENGINEER (B&R) EXECUTIVE ENGINEER (B&R)***

*BALDIA ZONE BALDIA ZONE*

*I/We hereby quoted Rates @ % above/below the S/R*

*The total amount is Rs: (Rupees:*

*(In Figure) (In Word)*

## *Contractor’s Signature:*

## 

## *Address:*