|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**M/R TO LIVE STOCK FARM ROHRI (SHED NO 04 ) REPAIR OF OFFICE & SHEDS).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Mud plaster on walls 1” thick.  (S.I.No. 1 P-50). | | | | | | | | | | |  | |  |
|  |  | | |  | | 1500 | | SFT | | 555/- | | %SFT | | 8325/- |
| 2/- | Lime Neru plaster 1:2 with fine finish of neru plaster mixed with 10% of cement ½ thick. (S.I.No.7 P-58). | | | | | | | | | | |  | |  |
|  |  | | | | | 1500 | | SFT | | 1428/35 | | %SFT | | 21425/- |
| 3/- | | Scraping ordinary distemper or oil bound on wall.  (S.I.No.54 (b) P-13). | | | | | | | | |  | |  | | |
|  | |  |  | | 4040 | | SFT | | 226/88 | | %SFT | | 9166/- | | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 04/- | Distempering two coats (S.I.No.24 P-53). | | | | |  |  |
|  |  |  | 4040 | SFT | 1079/65 | %SFT | 43618/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 05/- | Preparing the surface and painting with weather coat of approved make to old weather coat surface.(S.I.No.39 (A) P-55). | | | | |  |  |
|  |  |  | 3166 | SFT | 1498/48 | %SFT | 67066/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 06/- | POS, Painting doors & windows any type i/c edges 3 coats.  (S.I.No.4 P-68 ). | | | | |  |  |
|  |  |  | 433 | SFT | 1662/21 | %SFT | 7197/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 07/- | PNS, Painting guard bars gates irons bars grating, railing inclufing braces etc and similar open work 3 coats. (S.I.No.4 (d) P-70). | | | | |  |  |
|  |  |  | 144 | SFT | 674/19 | %SFT | 971/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Removing cement or lime plaster.  (S.I.No.53 P-14). | | | | |  |  |
|  |  |  | 630 | SFT | 121/- | %SFT | 762/- |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 9/- | Applying floating coat of cement 1/32”thick.  (S.I.No:14 P-52). | | | |  |  |
|  |  | 630 | SFT | 660/- | %SFT | 4158/- |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 10/- | Cement plaster (1:6) upto 20’ height ½”thick.  (S.I.No:13 (b) P-51). | | | |  |  |
|  |  | 630 | SFT | 2206/60 | %SFT | 13902/- |
| 11/- | Cement plaster (1:4) upto 20’ height 3/8”thick.  (S.I.No:11 (a) P-51). | | | |  |  |
|  |  | 630 | SFT | 2197/52 | %SFT | 13844/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels 3” thick (S.I.No:4 (c) P-16). | | | | |  |  |
|  |  |  | 5100 | SFT | 3275/50 | %SFT | 167051/- |

|  |  |  |  |
| --- | --- | --- | --- |
|  | BUILDINGS SCHEDULE ITEMS TOTAL | RS: | 3,57,485/- |

|  |  |  |  |
| --- | --- | --- | --- |
| PART "A" | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |

|  |
| --- |
| **BILL OF QUANTITIES** |
| Description & Rate of items based on Schedule/ Market (offered Rates). |

**M/R TO LIVE STOCK FARM ROHRI (SHED NO 04 ) REPAIR OF OFFICE & SHEDS).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.NO: | NAME OF ITEM. | QUANTITY. | RATE. | UNIT. | AMOUNT. |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/- | Mud plaster on walls 1” thick.  (S.I.No. 1 P-50). | | | | | | | | | | |  | |  |
|  |  | | |  | | 1500 | | SFT | | 555/- | | %SFT | | 8325/- |
| 2/- | Lime Neru plaster 1:2 with fine finish of neru plaster mixed with 10% of cement ½ thick. (S.I.No.7 P-58). | | | | | | | | | | |  | |  |
|  |  | | | | | 1500 | | SFT | | 1428/35 | | %SFT | | 21425/- |
| 3/- | | Scraping ordinary distemper or oil bound on wall.  (S.I.No.54 (b) P-13). | | | | | | | | |  | |  | | |
|  | |  |  | | 4040 | | SFT | | 226/88 | | %SFT | | 9166/- | | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 04/- | Distempering two coats (S.I.No.24 P-53). | | | | |  |  |
|  |  |  | 4040 | SFT | 1079/65 | %SFT | 43618/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 05/- | Preparing the surface and painting with weather coat of approved make to old weather coat surface.(S.I.No.39 (A) P-55). | | | | |  |  |
|  |  |  | 3166 | SFT | 1498/48 | %SFT | 67066/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 06/- | POS, Painting doors & windows any type i/c edges 3 coats.  (S.I.No.4 P-68 ). | | | | |  |  |
|  |  |  | 433 | SFT | 1662/21 | %SFT | 7197/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 07/- | PNS, Painting guard bars gates irons bars grating, railing inclufing braces etc and similar open work 3 coats. (S.I.No.4 (d) P-70). | | | | |  |  |
|  |  |  | 144 | SFT | 674/19 | %SFT | 971/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 8/- | Removing cement or lime plaster.  (S.I.No.53 P-14). | | | | |  |  |
|  |  |  | 630 | SFT | 121/- | %SFT | 762/- |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 9/- | Applying floating coat of cement 1/32”thick.  (S.I.No:14 P-52). | | | |  |  |
|  |  | 630 | SFT | 660/- | %SFT | 4158/- |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 10/- | Cement plaster (1:6) upto 20’ height ½”thick.  (S.I.No:13 (b) P-51). | | | |  |  |
|  |  | 630 | SFT | 2206/60 | %SFT | 13902/- |
| 11/- | Cement plaster (1:4) upto 20’ height 3/8”thick.  (S.I.No:11 (a) P-51). | | | |  |  |
|  |  | 630 | SFT | 2197/52 | %SFT | 13844/- |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 12/- | Providing and laying 1" thick topping cement concrete (1:2:4 ) including Surface finishing and dividing into panels 3” thick (S.I.No:4 (c) P-16). | | | | |  |  |
|  |  |  | 5100 | SFT | 4411/82 | %SFT | 225003/- |

|  |  |  |  |
| --- | --- | --- | --- |
|  | BUILDINGS SCHEDULE ITEMS TOTAL | RS: | 415,437/- |

|  |  |  |  |
| --- | --- | --- | --- |
| PART "A" | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_%Above/Below Buildings Schedule Items | **Total Rs:-** |  |

|  |  |  |
| --- | --- | --- |
| CONTRACTOR |  | EXECUTIVE ENGINEER  PROVINCIAL BUILDINGS DIVISION  SUKKUR |