**LAV: BLOCK**

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GGHS SALLAR MUHALLA TALUKA KINGRI DISTRICT KHAIRPUR SEMIS CODE: 415040378 (Lev: Block & C/Wall)**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_S;NO; DESCRIPTION. QTY; RATE. UNIT. AMOUNT.

1. Dismentling R.C.C work1;2;4 .(SI:NO:20 p-10)

62.0 Rs:5445/- %cft. 3376/-

2. Dismentling Pacca brick work 1;6.(SI:NO:13-b P-10)

299.0 RS:1285/63 %cft. 3844/-

3. Excavation in foundation of building bridges and other str:with excavated earth

Lead upto 5”ft.(SI:NO:18-b p-4)

240.0 Rs:3176/25 %cft. 762/-

4. Cement concerte brick or stone ballast 1 ½” to 2” guage ratio 1;5;10.(SI:NO:4-c p-14)

36.0 Rs:8694/95 %cft. 3130/-

5. Pacca brick work in foundation and plinth ratio 1;6.(SI:NO:4-aP-20).

342.0 Rs:11948/36 %cft. 40863/-

6. Filling watering and remaining earth in floor with new earth from out side

Lead upto 5”ft.(SI:NO: P- )

101.0 Rs:3630/- %0cft. 367/-

7. R.C.C. work i/c all labour and material except the cost of steel and its labour

For bending and binding which will be paid sepratelly.This rate also i/c all

Kinds of forms mould lifting shuttering curring rendering and finshing the

Exposed surface i/c screening and washing of shingle 1;2;4.(SI:NO:6-a P-16)

104.0 Rs;337/- P/cft. 35048/-

8. Fabrication of mild steel reinforcement for c.c.i/c cutting bending and binding

i/c rust removal from bars.(SI:NO:8-d P-20)

4.642 Rs:5001/70 P/cwt. 23218/-

9. Pacca brick work G/Floor ratio 1;6.(SI:NO:7-e P-22).

264.0 Rs:12674/36 %cft. 33460/-

10. M/F steel door frame chowkats size 7”x2” of 3”x4” type fixing in position

Using 20” guage sheet welding fixing.(SI:NO:29 p-92)

32.0 Rs:726/72 P/Rft. 23255/-

11. Cement plaster ½” thick upto 20” height ratio 1;6.(SI:NO:13-b P-51)

644.0 Rs:2206/60 %sft. 14211/-

12. Cement plaster 3/8” thick upto 20” height ratio 1;4.(SI:NO:11-a p-51)

644.0 Rs:2197/52 %sft. 14152/-

13. Cement concerte plain i/c compacing finshing and curring i/c screening and washing

Of stone aggregate without shuttering 1;2;4 (SI:NO:5-p P:NO:15)

12.0 Rs:14429/25 %sft. 1732/-

14.P/L 2” thick c.c.topping 1;2;4 i/c surface finshing and dividing into panels.

(SI:NO:16-c P-41)

107.0 Rs:3275/50 %sft. 3505/-

15. Cement pointing stricking of joints on walls ratio 1;2.(SI:NO: P- )

298.0 Rs:1287/44 %sft. 3837/-

16. Laying floor of approved with glazed tiles ¼” thick in white cement 1;2 over ¾”

Thick cement mortor 1;2 Complete.(SI:NO:24 P-42)

72.0 Rs:27678/86 %sft. 19929/-

17. White glazed tiles dado ¼” thick laid in pigment over 1;2 cement sand mortor ¾”

Thick i/c finshing.(SI:NO:38 P-44)

317.0 Rs:28253/86 %sft. 89564/-

18. First class deodar wood wrought joinery doors and windows etc fixed in position

i/c chowkats fasts hinges iron cleats.(SI:NO:7-b P-57)

30.0 Rs:902/93 P/sft. 27088/-

19. Colour washing two coats.(SI:NO:23 p-53)

298.0 Rs:859/90 %sft. 2563/-

20. White wash two coats.(SI:NO:26-b P-53)

105.0 Rs:425/84 %sft. 2851/-

21. Primary coats of chalk under distempering .(SI:NO:23 P-53)

644.0 Rs:442/75 %sft. 2851/-

22. Distempring two coats.(SI:NO:24-c P-53)

644.0 Rs:1079/75 %sft. 6953/-

23. Painting doors and windows i/c any type surface.(SI:NO:5c P-69).

82.0 Rs:1662/21 %sft. 1363/-

\_\_\_\_\_\_\_\_\_

3,55538/-