**LAV: BLOCK**

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GBHS MANGHANWARI TALUKA KINGRI DISTRICT KHAIRPUR SEMIS CODE: 415040382 (Lev: Block & C/Wall)**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_S;NO; DESCRIPTION. QTY; RATE. UNIT. AMOUNT.

1. Dismentling R.C.C work1;2;4 .(SI:NO:20 p-10)

61.0 Rs:5445/- %cft. 3321/-

2. Excavation in foundation of building bridges and other str:with excavated earth

Lead upto 5”ft.(SI:NO:18-b p-4)

240.0 Rs:3176/25 %cft. 762/-

3. Cement concerte brick or stone ballast 1 ½” to 2” guage ratio 1;5;10.(SI:NO:4-c p-14)

37.0 Rs:8694/95 %cft. 3217/-

4. Pacca brick work in foundation and plinth ratio 1;6.(SI:NO:4-aP-20).

138.0 Rs:11948/36 %cft. 16489/-

5. Filling watering and remaining earth in floor with new earth from out

Side lead upto 5”ft.(SI:NO: P- )

69.0 Rs:3630/- %0cft. 250/-

6. R.C.C. work i/c all labour and material except the cost of steel and its labour

For bending and binding which will be paid sepratelly.This rate also i/c all

Kinds of forms mould lifting shuttering curring rendering and finshing the

Exposed surface i/c screening and washing of shingle 1;2;4.(SI:NO:6-a P-16)

81.0 Rs;337/- P/cft. 27297/-

7. Fabrication of mild steel reinforcement for c.c.i/c cutting bending and binding

i/c rust removal from bars.(SI:NO:8-d P-20)

3.616 Rs:5001/70 P/cwt. 18086/-

8. Pacca brick work other than building ratio 1;6.(SI:NO:7-e P-22).

71.0 Rs:12346/65 %cft. 8999/-

9. M/F steel door frame chowkats size 7”x2” of 3”x4” type fixing in position

Using 20” guage sheet welding fixing.(SI:NO:29 p-92)

32.0 Rs:726/72 P/Rft. 23255/-

10. Cement plaster ½” thick upto 20” height ratio 1;6.(SI:NO:13-b P-51)

686.0 Rs:2206/60 %sft. 15138/-

11. Cement plaster 3/8” thick upto 20” height ratio 1;4.(SI:NO:11-a p-51)

686.0 Rs:2197/52 %sft. 15138/-

12. Cement concerte plain i/c compacing finshing and curring i/c screening and washing

Of stone aggregate without shuttering 1;2;4 (SI:NO:5-p P:NO:15)

7.0 Rs:14429/25 %sft. 1010/-

13.P/L 2” thick c.c.topping 1;2;4 i/c surface finshing and dividing into panels.

(SI:NO:16-c P-41)

103.0 Rs:3275/50 %sft. 3384/-

14. First class deodar wood wrought joinery doors and windows etc fixed in position

i/c chowkats fasts hinges iron cleats.(SI:NO:7-b P-93)

27.0 RS:902/93 P/sft. 24379/-

15. Laying floor of approved with glazed tiles ¼” thick in white cement 1;2 over ¾”

Thick cement mortor 1;2 Complete.(SI:NO:24 P-42)

72.0 Rs:27678/86 %sft. 19929/-

16. White glazed tiles dado ¼” thick laid in pigment over 1;2 cement sand mortor ¾”

Thick i/c finshing.(SI:NO:38 P-44)

180.0 Rs:28253/86 %sft. 50856/-

17. Colour washing two coats.(SI:NO:23 p-53)

686.0 Rs:859/90 %sft. 5899/-

18. White wash two coats.(SI:NO:26-b P-53)

40.0 Rs:425/84 %sft. 170/-

16. Painting doors and windows i/c any type surface.(SI:NO:5c P-69).

70.0 Rs:977/40 %sft. 684/-

\_\_\_\_\_\_\_\_\_

2,38200/-