Sr.No. 39 S. No: 13

BILL OF QUANTITES

(A) Description and rate of items based on composite schedule of rates.

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GBHS WAFA NAWAZ ALI SHAR TALUKA T.MIRWAH DISTRICT KHAIRPUR SEMIS CODE: 415060786 (Lev: Block & C/Wall)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S;No | Description/Measurement | Qty | Rate | Unit | Amount |

1. Dismentling RCC cement concrete plain (S:I:NO: 19b p10)

302.0 Rs:5445/0 %sft 16444/0

2. Dismentling cement concrete plain 1.3.6. ratio (CSI:NO: 19 b page 10 )

2074.0 Rs:1306/80 %sft 26664/0

3. Pacca brick work plinth and foundation in cement sand ratio 1:6 (S:I:NO:ec p 20

302.0 Rs:11948/36 %sft 251155/

4 RCC work i/c all ;abour and material except the cost of steel reinforcement and its

labour for bending binding laying in position removal of s rust from bars

RCC work in roof slab columns rafts lintel and other structure member laid in situ or

precast laid in position complete in all respect ratio 1:2:4.(S:I:NO: 60 p 16)

136.0 Rs:337/00 P;SFT 191753/0

5. Fabrication of mild steel reinforcement for cement concrete i/c cutting bending laying

In position making joints and fastening i/c cost of binding wire and also cost of binding wire i/c removal

Of rusr from bsrd(CSI:NO: 80p16)

Qty:same as item No; 4=569x5

.. 112 =25.401 Rs:5001/70 P:Cwt 127048/00

6. Pacca brick work other than building strucking joints on walls 1;6 ratio (S:I:NO:7e P 22)

3861.0 Rs:12346/65 %cft 1089768/00

7. Cement plaster 1:6 ratio upoto 20”height ½” thick (CSI:NO:13b p510

8712.0 Rs:2206/60 %sft 192239/0

8. Cement plaster 1:4 ratio upto 20” height 3/8” thick (S:I:NO: 10 a p 51)

Same qty of item no; 7= 8712.0 Rs:2197/52 %sft 191448/00

9. Applying flooting coalts (S:I:NO: 14 p520

Same qty of item no; .8=8712.0 Rs:660/0 %sft 57499/00

10. Cement pointing strucking jointsd on walls 1.3 ratio (S:I:NO: P )

4650.0 Rs:1213/58 %sft 56431/0

11. P:Fixing Halla Tiles glazed 8”x8” 0n floor or walls in required patterns of steel specified

Jointed in white cement pigment over 1.2 grey cement mortor ¾” thick and filling paint

white sulary of white cement etc complete (S:I:NO: 62 P:47)

45.0 Rs:34520/31 %sft 15534/0

12. Colour washing two coalts (CSI:NO: P: ) =

13362.0 Rs:- 859/90 %sft 114900/00

13 Preparing Painting guard bars gates of iron bars three coalts (old surface)

(S:I:NO:14 d p; 68)

240.0 Rs:674/60 %sft 1619/0

14 Preparing Painting guard bars gates of iron bars three coalts (old surface)

(S:I:NO:14 d p; 68)

349.0 Rs:10770/60 %sft 37591/0

15 broden glasses(S:I:NO:6 d p;104)

930.0 Rs:70/44 %sft 65509/0

Total Rs:- 1822538/0

**NAME OF WORK: REPAIR & MAINTENANCE OF EXISTING NONFUNCTIONAL TOILETS & DAMAGED BOUNDARY WALLS OF SECONDARY SCHOOLS IN DISTRICT KHAIRPUR (24 UNITS) @ GBHS WAFA NAWAZ ALI SHAR TALUKA T.MIRWAH DISTRICT KHAIRPUR SEMIS CODE: 415060786 (Lev: Block & C/Wall)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S;No | Description/Measurement | Qty | Rate | Unit | Amount |

1. Dismentling RCC cement concrete plain (S:I:NO: 19b p10)

80.0 Rs:5445/0 %sft 4356/0

2. Removing cement or lime plaster from walls (CSI:NO: 53p 13)

683.0 Rs:121/05 %sft 826/0

3. Dismentling cement concrete plain 1.3.6. ratio (CSI:NO: 19 b page 10 )

7.0 Rs:1306/80 %sft 91/0

4. Pacca brick work in ground floor in cement sand mortor 1:6 ratio (S:I:NO:5e p;20)

27.0 Rs:12674/36 %sft 3422/0

5 RCC work i/c all ;abour and material except the cost of steel reinforcement and its

labour for bending binding laying in position removal of s rust from bars

RCC work in roof slab columns rafts lintel and other structure member laid in situ or

precast laid in position complete in all respect ratio 1:2:4.(S:I:NO: 60 p 16)

1365.0 Rs:337/00 P;SFT 460005/0

6. Fabrication of mild steel reinforcement for cement concrete i/c cutting bending laying

In position making joints and fastening i/c cost of binding wire and also cost of binding wire i/c removal

Of rusr from bsrd(CSI:NO: 80p16)

Qty:same as item No; 5=1365x5

.. 112 =4.33 Rs:5001/70 P:Cwt 21657/00

7

S/Fixing G:I Frame Chowkats steel Door frame size 7”x2” of 3”x4” type i/c

27,

ixing in position using 20”guage (Bos Type)(S:I:NO:29p 92

32.0 Rs:228/90 P:Rft 7325/0

8. First class deodar wood wrought joinery inn doors and windows etc fixed in position

i/c hooks bolts nuts iron bolts handles and cords with hooks deodar panneled

Hinges iro i/c fixing in position complete (only shutters) (S:I:NO: 7b p 57

28.0Rs:902/93 P:Sft 25282/00

9. Cement plaster 1:6 ratio upoto 20”height ½” thick (CSI:NO:13b p510

Same qty:of item No 2

683.0 Rs:2206/60 %sft 15071/0

10. Applying flooting coalts (S:I:NO: 14 p520

Same qty of item no; .9=683.0 Rs:660/0 %sft 4508/00

11. Cement plaster 1:4 ratio upto 20” height 3/8” thick (S:I:NO: 10 a p 51)

Same qty of item no; 10= 683.0 Rs:2197/52 %sft 15009/00

12. Cement plaster pointing

479.0 Rs:1213/58 %sft 5813/0

13. white glazed tiles

40.0 Rs:27747/06 %sft 11093/0

14. white glazed tiles

108.0 Rs:28299/30 %sft 30563/0

15. White washing three coaltrs (CSI:NO: P: )

40.0 Rs:425/54 %sft 47639/0

16. Colour washing two coalts (CSI:NO: P: ) =

1036.0 Rs:- 859/90 %sft 8909/00

17. painting doors (CSI:NO: P: ) =

35.0 Rs:- 1160/06 %sft 406/00

RS= 187190